<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="59.187278125" y2="0" width="0" layer="20"/>
<wire x1="59.187278125" y1="0" x2="59.187284375" y2="55.036878125" width="0" layer="20"/>
<wire x1="59.187284375" y1="55.036878125" x2="0" y2="55.036878125" width="0" layer="20"/>
<wire x1="0" y1="55.036878125" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="1X06SMD">
</package>
<package name="2X03SMD">
</package>
<package name="2X02SMD">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA168"/>
<element name="U$1" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="JP1" library="fab" package="2X03SMD" value=""/>
<element name="SOLENOID" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$3" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$5" library="fab" package="SOIC8" value="A4953-H-BRIDGE-MOTOR-DRIVER"/>
<element name="U$6" library="fab" package="SOIC8" value="A4953-H-BRIDGE-MOTOR-DRIVER"/>
<element name="U$7" library="fab" package="SOIC8" value="A4953-H-BRIDGE-MOTOR-DRIVER"/>
<element name="STEPPER_1_A" library="fab" package="SOIC8" value="A4953-H-BRIDGE-MOTOR-DRIVER"/>
<element name="R1" library="fab" package="R1206" value="10k"/>
<element name="IC1" library="fab" package="SOT23" value=""/>
<element name="C1" library="fab" package="C1206" value="1uF"/>
<element name="T1" library="fab" package="SOT-23" value=""/>
<element name="STEPPER_1" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="STEPPER_2" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="C2" library="fab" package="C1206" value="10uF"/>
<element name="C3" library="fab" package="C1206" value=".1uF"/>
<element name="C4" library="fab" package="C1206" value="10uF"/>
<element name="C5" library="fab" package="C1206" value=".1uF"/>
<element name="C6" library="fab" package="C1206" value="10uF"/>
<element name="C7" library="fab" package="C1206" value="10uF"/>
<element name="C8" library="fab" package="C1206" value="0.1uF"/>
<element name="C9" library="fab" package="C1206" value="0.1uF"/>
</elements>
<signals>
<signal name="RX">
<contactref element="U$1" pad="5"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="TX">
<contactref element="U$1" pad="4"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="29"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="4"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="3"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="5V">
<contactref element="JP1" pad="5"/>
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="U$1" pad="3"/>
<contactref element="SOLENOID" pad="3"/>
<contactref element="SOLENOID" pad="4"/>
<contactref element="STEPPER_1_A" pad="4"/>
<contactref element="U$5" pad="4"/>
<contactref element="U$7" pad="4"/>
<contactref element="U$6" pad="4"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="U$3" pad="3"/>
<contactref element="U$3" pad="4"/>
<contactref element="U$1" pad="1"/>
<contactref element="T1" pad="2"/>
<contactref element="STEPPER_1_A" pad="1"/>
<contactref element="U$7" pad="1"/>
<contactref element="U$6" pad="1"/>
<contactref element="U$5" pad="1"/>
<contactref element="U$5" pad="7"/>
<contactref element="STEPPER_1_A" pad="7"/>
<contactref element="U$6" pad="7"/>
<contactref element="U$7" pad="7"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="21"/>
<contactref element="C7" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="12V">
<contactref element="IC1" pad="2"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="STEPPER_1_A" pad="5"/>
<contactref element="U$7" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$5" pad="5"/>
<contactref element="U$6" pad="5"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="JP1" pad="6"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="SOL_GATE">
<contactref element="T1" pad="3"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="SOL">
<contactref element="T1" pad="1"/>
<contactref element="SOLENOID" pad="2"/>
<contactref element="SOLENOID" pad="1"/>
</signal>
<signal name="S1_A_OUT2">
<contactref element="STEPPER_1_A" pad="8"/>
<contactref element="STEPPER_1" pad="3"/>
</signal>
<signal name="S1_A_OUT1">
<contactref element="STEPPER_1_A" pad="6"/>
<contactref element="STEPPER_1" pad="1"/>
</signal>
<signal name="S1_B_OUT2">
<contactref element="U$7" pad="8"/>
<contactref element="STEPPER_1" pad="4"/>
</signal>
<signal name="S1_B_OUT1">
<contactref element="U$7" pad="6"/>
<contactref element="STEPPER_1" pad="2"/>
</signal>
<signal name="S1_B_IN2">
<contactref element="U$7" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="S1_B_IN1">
<contactref element="U$7" pad="3"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="S2_A_IN1">
<contactref element="U$5" pad="3"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="S2_B_IN2">
<contactref element="U$6" pad="2"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="S2_A_OUT2">
<contactref element="U$5" pad="8"/>
<contactref element="STEPPER_2" pad="3"/>
</signal>
<signal name="S2_A_OUT1">
<contactref element="U$5" pad="6"/>
<contactref element="STEPPER_2" pad="1"/>
</signal>
<signal name="S2_B_OUT2">
<contactref element="U$6" pad="8"/>
<contactref element="STEPPER_2" pad="4"/>
</signal>
<signal name="S2_B_OUT1">
<contactref element="U$6" pad="6"/>
<contactref element="STEPPER_2" pad="2"/>
</signal>
<signal name="S1_A_IN2">
<contactref element="STEPPER_1_A" pad="2"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="S1_A_IN1">
<contactref element="STEPPER_1_A" pad="3"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="S2_A_IN2">
<contactref element="U$5" pad="2"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="S2_B_IN1">
<contactref element="U$6" pad="3"/>
<contactref element="U1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
