<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="1.5875" y1="28.2575" x2="1.905" y2="27.94" width="0.4064" layer="20"/>
<wire x1="1.905" y1="27.94" x2="9.525" y2="20.32" width="0.4064" layer="20"/>
<wire x1="9.525" y1="20.32" x2="31.115" y2="20.32" width="0.4064" layer="20"/>
<wire x1="31.115" y1="20.32" x2="40.64" y2="29.845" width="0.4064" layer="20"/>
<wire x1="40.64" y1="29.845" x2="40.64" y2="39.6875" width="0.4064" layer="20"/>
<wire x1="40.64" y1="39.6875" x2="42.2275" y2="41.275" width="0.4064" layer="20"/>
<wire x1="42.2275" y1="41.275" x2="42.2275" y2="49.8475" width="0.4064" layer="20"/>
<wire x1="42.2275" y1="49.8475" x2="38.4175" y2="53.6575" width="0.4064" layer="20"/>
<wire x1="38.4175" y1="53.6575" x2="4.1275" y2="53.6575" width="0.4064" layer="20"/>
<wire x1="4.1275" y1="53.6575" x2="0.635" y2="50.165" width="0.4064" layer="20"/>
<wire x1="0.635" y1="50.165" x2="0.635" y2="29.21" width="0.4064" layer="20"/>
<wire x1="0.635" y1="29.21" x2="1.5875" y2="28.2575" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="R1206FAB">
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="2X02SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1uF"/>
<element name="C2" library="fab" package="C1206FAB" value=".1uF"/>
<element name="C3" library="fab" package="C1206FAB" value="10uF"/>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="IC2" library="fab" package="SOT23" value=""/>
<element name="R1" library="fab" package="R1206FAB" value="10k"/>
<element name="HBRDG" library="fab" package="SOIC8" value="A4953-H-BRIDGE-MOTOR-DRIVER"/>
<element name="U$2" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$3" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$4" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$5" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$7" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="R2" library="fab" package="R1206FAB" value="1k"/>
</elements>
<signals>
<signal name="N$3">
<contactref element="HBRDG" pad="8"/>
<contactref element="U$3" pad="4"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="HBRDG" pad="6"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="U$4" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="HBRDG" pad="1"/>
<contactref element="HBRDG" pad="7"/>
<contactref element="U$2" pad="6"/>
<contactref element="U$7" pad="2"/>
<contactref element="U$5" pad="1"/>
<contactref element="U$5" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="HBRDG" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="U$4" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="U$4" pad="2"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U$4" pad="1"/>
<contactref element="HBRDG" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U$2" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$11">
<contactref element="U$2" pad="5"/>
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U$2" pad="3"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$12">
<contactref element="U$2" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$14">
<contactref element="U$5" pad="4"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$15">
<contactref element="U$5" pad="2"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="R2" pad="1"/>
<contactref element="U$7" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="11"/>
<contactref element="HBRDG" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="10"/>
<contactref element="HBRDG" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
