<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="8.255" y1="53.721" x2="8.255" y2="7.747" width="0.254" layer="20"/>
<wire x1="8.255" y1="7.747" x2="59.817" y2="7.747" width="0.254" layer="20"/>
<wire x1="59.817" y1="7.747" x2="59.817" y2="53.721" width="0.254" layer="20"/>
<wire x1="59.817" y1="53.721" x2="8.255" y2="53.721" width="0.254" layer="20"/>
</plain>
<libraries>
<library name="fab_copy">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="R1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="1X06SMD">
</package>
<package name="2X03SMD">
</package>
<package name="C1206FAB">
</package>
<package name="2X02SMD">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B2,54">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="fab_copy" package="SOIC14" value="ATTINY44-SSU"/>
<element name="NMOS1" library="fab_copy" package="SOT-23" value=""/>
<element name="NMOS2" library="fab_copy" package="SOT-23" value=""/>
<element name="NMOS3" library="fab_copy" package="SOT-23" value=""/>
<element name="PMOS1" library="fab_copy" package="SOT-23" value=""/>
<element name="PMOS2" library="fab_copy" package="SOT-23" value=""/>
<element name="R1" library="fab_copy" package="R1206FAB" value="10k"/>
<element name="R2" library="fab_copy" package="R1206FAB" value="10k"/>
<element name="R3" library="fab_copy" package="R1206FAB" value="10k"/>
<element name="R4" library="fab_copy" package="R1206FAB" value="10k"/>
<element name="U$1" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="U$2" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="C1" library="fab" package="C1206FAB" value="CAP-US1206FAB"/>
<element name="PMOS3" library="fab_copy" package="SOT-23" value=""/>
<element name="V+" library="testpad" package="B2,54" value="PTR1B2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="R6" library="fab_copy" package="R1206FAB" value="0"/>
<element name="R8" library="fab_copy" package="R1206FAB" value="0"/>
<element name="GND" library="testpad" package="B2,54" value="PTR1B2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="U$3" library="fab_copy" package="LED1206FAB" value="LEDFAB1206"/>
<element name="R9" library="fab_copy" package="R1206FAB" value="499"/>
<element name="R7" library="fab_copy" package="R1206FAB" value="10k"/>
<element name="R10" library="fab_copy" package="R1206FAB" value="10k"/>
<element name="R11" library="fab_copy" package="R1206FAB" value="10k"/>
<element name="NMOS4" library="fab_copy" package="SOT-23" value=""/>
<element name="R12" library="fab_copy" package="R1206FAB" value="10k"/>
<element name="U$4" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$5" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="U$6" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="R5" library="fab_copy" package="R1206FAB" value="0"/>
</elements>
<signals>
<signal name="GND">
<contactref element="NMOS2" pad="2"/>
<contactref element="NMOS3" pad="2"/>
<contactref element="NMOS1" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="U$2" pad="6"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="GND" pad="TP"/>
<contactref element="U$3" pad="2"/>
<contactref element="NMOS4" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="U$6" pad="3"/>
</signal>
<signal name="PA5">
<contactref element="IC1" pad="8"/>
<contactref element="U$2" pad="1"/>
<contactref element="PMOS3" pad="3"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="PA3">
<contactref element="IC1" pad="10"/>
<contactref element="NMOS1" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="PA2">
<contactref element="IC1" pad="11"/>
<contactref element="R2" pad="1"/>
<contactref element="NMOS2" pad="3"/>
</signal>
<signal name="PA1">
<contactref element="IC1" pad="12"/>
<contactref element="R3" pad="1"/>
<contactref element="NMOS3" pad="3"/>
</signal>
<signal name="PA4">
<contactref element="U$2" pad="3"/>
<contactref element="PMOS1" pad="3"/>
<contactref element="IC1" pad="9"/>
<contactref element="R6" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="PA7">
<contactref element="IC1" pad="6"/>
<contactref element="R7" pad="2"/>
<contactref element="PMOS2" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="PMOS1" pad="1"/>
<contactref element="U$5" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="PMOS2" pad="1"/>
<contactref element="U$5" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="PMOS3" pad="1"/>
<contactref element="U$5" pad="3"/>
</signal>
<signal name="V+">
<contactref element="PMOS3" pad="2"/>
<contactref element="PMOS1" pad="2"/>
<contactref element="PMOS2" pad="2"/>
<contactref element="V+" pad="TP"/>
<contactref element="R11" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="U$6" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U$1" pad="4"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="RX">
<contactref element="U$1" pad="6"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="PA6">
<contactref element="U$2" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$10">
<contactref element="R9" pad="2"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="5"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="4"/>
<contactref element="U$2" pad="5"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="PA0">
<contactref element="IC1" pad="13"/>
<contactref element="R12" pad="1"/>
<contactref element="NMOS4" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="NMOS4" pad="1"/>
<contactref element="U$4" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="NMOS1" pad="1"/>
<contactref element="U$4" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="NMOS2" pad="1"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="NMOS3" pad="1"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="U$5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
