<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<packages>
<package name="2X03SMD">
</package>
<package name="ELECTRET_2742PBJ-A">
</package>
<package name="USB_MINIB">
</package>
<package name="SJFAB">
</package>
<package name="OP1206">
</package>
<package name="2X02SMD">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="EFOBM">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="QFN/MLF20">
<description>&lt;b&gt;HP-VFQFP-N20&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="DO41Z10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="P-LCC-4-3">
<description>&lt;b&gt;Hyper TOPLED® &lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/</description>
</package>
<package name="P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="TQFP32-08THIN">
</package>
<package name="JACK_2.1MM">
</package>
<package name="JACK_.65MM">
</package>
<package name="2-SMD-5X3MM">
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C1206K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1206 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3216</description>
</package>
<package name="R1206FAB">
</package>
<package name="C1206FAB">
</package>
<package name="1X06SMD">
</package>
<package name="MSOP">
</package>
<package name="SOIC16">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
<package name="5MM">
<description>5mm round through hole part.</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;, 5 lead</description>
</package>
<package name="S008">
<description>Small outline package</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="8-LCC">
</package>
<package name="2X05SMD">
</package>
<package name="SPDTSWITCH">
</package>
<package name="LCC16">
<description>&lt;b&gt;LCC16&lt;/b&gt; Package&lt;p&gt;
Source: http://www.memsic.com/data/products/MXR9500G&amp;M/MXR9500G&amp;M.pdf</description>
</package>
<package name="SMD_COIL">
<description>ELL-CTV series SMD choke coils
:
Panasonic Electronic Components ELL-CTV choke coils, 1.2-100uH, surface mount</description>
</package>
<package name="CSP-4PIN">
<description>Knowles SPU0414HR5H-SB

MEMS microphone, SiSonic series</description>
</package>
<package name="MIC_BOTTOM_PORT">
<description>Knowles SPH0645LM4H-B

I2S Output Digital Microphone, 18-bit precision</description>
</package>
<package name="MIC_MEMS_ANALOG_SPU0414HR5H">
<description>http://www.digikey.com/product-search/en?keywords=423-1134-1-ND%09</description>
</package>
<package name="2X04_THRU">
<description>2x4 header.  

Meant for nRF24L01+, but could be used for any header or 2x4 part.

Extra-wide pads for greater durability in soldering.</description>
</package>
<package name="ELLCTV">
</package>
<package name="PJ-002AH-SMT">
</package>
<package name="DX4R005HJ5_100">
</package>
<package name="DX4R005HJ5">
</package>
<package name="DX4R005HJ5_64">
</package>
<package name="AYZ0102AGRLC">
</package>
<package name="3.5MMTERM">
</package>
<package name="ED555DS-2DS">
</package>
<package name="ED555DS-3DS">
</package>
<package name="MINI-SMA">
<description>mini-SMA diode</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="ELECTRET">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
<pin name="SHIELD" direction="pas"/>
</symbol>
<symbol name="SJFAB">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PHOTOTRANSISTOR">
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PINH2X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
</symbol>
<symbol name="PINH2X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
</symbol>
<symbol name="AVRISP">
<pin name="MISO" direction="pas" function="dot"/>
<pin name="VCC" direction="pas" function="dot"/>
<pin name="SCK" direction="pas" function="dot"/>
<pin name="MOSI" direction="pas" function="dot"/>
<pin name="RST" direction="pas" function="dot"/>
<pin name="GND" direction="pas" function="dot"/>
</symbol>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="ATTINY45">
<pin name="GND"/>
<pin name="PB5/PCINT5/-RESET/ADC0/DW"/>
<pin name="PB3/PCINT3/XTAL1/CLKI/-OC1B/ADC3"/>
<pin name="PB4/PCINT4/XTAL2/CLKO/OC1B/ADC2"/>
<pin name="VCC"/>
<pin name="SCK/USCK/SCL/ADC1/T0/INT0/PCINT2/PB2"/>
<pin name="MISO/DO/AIN1/OC0B/OC1A/PCINT1/PB1"/>
<pin name="MOSI/DI/SDA/AIN0/OC0A/-OC1A/AREF/PCINT0/PB0"/>
</symbol>
<symbol name="N_MOSFET">
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="D">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="REGULATOR">
<pin name="IN"/>
<pin name="GND"/>
<pin name="OUT"/>
</symbol>
<symbol name="CERAMIC_RESONATOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="ATTINY24/44/84">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="(PCINT7/ICP/OC0B/ADC7)PA7"/>
<pin name="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6"/>
<pin name="(PCINT5/OC1B/MISO/DO/ADC5)PA5"/>
<pin name="(PCINT4/T1/SCL/USCK/ADC4)PA4"/>
<pin name="(PCINT3/T0/ADC3)PA3"/>
<pin name="(PCINT2/AIN1/ADC2)PA2"/>
<pin name="(PCINT1/AIN0/ADC1)PA1"/>
<pin name="(PCINT0/AREF/ADC0)PA0"/>
<pin name="(PCINT11/RESET/DW)PB3"/>
<pin name="(PCINT10/INT0/OC0A/CKOUT)PB2"/>
<pin name="(PCINT9/XTAL2)PB1"/>
<pin name="(PCINT8/XTAL1/CLKI)PB0"/>
</symbol>
<symbol name="P_MOSFET">
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="ZENER">
<pin name="ANODE" direction="pas"/>
<pin name="CATHODE" direction="pas"/>
</symbol>
<symbol name="LED-RGB">
<pin name="CGREEN" direction="pas"/>
<pin name="CBLUE" direction="pas"/>
<pin name="CRED" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="23-I/O">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="JACK">
<pin name="PIN"/>
<pin name="CONTACT"/>
<pin name="SHUNT"/>
</symbol>
<symbol name="CRYSTAL">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="C-US">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="FTDI">
<pin name="GND"/>
<pin name="CTS"/>
<pin name="VCC"/>
<pin name="TXD"/>
<pin name="RXD"/>
<pin name="RTS"/>
</symbol>
<symbol name="A4953-H-BRIDGE-MOTOR-DRIVER">
<pin name="GND"/>
<pin name="IN2"/>
<pin name="IN1"/>
<pin name="VREF"/>
<pin name="VBB"/>
<pin name="OUT1"/>
<pin name="LSS"/>
<pin name="OUT2"/>
</symbol>
<symbol name="12-BIT_ADC">
<pin name="CS"/>
<pin name="CH0"/>
<pin name="CH1"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="CLK"/>
<pin name="DOUT"/>
<pin name="DIN"/>
</symbol>
<symbol name="12-BIT_ADC_8CH">
<pin name="CH0"/>
<pin name="CH1"/>
<pin name="CH2"/>
<pin name="CH3"/>
<pin name="CH4"/>
<pin name="CH5"/>
<pin name="CH6"/>
<pin name="CH7"/>
<pin name="VDD"/>
<pin name="VREF"/>
<pin name="AGND"/>
<pin name="CLK"/>
<pin name="DOUT"/>
<pin name="DIN"/>
<pin name="CS"/>
<pin name="DGND"/>
</symbol>
<symbol name="LED">
<description>LED</description>
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="CAP-NONPOLARIZED">
<description>non-polarized capacitor</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="OPAMP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="MXD6235M">
<pin name="PD"/>
<pin name="TP"/>
<pin name="GND" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="Y_OUT"/>
<pin name="X_OUT"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PINH2X5">
<pin name="1" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="SPDTSWITCH">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="ACCEL_MXR9150MZ">
<description>Three-axis surface-mount 3.3V accelerometer</description>
<pin name="DI1"/>
<pin name="VDD1"/>
<pin name="VSA2"/>
<pin name="DI2"/>
<pin name="SCK2"/>
<pin name="ZOUT"/>
<pin name="VDD3"/>
<pin name="XOUT"/>
<pin name="YOUT"/>
<pin name="VDD2"/>
<pin name="VSA1"/>
<pin name="SCK1"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="MEMS_MIC_ANALOG">
<description>Knowles SPU0414HR5H-SB

Amplified SiSonic (TM) Microphone</description>
<pin name="OUT"/>
<pin name="GND"/>
<pin name="GAIN"/>
<pin name="VDD"/>
</symbol>
<symbol name="MEMS_MIC_I2S">
<pin name="VDD"/>
<pin name="WS"/>
<pin name="CLK"/>
<pin name="DATA"/>
<pin name="SEL"/>
<pin name="GND"/>
</symbol>
<symbol name="MIC_MEMS_ANALOG_SPU0414HR5H">
<description>http://www.digikey.com/product-search/en?keywords=423-1134-1-ND%09</description>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="GAIN"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="ATMEGA16U2">
<description>ATmega8U2/16U2/32U2 USB microcontroller</description>
<pin name="UCAP"/>
<pin name="UGND"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="UVCC"/>
<pin name="AVCC"/>
<pin name="XTAL1"/>
<pin name="(PC0)XTAL2"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="(PCINT10)PC4"/>
<pin name="(PCINT9/OC.1B)PC5"/>
<pin name="(PC1/DW)!RESET"/>
<pin name="(OC.1A/PCINT8)PC6"/>
<pin name="(INT4/ICP1/CLKO)PC7"/>
<pin name="(PCINT7/OC.0A/OC.1C)PB7"/>
<pin name="(PCINT6)PB6"/>
<pin name="(PCINT5)PB5"/>
<pin name="(T1/PCINT4)PB4"/>
<pin name="(PDO/MISO/PCINT3)PB3"/>
<pin name="(PDI/MOSI/PCINT2)PB2"/>
<pin name="(SCLK/PCINT1)PB1"/>
<pin name="(!SS!/PCINT0)PB0"/>
<pin name="(!CTS!/!HWB!/AIN6/T0/INT7)PD7"/>
<pin name="(!RTS!/AIN5/INT6)PD6"/>
<pin name="(XCK/AIN4/PCINT12)PD5"/>
<pin name="(PCINT11/AIN2)PC2"/>
<pin name="(OC.0B/INT0)PD0"/>
<pin name="(AIN0/INT1)PD1"/>
<pin name="(RXD1/AIN1/INT2)PD2"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(INT5/AIN3)PD4"/>
</symbol>
<symbol name="NRF24L01+">
<description>nRF24L01+ 2.4GHz Wireless transceiver module</description>
<pin name="GND"/>
<pin name="CE"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="VCC"/>
<pin name="CSN"/>
<pin name="MOSI"/>
<pin name="IRQ"/>
</symbol>
<symbol name="COIL">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="DC-POWER-JACK">
<pin name="PIN1" direction="pwr"/>
<pin name="SHUNT" direction="pwr"/>
<pin name="CONTACT" direction="pwr"/>
<pin name="PIN2" direction="pwr"/>
</symbol>
<symbol name="USB-1">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS"/>
<pin name="GND"/>
</symbol>
<symbol name="SWITCH-SPDT">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
</symbol>
<symbol name="1X2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
<symbol name="1X3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="DIODE">
<pin name="KATHODE"/>
<pin name="ANODE"/>
</symbol>
<symbol name="78ADJ">
<pin name="IN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OUT@1" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ELECTRET">
<gates>
<gate name="G$1" symbol="ELECTRET"/>
</gates>
<devices>
<device name="" package="ELECTRET_2742PBJ-A">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB_MINIB">
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="" package="USB_MINIB">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SHIELD" pad="SHIELD@1 SHIELD@2 SHIELD@3 SHIELD@4"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOLDER_JUMPER">
<gates>
<gate name="G$1" symbol="SJFAB"/>
</gates>
<devices>
<device name="" package="SJFAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PHOTOTRANSISTOR-NPN">
<gates>
<gate name="G$1" symbol="PHOTOTRANSISTOR"/>
</gates>
<devices>
<device name="1206" package="OP1206">
<connects>
<connect gate="G$1" pin="C" pad="COLLECTOR"/>
<connect gate="G$1" pin="E" pad="EMITTER"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X2-SMD">
<gates>
<gate name="G$1" symbol="PINH2X2"/>
</gates>
<devices>
<device name="" package="2X02SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X3-SMD" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINH2X3"/>
</gates>
<devices>
<device name="" package="2X03SMD">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AVRISP">
<gates>
<gate name="G$1" symbol="AVRISP"/>
</gates>
<devices>
<device name="SMD" package="2X03SMD">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="2X03">
<connects>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="MISO" pad="1"/>
<connect gate="G$1" pin="MOSI" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6MM_SWITCH" prefix="S" uservalue="yes">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
<gates>
<gate name="2" symbol="TS2"/>
</gates>
<devices>
<device name="6MM_SWITCH" package="6MM_SWITCH">
<connects>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="P1" pad="2"/>
<connect gate="2" pin="S" pad="3"/>
<connect gate="2" pin="S1" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY45">
<gates>
<gate name="G$1" symbol="ATTINY45"/>
</gates>
<devices>
<device name="SI" package="SOIC8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="MISO/DO/AIN1/OC0B/OC1A/PCINT1/PB1" pad="6"/>
<connect gate="G$1" pin="MOSI/DI/SDA/AIN0/OC0A/-OC1A/AREF/PCINT0/PB0" pad="5"/>
<connect gate="G$1" pin="PB3/PCINT3/XTAL1/CLKI/-OC1B/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/XTAL2/CLKO/OC1B/ADC2" pad="3"/>
<connect gate="G$1" pin="PB5/PCINT5/-RESET/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="SCK/USCK/SCL/ADC1/T0/INT0/PCINT2/PB2" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NMOSFET" prefix="T" uservalue="yes">
<description>&lt;b&gt;MOS FET&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="N_MOSFET"/>
</gates>
<devices>
<device name="SOT23" package="SOT-23">
<connects>
<connect gate="A" pin="D" pad="1"/>
<connect gate="A" pin="G" pad="3"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TO252" package="TO252">
<connects>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D" uservalue="yes">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
high speed (Philips)</description>
<gates>
<gate name="G$1" symbol="D"/>
</gates>
<devices>
<device name="SOD123" package="SOD123">
<connects>
<connect gate="G$1" pin="A" pad="ANODE"/>
<connect gate="G$1" pin="C" pad="CATHODE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REGULATOR" prefix="IC" uservalue="yes">
<gates>
<gate name="G$1" symbol="REGULATOR"/>
</gates>
<devices>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESONATOR">
<gates>
<gate name="G$1" symbol="CERAMIC_RESONATOR"/>
</gates>
<devices>
<device name="" package="EFOBM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY44" prefix="IC">
<gates>
<gate name="1" symbol="ATTINY24/44/84"/>
</gates>
<devices>
<device name="-SSU" package="SOIC14">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="4"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-PU" package="DIL14">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="13"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="12"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="5"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="4"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="11"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="10"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="9"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="8"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="7"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="6"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="2"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="3"/>
<connect gate="1" pin="GND" pad="14"/>
<connect gate="1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MU" package="QFN/MLF20">
<connects>
<connect gate="1" pin="(PCINT0/AREF/ADC0)PA0" pad="5"/>
<connect gate="1" pin="(PCINT1/AIN0/ADC1)PA1" pad="4"/>
<connect gate="1" pin="(PCINT10/INT0/OC0A/CKOUT)PB2" pad="14"/>
<connect gate="1" pin="(PCINT11/RESET/DW)PB3" pad="13"/>
<connect gate="1" pin="(PCINT2/AIN1/ADC2)PA2" pad="3"/>
<connect gate="1" pin="(PCINT3/T0/ADC3)PA3" pad="2"/>
<connect gate="1" pin="(PCINT4/T1/SCL/USCK/ADC4)PA4" pad="1"/>
<connect gate="1" pin="(PCINT5/OC1B/MISO/DO/ADC5)PA5" pad="20"/>
<connect gate="1" pin="(PCINT6/OC1A/SDA/MOSI/ADC6)PA6" pad="16"/>
<connect gate="1" pin="(PCINT7/ICP/OC0B/ADC7)PA7" pad="15"/>
<connect gate="1" pin="(PCINT8/XTAL1/CLKI)PB0" pad="11"/>
<connect gate="1" pin="(PCINT9/XTAL2)PB1" pad="12"/>
<connect gate="1" pin="GND" pad="8"/>
<connect gate="1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PMOSFET" prefix="T" uservalue="yes">
<description>&lt;b&gt;MOS FET&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="P_MOSFET"/>
</gates>
<devices>
<device name="SOT23" package="SOT-23">
<connects>
<connect gate="A" pin="D" pad="1"/>
<connect gate="A" pin="G" pad="3"/>
<connect gate="A" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZENER_DIODE" prefix="D" uservalue="yes">
<description>zener diode</description>
<gates>
<gate name="1" symbol="ZENER"/>
</gates>
<devices>
<device name="DO41Z10" package="DO41Z10">
<connects>
<connect gate="1" pin="ANODE" pad="A"/>
<connect gate="1" pin="CATHODE" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOD123" package="SOD123">
<connects>
<connect gate="1" pin="ANODE" pad="ANODE"/>
<connect gate="1" pin="CATHODE" pad="CATHODE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LEDRGBOLD" prefix="LED" uservalue="yes">
<description>&lt;b&gt;OSRAM&lt;/b&gt;&lt;p&gt;
&lt;u&gt;Hyper Multi TOPLED® Hyper-Bright LED&lt;/u&gt;&lt;br&gt;
LATB T686&lt;br&gt;

&lt;p&gt;
Source: http://www.osram.convergy.de/</description>
<gates>
<gate name="G$1" symbol="LED-RGB"/>
</gates>
<devices>
<device name="" package="P-LCC-4-3">
<connects>
<connect gate="G$1" pin="A2" pad="A"/>
<connect gate="G$1" pin="CBLUE" pad="B"/>
<connect gate="G$1" pin="CGREEN" pad="G"/>
<connect gate="G$1" pin="CRED" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LEDRGBNEW">
<gates>
<gate name="G$1" symbol="LED-RGB"/>
</gates>
<devices>
<device name="" package="P-LCC-4">
<connects>
<connect gate="G$1" pin="A2" pad="A"/>
<connect gate="G$1" pin="CBLUE" pad="B"/>
<connect gate="G$1" pin="CGREEN" pad="G"/>
<connect gate="G$1" pin="CRED" pad="R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA88-THIN" prefix="IC">
<gates>
<gate name="G$1" symbol="23-I/O"/>
</gates>
<devices>
<device name="" package="TQFP32-08THIN">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JACK" prefix="J">
<gates>
<gate name="G$1" symbol="JACK"/>
</gates>
<devices>
<device name="2.1MM" package="JACK_2.1MM">
<connects>
<connect gate="G$1" pin="CONTACT" pad="CONTACT"/>
<connect gate="G$1" pin="PIN" pad="PIN"/>
<connect gate="G$1" pin="SHUNT" pad="SHUNT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name=".65MM" package="JACK_.65MM">
<connects>
<connect gate="G$1" pin="CONTACT" pad="SHUNT"/>
<connect gate="G$1" pin="PIN" pad="PIN"/>
<connect gate="G$1" pin="SHUNT" pad="CONTACT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTAL">
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="" package="2-SMD-5X3MM">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-US" prefix="C">
<gates>
<gate name="G$1" symbol="C-US"/>
</gates>
<devices>
<device name="1206" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206K" package="C1206K">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="C1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RES-US" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor (US Symbol)&lt;/b&gt;
&lt;p&gt;
Variants with postfix FAB are widened to allow the routing of internal traces</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="1206" package="R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206W" package="R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="1206FAB" package="R1206FAB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTDI-SMD-HEADER">
<gates>
<gate name="G$1" symbol="FTDI"/>
</gates>
<devices>
<device name="" package="1X06SMD">
<connects>
<connect gate="G$1" pin="CTS" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="RTS" pad="6"/>
<connect gate="G$1" pin="RXD" pad="5"/>
<connect gate="G$1" pin="TXD" pad="4"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A4953-H-BRIDGE-MOTOR-DRIVER">
<gates>
<gate name="G$1" symbol="A4953-H-BRIDGE-MOTOR-DRIVER"/>
</gates>
<devices>
<device name="" package="SOIC8">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="LSS" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="6"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="VBB" pad="5"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12-BIT_DUAL_ADC_MSOP">
<gates>
<gate name="G$1" symbol="12-BIT_ADC"/>
</gates>
<devices>
<device name="" package="MSOP">
<connects>
<connect gate="G$1" pin="CH0" pad="P$2"/>
<connect gate="G$1" pin="CH1" pad="P$3"/>
<connect gate="G$1" pin="CLK" pad="P$7"/>
<connect gate="G$1" pin="CS" pad="P$1"/>
<connect gate="G$1" pin="DIN" pad="P$5"/>
<connect gate="G$1" pin="DOUT" pad="P$6"/>
<connect gate="G$1" pin="VDD" pad="P$8"/>
<connect gate="G$1" pin="VSS" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="12-BIT_ADC_8CH_SOIC">
<gates>
<gate name="G$1" symbol="12-BIT_ADC_8CH"/>
</gates>
<devices>
<device name="" package="SOIC16">
<connects>
<connect gate="G$1" pin="AGND" pad="14"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CH4" pad="5"/>
<connect gate="G$1" pin="CH5" pad="6"/>
<connect gate="G$1" pin="CH6" pad="7"/>
<connect gate="G$1" pin="CH7" pad="8"/>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="CS" pad="10"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="DIN" pad="11"/>
<connect gate="G$1" pin="DOUT" pad="12"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED">
<description>LED</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED1206">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB1206" package="LED1206FAB">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="5MM">
<connects>
<connect gate="G$1" pin="A" pad="IN"/>
<connect gate="G$1" pin="C" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP-UNPOLARIZED" prefix="C" uservalue="yes">
<gates>
<gate name="&gt;NAME" symbol="CAP-NONPOLARIZED"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FAB" package="C1206FAB">
<connects>
<connect gate="&gt;NAME" pin="1" pad="1"/>
<connect gate="&gt;NAME" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPAMP" prefix="IC">
<description>&lt;b&gt;Rail-to-Rail Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Single-Supply, MicroAmplifier(TM) Series</description>
<gates>
<gate name="G$1" symbol="OPAMP"/>
</gates>
<devices>
<device name="SOT23-5" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SO08" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MXD6235M">
<gates>
<gate name="G$1" symbol="MXD6235M"/>
</gates>
<devices>
<device name="-SMD" package="8-LCC">
<connects>
<connect gate="G$1" pin="GND" pad="P$3"/>
<connect gate="G$1" pin="NC" pad="P$4"/>
<connect gate="G$1" pin="NC2" pad="P$5"/>
<connect gate="G$1" pin="PD" pad="P$1"/>
<connect gate="G$1" pin="TP" pad="P$2"/>
<connect gate="G$1" pin="VDD" pad="P$8"/>
<connect gate="G$1" pin="X_OUT" pad="P$7"/>
<connect gate="G$1" pin="Y_OUT" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHD-2X5-SMD">
<gates>
<gate name="G$1" symbol="PINH2X5"/>
</gates>
<devices>
<device name="" package="2X05SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPDTSWITCH">
<gates>
<gate name="G$1" symbol="SPDTSWITCH"/>
</gates>
<devices>
<device name="" package="SPDTSWITCH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACCEL_MXR9150MZ">
<description>3-axis 3.3V accelerometer</description>
<gates>
<gate name="G$1" symbol="ACCEL_MXR9150MZ"/>
</gates>
<devices>
<device name="" package="LCC16">
<connects>
<connect gate="G$1" pin="DI1" pad="5"/>
<connect gate="G$1" pin="DI2" pad="16"/>
<connect gate="G$1" pin="SCK1" pad="6"/>
<connect gate="G$1" pin="SCK2" pad="15"/>
<connect gate="G$1" pin="VDD1" pad="4"/>
<connect gate="G$1" pin="VDD2" pad="11"/>
<connect gate="G$1" pin="VDD3" pad="14"/>
<connect gate="G$1" pin="VSA1" pad="8"/>
<connect gate="G$1" pin="VSA2" pad="3"/>
<connect gate="G$1" pin="XOUT" pad="13"/>
<connect gate="G$1" pin="YOUT" pad="12"/>
<connect gate="G$1" pin="ZOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L" uservalue="yes">
<description>&lt;b&gt;Inductors&lt;/b&gt;&lt;p&gt;
Basic Inductor/Choke - 0603 and 1206. Footprints are not proven and vary greatly between part numbers.&lt;br&gt;
INDUCTOR POWER 3.3UH 4.0A SMD&lt;br&gt;
0.197" L x 0.197" W x 0.177" H (5.00mm x 5.00mm x 4.50mm)</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="" package="SMD_COIL">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEMS_MIC_SPU0414HR5H-SB">
<gates>
<gate name="G$1" symbol="MEMS_MIC_ANALOG"/>
</gates>
<devices>
<device name="" package="CSP-4PIN">
<connects>
<connect gate="G$1" pin="GAIN" pad="P$3"/>
<connect gate="G$1" pin="GND" pad="P$2"/>
<connect gate="G$1" pin="OUT" pad="P$4"/>
<connect gate="G$1" pin="VDD" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEMS_MIC_SPH0645LM4H-B">
<gates>
<gate name="G$1" symbol="MEMS_MIC_I2S"/>
</gates>
<devices>
<device name="I2S" package="MIC_BOTTOM_PORT">
<connects>
<connect gate="G$1" pin="CLK" pad="4"/>
<connect gate="G$1" pin="DATA" pad="6"/>
<connect gate="G$1" pin="GND" pad="3 P$1"/>
<connect gate="G$1" pin="SEL" pad="2"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="WS" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC_MEMS_ANALOG_SPU0414HR5H">
<gates>
<gate name="G$1" symbol="MIC_MEMS_ANALOG_SPU0414HR5H"/>
</gates>
<devices>
<device name="" package="MIC_MEMS_ANALOG_SPU0414HR5H">
<connects>
<connect gate="G$1" pin="GAIN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA16U2">
<gates>
<gate name="G$1" symbol="ATMEGA16U2"/>
</gates>
<devices>
<device name="-TQ" package="TQFP32-08THIN">
<connects>
<connect gate="G$1" pin="(!CTS!/!HWB!/AIN6/T0/INT7)PD7" pad="13"/>
<connect gate="G$1" pin="(!RTS!/AIN5/INT6)PD6" pad="12"/>
<connect gate="G$1" pin="(!SS!/PCINT0)PB0" pad="14"/>
<connect gate="G$1" pin="(AIN0/INT1)PD1" pad="7"/>
<connect gate="G$1" pin="(INT4/ICP1/CLKO)PC7" pad="22"/>
<connect gate="G$1" pin="(INT5/AIN3)PD4" pad="10"/>
<connect gate="G$1" pin="(OC.0B/INT0)PD0" pad="6"/>
<connect gate="G$1" pin="(OC.1A/PCINT8)PC6" pad="23"/>
<connect gate="G$1" pin="(PC0)XTAL2" pad="2"/>
<connect gate="G$1" pin="(PC1/DW)!RESET" pad="24"/>
<connect gate="G$1" pin="(PCINT10)PC4" pad="26"/>
<connect gate="G$1" pin="(PCINT11/AIN2)PC2" pad="5"/>
<connect gate="G$1" pin="(PCINT5)PB5" pad="19"/>
<connect gate="G$1" pin="(PCINT6)PB6" pad="20"/>
<connect gate="G$1" pin="(PCINT7/OC.0A/OC.1C)PB7" pad="21"/>
<connect gate="G$1" pin="(PCINT9/OC.1B)PC5" pad="25"/>
<connect gate="G$1" pin="(PDI/MOSI/PCINT2)PB2" pad="16"/>
<connect gate="G$1" pin="(PDO/MISO/PCINT3)PB3" pad="17"/>
<connect gate="G$1" pin="(RXD1/AIN1/INT2)PD2" pad="8"/>
<connect gate="G$1" pin="(SCLK/PCINT1)PB1" pad="15"/>
<connect gate="G$1" pin="(T1/PCINT4)PB4" pad="18"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="9"/>
<connect gate="G$1" pin="(XCK/AIN4/PCINT12)PD5" pad="11"/>
<connect gate="G$1" pin="AVCC" pad="32"/>
<connect gate="G$1" pin="D+" pad="29"/>
<connect gate="G$1" pin="D-" pad="30"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="UCAP" pad="27"/>
<connect gate="G$1" pin="UGND" pad="28"/>
<connect gate="G$1" pin="UVCC" pad="31"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NRF24L01+">
<description>nRF24L01+ 2.4GHz Wireless Transceiver module</description>
<gates>
<gate name="G$1" symbol="NRF24L01+"/>
</gates>
<devices>
<device name="" package="2X04_THRU">
<connects>
<connect gate="G$1" pin="CE" pad="2"/>
<connect gate="G$1" pin="CSN" pad="7"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IRQ" pad="5"/>
<connect gate="G$1" pin="MISO" pad="4"/>
<connect gate="G$1" pin="MOSI" pad="6"/>
<connect gate="G$1" pin="SCK" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CHOKE" prefix="L">
<description>SMD choke (inductor/coil) ELL-CTV000M as found in the fablab inventory.

&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="U1" symbol="COIL"/>
</gates>
<devices>
<device name="SMD" package="ELLCTV">
<connects>
<connect gate="U1" pin="P$1" pad="1"/>
<connect gate="U1" pin="P$2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JACK-2.1MM" prefix="J">
<description>SMD DC power jack PJ-002AH-SMT As found in the fablab inventory.

&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="DC-POWER-JACK"/>
</gates>
<devices>
<device name="" package="PJ-002AH-SMT">
<connects>
<connect gate="G$1" pin="CONTACT" pad="CONTACT"/>
<connect gate="G$1" pin="PIN1" pad="PIN1"/>
<connect gate="G$1" pin="PIN2" pad="PIN2"/>
<connect gate="G$1" pin="SHUNT" pad="SHUNT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICRO-USB">
<description>SMD micro USB connector as found in the fablab inventory. 
Three footprint variants included: 
&lt;ol&gt;
&lt;li&gt; original, as described by manufacturer's datasheet
&lt;li&gt; for milling with the 1/100" bit
&lt;li&gt; for milling with the 1/64" bit
&lt;/ol&gt;
&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="USB-1"/>
</gates>
<devices>
<device name="_1/100" package="DX4R005HJ5_100">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_ORIG" package="DX4R005HJ5">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1/64" package="DX4R005HJ5_64">
<connects>
<connect gate="G$1" pin="D+" pad="D+"/>
<connect gate="G$1" pin="D-" pad="D-"/>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="VBUS" pad="VBUS"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SLIDE-SWITCH" prefix="S">
<description>SMD slide-switch AYZ0102AGRLC as found in the fablab inventory.  Includes the mounting holes.

&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="SWITCH-SPDT"/>
</gates>
<devices>
<device name="" package="AYZ0102AGRLC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TERM-1X02" prefix="J">
<description>3.5mm terminal block, 2 positions ED555-2DS as found in the fablab inventory. 
&lt;p&gt;Stolen from &lt;a href="http://www.ladyada.net/library/pcb/eaglelibrary.html"&gt;Adafruit&lt;/a&gt;, adapted by Zaerc.</description>
<gates>
<gate name="G$1" symbol="1X2"/>
</gates>
<devices>
<device name="-ADAFRUIT" package="3.5MMTERM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-FABLAB" package="ED555DS-2DS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TERM-1X03">
<description>3.5mm terminal block, 3 positions ED555-3DS as found in the fablab inventory.
&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="1X3"/>
</gates>
<devices>
<device name="'-FABLAB'" package="ED555DS-3DS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CDBM1100-G" prefix="D">
<description>Diode schottky 100V 1A mini-SMA as found in the fablab inventory
&lt;ul&gt;
&lt;li&gt;Reverse Voltage: 100 Volts
&lt;li&gt;Forward Current: 1.0 Amp
&lt;li&gt;Maximum forward voltage: 0.85 Volts
&lt;/ul&gt;
&lt;p&gt;Made by Zaerc.</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="" package="MINI-SMA">
<connects>
<connect gate="G$1" pin="ANODE" pad="ANODE"/>
<connect gate="G$1" pin="KATHODE" pad="KATHODE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V_REG_LM1117" prefix="U" uservalue="yes">
<description>&lt;b&gt;Voltage Regulator LM1117&lt;/b&gt;
Standard adjustable voltage regulator but in SMD form. Spark Fun Electronics SKU : COM-00595</description>
<gates>
<gate name="G$1" symbol="78ADJ"/>
</gates>
<devices>
<device name="SOT223" package="SOT223">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="OUT@1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="VREG-08170"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
