<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="20.32" width="0.254" layer="20"/>
<wire x1="0" y1="20.32" x2="23.622" y2="20.32" width="0.254" layer="20"/>
<wire x1="23.622" y1="20.32" x2="23.622" y2="0" width="0.254" layer="20"/>
<wire x1="23.622" y1="0" x2="0" y2="0" width="0.254" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;, 5 lead</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TRIMPOT-SMD-3MM-CLOSED">
<description>&lt;h3&gt;Trimpot - SMD, 3mm Square, Closed-Frame&lt;/h3&gt;
&lt;p&gt;Used on e.g. &lt;a href="https://www.sparkfun.com/products/12779"&gt;EasyDriver - Stepper Motor Driver&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.bitechnologies.com/pdfs/22.pdf"&gt;Datasheet&lt;/a&gt; (22AR10KTR)&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206" value="CAP-US1206 10uF"/>
<element name="C2" library="fab" package="C1206" value="CAP-US1206 10uF"/>
<element name="IC1" library="fab" package="SOT23-5" value="OPAMPSOT23-5"/>
<element name="R1" library="fab" package="R1206" value="100k"/>
<element name="R4" library="fab" package="R1206" value="10k"/>
<element name="R5" library="fab" package="R1206" value="10k"/>
<element name="R6" library="fab" package="R1206" value="10k"/>
<element name="R7" library="fab" package="R1206" value="1M"/>
<element name="U$1" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="VR1" library="SparkFun-Resistors" package="TRIMPOT-SMD-3MM-CLOSED" value="100k">
<attribute name="PROD_ID" value="RES-09285"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="2"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="5"/>
<contactref element="R5" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="VR1" pad="3"/>
</signal>
<signal name="+5V">
<contactref element="U$1" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="VR1" pad="2"/>
</signal>
<signal name="OA_OUTPUT">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="C2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
