<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="14.478" y1="0" x2="52.756" y2="0" width="0" layer="20"/>
<wire x1="52.756" y1="0" x2="52.756" y2="26.66" width="0" layer="20"/>
<wire x1="52.756" y1="26.66" x2="14.478" y2="26.66" width="0" layer="20"/>
<wire x1="14.478" y1="26.66" x2="14.478" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="1X06SMD">
</package>
<package name="2X03SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1uF"/>
<element name="IC1" library="fab" package="SOIC14" value="attiny44"/>
<element name="J1" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="J2" library="fab" package="2X03SMD" value="ISP"/>
<element name="L1" library="fab" package="LED1206FAB" value="red"/>
<element name="L2" library="fab" package="LED1206FAB" value="wht"/>
<element name="L3" library="fab" package="LED1206FAB" value="wht"/>
<element name="L4" library="fab" package="LED1206FAB" value="wht"/>
<element name="L5" library="fab" package="LED1206FAB" value="wht"/>
<element name="R1" library="fab" package="R1206FAB" value="10k"/>
<element name="R2" library="fab" package="R1206FAB" value="500"/>
<element name="R3" library="fab" package="R1206FAB" value="100"/>
<element name="R4" library="fab" package="R1206FAB" value="100"/>
<element name="R5" library="fab" package="R1206FAB" value="100"/>
<element name="R6" library="fab" package="R1206FAB" value="100"/>
<element name="R7" library="fab" package="R1206FAB" value=""/>
<element name="R8" library="fab" package="R1206FAB" value=""/>
<element name="L6" library="fab" package="LED1206FAB" value="s-wht"/>
<element name="L7" library="fab" package="LED1206FAB" value="s-wht"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="2"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="2"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="2"/>
<contactref element="L4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="2"/>
<contactref element="L5" pad="1"/>
</signal>
<signal name="RST">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="5V">
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="L1" pad="2"/>
<contactref element="L2" pad="2"/>
<contactref element="L3" pad="2"/>
<contactref element="L4" pad="2"/>
<contactref element="L5" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="6"/>
<contactref element="L6" pad="2"/>
<contactref element="L7" pad="2"/>
</signal>
<signal name="L2">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="L3">
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="L4">
<contactref element="R5" pad="1"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="L5">
<contactref element="R6" pad="1"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="TX">
<contactref element="J1" pad="4"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="RX">
<contactref element="J1" pad="5"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="7"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="8"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="IC1" pad="9"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="L6">
<contactref element="R7" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="L7">
<contactref element="IC1" pad="6"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R7" pad="2"/>
<contactref element="L6" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R8" pad="2"/>
<contactref element="L7" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
