<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0.127" x2="42.596" y2="0.127" width="0" layer="20"/>
<wire x1="42.596" y1="0.127" x2="42.723" y2="36.566" width="0" layer="20"/>
<wire x1="42.723" y1="36.566" x2="0" y2="36.693" width="0" layer="20"/>
<wire x1="0" y1="36.693" x2="0" y2="0.127" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="TQFP32-08THIN">
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="EFOBM">
</package>
<package name="1X06SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="2X03SMD">
</package>
<package name="2X02SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1uF"/>
<element name="C2" library="fab" package="C1206FAB" value="0.1uF"/>
<element name="IC1" library="fab" package="TQFP32-08THIN" value="ATMEGA88-THIN"/>
<element name="R1" library="fab" package="R1206FAB" value="1k"/>
<element name="R2" library="fab" package="R1206FAB" value="10k"/>
<element name="R3" library="fab" package="R1206FAB" value="0"/>
<element name="R4" library="fab" package="R1206FAB" value="1M"/>
<element name="R5" library="fab" package="R1206FAB" value="1M"/>
<element name="S1" library="fab" package="6MM_SWITCH" value=""/>
<element name="U$1" library="fab" package="EFOBM" value="RESONATOR"/>
<element name="U$2" library="fab" package="1X06SMD" value="FTDI-SMD-HEADER"/>
<element name="U$3" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="U$4" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$5" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$6" library="fab" package="2X02SMD" value="PINHD-2X2-SMD"/>
<element name="C3" library="fab" package="C1206FAB" value="1uF"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="C2" pad="2"/>
<contactref element="IC1" pad="29"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="3"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="S$2">
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="IC1" pad="21"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$5" pad="6"/>
</signal>
<signal name="MISO">
<contactref element="U$5" pad="1"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="SCK">
<contactref element="U$5" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="S$5">
<contactref element="C2" pad="1"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="RST">
<contactref element="U$5" pad="5"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="S$4">
<contactref element="U$5" pad="2"/>
</signal>
<signal name="S$3">
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="3"/>
</signal>
<signal name="MOSI">
<contactref element="U$5" pad="4"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$5">
<contactref element="U$3" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="2"/>
</signal>
<signal name="PD2">
<contactref element="U$2" pad="2"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="PD0">
<contactref element="U$2" pad="4"/>
<contactref element="IC1" pad="30"/>
</signal>
<signal name="PD1">
<contactref element="U$2" pad="5"/>
<contactref element="IC1" pad="31"/>
</signal>
<signal name="PB2">
<contactref element="U$4" pad="1"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="PB0">
<contactref element="U$4" pad="3"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="PD6">
<contactref element="U$4" pad="5"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="PB1">
<contactref element="U$4" pad="2"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="PD7">
<contactref element="U$4" pad="4"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="PD5">
<contactref element="U$4" pad="6"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="PC1">
<contactref element="IC1" pad="24"/>
</signal>
<signal name="S$6">
</signal>
<signal name="S$7">
</signal>
<signal name="S$8">
</signal>
<signal name="S$10">
</signal>
<signal name="S$11">
</signal>
<signal name="S$9">
</signal>
<signal name="S$12">
</signal>
<signal name="S$14">
</signal>
<signal name="S$1">
</signal>
</signals>
</board>
</drawing>
</eagle>
