<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="-3.937" y1="1.27" x2="51.816" y2="1.27" width="0" layer="20"/>
<wire x1="51.816" y1="1.27" x2="51.796" y2="26.467" width="0" layer="20"/>
<wire x1="51.796" y1="26.467" x2="-3.937" y2="26.467" width="0" layer="20"/>
<wire x1="-3.937" y1="26.467" x2="-3.937" y2="1.27" width="0" layer="20"/>
</plain>
<libraries>
<library name="fabPatil">
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="2X03SMD">
<description>2x5SMD</description>
</package>
<package name="1X06-SMD">
</package>
<package name="USB-A-PCB">
<description>Card-edge USB A connector.

For boards designed to be plugged directly into a USB slot. If possible, ensure that your PCB is about 2.4mm thick to fit snugly.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="fabPatil" package="SO08-EIAJ" value="Tiny45">
<attribute name="PROD_ID" value="IC-08922"/>
<attribute name="VALUE" value="Tiny45-20-SMT"/>
</element>
<element name="D1" library="fabPatil" package="SOD123" value=""/>
<element name="D2" library="fabPatil" package="SOD123" value=""/>
<element name="R1" library="fabPatil" package="1206" value="49"/>
<element name="R2" library="fabPatil" package="1206" value="49"/>
<element name="R3" library="fabPatil" package="1206" value="499"/>
<element name="R4" library="fabPatil" package="1206" value="1K"/>
<element name="U$2" library="fabPatil" package="2X03SMD" value="ISP"/>
<element name="JP1" library="fabPatil" package="1X06-SMD" value=""/>
<element name="C1" library="fabPatil" package="1206" value="0.1uF"/>
<element name="JP2" library="fabPatil" package="USB-A-PCB" value="USBPCB"/>
<element name="R5" library="fabPatil" package="1206" value="470"/>
<element name="R6" library="fabPatil" package="1206" value="470"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="D1" pad="ANODE"/>
<contactref element="D2" pad="ANODE"/>
<contactref element="U$2" pad="6"/>
<contactref element="JP1" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="JP2" pad="GND"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
<contactref element="R4" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="JP1" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="JP2" pad="5V"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="CATHODE"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="JP2" pad="USB_M"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="CATHODE"/>
<contactref element="R2" pad="1"/>
<contactref element="JP2" pad="USB_P"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="3"/>
<contactref element="U1" pad="7"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U$2" pad="5"/>
<contactref element="U1" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="4"/>
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
<contactref element="R6" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
