<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>Vcc and GND</text>
<wire x1="3.175" y1="62.23" x2="3.175" y2="5.715" width="0.4064" layer="20"/>
<wire x1="3.175" y1="5.715" x2="51.1048" y2="5.715" width="0.4064" layer="20"/>
<wire x1="51.1048" y1="5.715" x2="51.1048" y2="62.23" width="0.4064" layer="20"/>
<wire x1="51.1048" y1="62.23" x2="3.175" y2="62.23" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
<package name="R1206FAB">
</package>
<package name="2-SMD-5X3MM">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
</packages>
</library>
<library name="ATMEGA328P-AU">
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1uF">
<attribute name="C1" value="1uF"/>
</element>
<element name="C2" library="fab" package="C1206" value="10pF"/>
<element name="C3" library="fab" package="C1206" value="10pF"/>
<element name="J1" library="fab" package="2X03SMD" value="ISP">
<attribute name="J1" value="ISP"/>
</element>
<element name="J2" library="fab" package="1X06SMD" value="FTDI">
<attribute name="J2" value="FTDI"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="10K">
<attribute name="R1" value="10K"/>
</element>
<element name="U$1" library="fab" package="2-SMD-5X3MM" value="CRYSTAL"/>
<element name="U1" library="ATMEGA328P-AU" package="QFP80P900X900X120-32N" value="ATMEGA328P-AU">
<attribute name="MP" value="ATMEGA328P-AU"/>
<attribute name="MF" value="Atmel"/>
<attribute name="PRICE" value="2.80 USD"/>
<attribute name="DESCRIPTION" value="ATmega Series 20 MHz 32 KB Flash 2 KB SRAM 8-Bit Microcontroller - TQFP-32"/>
<attribute name="PACKAGE" value="TQFP-32 Atmel"/>
<attribute name="AVAILABILITY" value="Good"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="0">
<attribute name="R1" value="10K"/>
</element>
<element name="C4" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="C1" value="1uF"/>
</element>
<element name="U$2" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="R3" library="fab" package="R1206FAB" value="1K">
<attribute name="R1" value="10K"/>
</element>
<element name="R4" library="fab" package="R1206FAB" value="0">
<attribute name="R1" value="10K"/>
</element>
<element name="R5" library="fab" package="R1206FAB" value="0">
<attribute name="R1" value="10K"/>
</element>
<element name="R6" library="fab" package="R1206FAB" value="0">
<attribute name="R1" value="10K"/>
</element>
<element name="R7" library="fab" package="R1206FAB" value="0">
<attribute name="R1" value="10K"/>
</element>
</elements>
<signals>
<signal name="PB0">
<contactref element="U1" pad="12"/>
</signal>
<signal name="PB1">
<contactref element="U1" pad="13"/>
</signal>
<signal name="PB3">
<contactref element="U1" pad="15"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="PB2">
<contactref element="U1" pad="14"/>
</signal>
<signal name="ADC0">
<contactref element="U1" pad="23"/>
</signal>
<signal name="ADC1">
<contactref element="U1" pad="24"/>
</signal>
<signal name="ADC2">
<contactref element="U1" pad="25"/>
</signal>
<signal name="ADC3">
<contactref element="U1" pad="26"/>
</signal>
<signal name="ADC4">
<contactref element="U1" pad="27"/>
</signal>
<signal name="ADC5">
<contactref element="U1" pad="28"/>
</signal>
<signal name="PC6">
<contactref element="U1" pad="29"/>
<contactref element="C4" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="PB4">
<contactref element="U1" pad="16"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="PB5">
<contactref element="U1" pad="17"/>
<contactref element="J1" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="PB6">
<contactref element="U1" pad="7"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="PB7">
<contactref element="U1" pad="8"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="J2" pad="5"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="TXD">
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="INT1">
<contactref element="U1" pad="1"/>
</signal>
<signal name="T0">
<contactref element="U1" pad="2"/>
</signal>
<signal name="T1">
<contactref element="U1" pad="9"/>
</signal>
<signal name="AIN0">
<contactref element="U1" pad="10"/>
</signal>
<signal name="AIN1">
<contactref element="U1" pad="11"/>
</signal>
<signal name="ADC6">
<contactref element="U1" pad="19"/>
</signal>
<signal name="ADC7">
<contactref element="U1" pad="22"/>
</signal>
<signal name="AVCC">
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="PD2">
<contactref element="U1" pad="32"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="6"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="RST">
<contactref element="J1" pad="5"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="X1">
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="X2">
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
