(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 2)
    (tracks 112)
    (zones 0)
    (modules 16)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 /VCC3.3)
  (net 4 "Net-(FTDI1-Pad6)")
  (net 5 /RX)
  (net 6 /TX)
  (net 7 "Net-(FTDI1-Pad2)")
  (net 8 "Net-(MOD1-Pad25)")
  (net 9 "Net-(MOD1-Pad27)")
  (net 10 "Net-(MOD1-Pad28)")
  (net 11 "Net-(MOD1-Pad29)")
  (net 12 "Net-(MOD1-Pad30)")
  (net 13 "Net-(MOD1-Pad31)")
  (net 14 "Net-(MOD1-Pad32)")
  (net 15 "Net-(MOD1-Pad33)")
  (net 16 "Net-(MOD1-Pad36)")
  (net 17 "Net-(MOD1-Pad37)")
  (net 18 "Net-(MOD1-Pad12)")
  (net 19 "Net-(MOD1-Pad11)")
  (net 20 "Net-(MOD1-Pad10)")
  (net 21 "Net-(MOD1-Pad9)")
  (net 22 "Net-(MOD1-Pad8)")
  (net 23 "Net-(MOD1-Pad7)")
  (net 24 "Net-(MOD1-Pad6)")
  (net 25 "Net-(MOD1-Pad5)")
  (net 26 "Net-(MOD1-Pad4)")
  (net 27 /EN)
  (net 28 "Net-(MOD1-Pad22)")
  (net 29 "Net-(MOD1-Pad21)")
  (net 30 "Net-(MOD1-Pad20)")
  (net 31 "Net-(MOD1-Pad19)")
  (net 32 "Net-(MOD1-Pad18)")
  (net 33 "Net-(MOD1-Pad17)")
  (net 34 "Net-(J1-Pad10)")
  (net 35 "Net-(J1-Pad11)")
  (net 36 /Dat2)
  (net 37 "Net-(J1-Pad2)")
  (net 38 "Net-(J1-Pad3)")
  (net 39 "Net-(J1-Pad4)")
  (net 40 "Net-(J1-Pad5)")
  (net 41 "Net-(J1-Pad6)")
  (net 42 "Net-(J1-Pad7)")
  (net 43 "Net-(J1-Pad9)")
  (net 44 "Net-(J1-Pad8)")
  (net 45 /Dat1)
  (net 46 /CLK)
  (net 47 /Dat0)
  (net 48 /CMD)
  (net 49 /Dat3)
  (net 50 "Net-(progrun1-Pad1)")
  (net 51 "Net-(FTDI1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CLK)
    (add_net /CMD)
    (add_net /Dat0)
    (add_net /Dat1)
    (add_net /Dat2)
    (add_net /Dat3)
    (add_net /EN)
    (add_net /RX)
    (add_net /TX)
    (add_net /VCC3.3)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(FTDI1-Pad2)")
    (add_net "Net-(FTDI1-Pad5)")
    (add_net "Net-(FTDI1-Pad6)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(MOD1-Pad10)")
    (add_net "Net-(MOD1-Pad11)")
    (add_net "Net-(MOD1-Pad12)")
    (add_net "Net-(MOD1-Pad17)")
    (add_net "Net-(MOD1-Pad18)")
    (add_net "Net-(MOD1-Pad19)")
    (add_net "Net-(MOD1-Pad20)")
    (add_net "Net-(MOD1-Pad21)")
    (add_net "Net-(MOD1-Pad22)")
    (add_net "Net-(MOD1-Pad25)")
    (add_net "Net-(MOD1-Pad27)")
    (add_net "Net-(MOD1-Pad28)")
    (add_net "Net-(MOD1-Pad29)")
    (add_net "Net-(MOD1-Pad30)")
    (add_net "Net-(MOD1-Pad31)")
    (add_net "Net-(MOD1-Pad32)")
    (add_net "Net-(MOD1-Pad33)")
    (add_net "Net-(MOD1-Pad36)")
    (add_net "Net-(MOD1-Pad37)")
    (add_net "Net-(MOD1-Pad4)")
    (add_net "Net-(MOD1-Pad5)")
    (add_net "Net-(MOD1-Pad6)")
    (add_net "Net-(MOD1-Pad7)")
    (add_net "Net-(MOD1-Pad8)")
    (add_net "Net-(MOD1-Pad9)")
    (add_net "Net-(progrun1-Pad1)")
  )
  (module digikey-footprints:ESP32-WROOM-32D (layer F.Cu) (tedit 5D288F29)
    (at 140.843 91.821 90)
    (attr smd)
    (fp_text reference MOD1 (at 0.01 -16.69 90) (layer F.SilkS))
    (fp_text value ESP32-WROOM-32 (at 0 11.88 90) (layer F.Fab))
    (fp_text user REF** (at 0.01 -5.37 90) (layer F.Fab))
    (pad 39 smd rect (at -1 -1.755 90) (size 5 5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 25 smd rect (at 8.5 8.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(MOD1-Pad25)"))
    (pad 26 smd rect (at 8.5 6.985 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 /Dat1))
    (pad 27 smd rect (at 8.5 5.715 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(MOD1-Pad27)"))
    (pad 28 smd rect (at 8.5 4.445 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(MOD1-Pad28)"))
    (pad 29 smd rect (at 8.5 3.175 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(MOD1-Pad29)"))
    (pad 30 smd rect (at 8.5 1.905 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(MOD1-Pad30)"))
    (pad 31 smd rect (at 8.5 0.635 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(MOD1-Pad31)"))
    (pad 32 smd rect (at 8.5 -0.635 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(MOD1-Pad32)"))
    (pad 33 smd rect (at 8.5 -1.905 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(MOD1-Pad33)"))
    (pad 34 smd rect (at 8.5 -3.175 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /RX))
    (pad 35 smd rect (at 8.5 -4.445 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /TX))
    (pad 36 smd rect (at 8.5 -5.715 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(MOD1-Pad36)"))
    (pad 37 smd rect (at 8.5 -6.985 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(MOD1-Pad37)"))
    (pad 38 smd rect (at 8.5 -8.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -8.5 8.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 /Dat2))
    (pad 13 smd rect (at -8.5 6.985 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 /CLK))
    (pad 12 smd rect (at -8.5 5.715 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(MOD1-Pad12)"))
    (pad 11 smd rect (at -8.5 4.445 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(MOD1-Pad11)"))
    (pad 10 smd rect (at -8.5 3.175 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(MOD1-Pad10)"))
    (pad 9 smd rect (at -8.5 1.905 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(MOD1-Pad9)"))
    (pad 8 smd rect (at -8.5 0.635 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(MOD1-Pad8)"))
    (pad 7 smd rect (at -8.5 -0.635 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(MOD1-Pad7)"))
    (pad 6 smd rect (at -8.5 -1.905 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(MOD1-Pad6)"))
    (pad 5 smd rect (at -8.5 -3.175 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(MOD1-Pad5)"))
    (pad 4 smd rect (at -8.5 -4.445 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(MOD1-Pad4)"))
    (pad 3 smd rect (at -8.5 -5.715 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 /EN))
    (pad 2 smd rect (at -8.5 -6.985 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3.3))
    (pad 24 smd rect (at 5.715 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 /Dat0))
    (pad 23 smd rect (at 4.445 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 /CMD))
    (pad 22 smd rect (at 3.175 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(MOD1-Pad22)"))
    (pad 21 smd rect (at 1.905 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(MOD1-Pad21)"))
    (pad 20 smd rect (at 0.635 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(MOD1-Pad20)"))
    (pad 19 smd rect (at -0.635 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(MOD1-Pad19)"))
    (pad 18 smd rect (at -1.905 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(MOD1-Pad18)"))
    (pad 17 smd rect (at -3.175 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(MOD1-Pad17)"))
    (pad 16 smd rect (at -4.445 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 /Dat3))
    (pad 15 smd rect (at -5.715 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -8.5 -8.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 177.673 82.55)
    (attr smd)
    (fp_text reference R7 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 0 (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(FTDI1-Pad5)"))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 5 /RX))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 154.94 84.455)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R6 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value 10k (at 2.54 1.905) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J1-Pad8)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 45 /Dat1))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 154.94 86.868)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R5 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value 10k (at 2.54 1.905) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J1-Pad7)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 47 /Dat0))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 154.94 89.281)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R4 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value 10k (at 2.54 1.905) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J1-Pad5)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 46 /CLK))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 154.94 91.694)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R3 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value 10k (at 2.54 1.905) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J1-Pad3)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 48 /CMD))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 154.94 93.98)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R2 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value 10k (at 2.54 1.905) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 49 /Dat3))
  )
  (module Connector_Card:microSD_HC_Hirose_DM3D-SF (layer F.Cu) (tedit 5B82D16A)
    (at 164.211 90.805 270)
    (descr "Micro SD, SMD, right-angle, push-pull (https://media.digikey.com/PDF/Data%20Sheets/Hirose%20PDFs/DM3D-SF.pdf)")
    (tags "Micro SD")
    (attr smd)
    (fp_text reference J1 (at -0.025 -7.625 90) (layer F.SilkS))
    (fp_text value Micro_SD_Card_Det_Hirose_DM3AT (at -0.025 6.975 90) (layer F.Fab))
    (fp_text user KEEPOUT (at -0.725 -4.8 90) (layer Cmts.User))
    (fp_text user %R (at -0.025 1.475 90) (layer F.Fab))
    (fp_text user KEEPOUT (at -0.275 -0.525 90) (layer Cmts.User))
    (pad 10 smd rect (at 5.575 -5.45 270) (size 1 1.55) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J1-Pad10)"))
    (pad 11 smd rect (at 5.625 5.225 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J1-Pad11)"))
    (pad 1 smd rect (at 3.175 5.35 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 36 /Dat2))
    (pad 2 smd rect (at 2.075 5.35 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 0.975 5.35 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at -0.125 5.35 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -1.225 5.35 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at -2.325 5.35 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at -3.425 5.35 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J1-Pad7)"))
    (pad 11 smd rect (at 5.975 -3.025 270) (size 0.8 1.4) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J1-Pad11)"))
    (pad 9 smd rect (at -5.65 -3.875 270) (size 1.45 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J1-Pad9)"))
    (pad 11 smd rect (at -5.975 -2.375 270) (size 0.8 1.5) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J1-Pad11)"))
    (pad 11 smd rect (at -5.725 5.225 270) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J1-Pad11)"))
    (pad 8 smd rect (at -4.525 5.35 270) (size 0.7 1.75) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J1-Pad8)"))
    (model ${KISYS3DMOD}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3D-SF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 200000)
    (at 138.811 106.172)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference Reset1 (at 0.127 -4.318) (layer F.SilkS))
    (fp_text value " " (at 0.762 4.445) (layer F.SilkS))
    (fp_text user 4 (at 4.191 2.159) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159) (layer B.SilkS))
    (fp_text user 1 (at -3.683 -2.286) (layer B.SilkS))
    (pad 4 smd rect (at 3.302 2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.302 2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.302 -2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 27 /EN))
    (pad 1 smd rect (at -3.302 -2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 27 /EN))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 146.939 105.918 270)
    (attr smd)
    (fp_text reference R1 (at 0.762 -1.778 90) (layer F.SilkS))
    (fp_text value 10k (at 1.27 1.778 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3.3))
    (pad 1 smd rect (at -1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 27 /EN))
  )
  (module fab:fab-AYZ0102AGRLC (layer F.Cu) (tedit 200000)
    (at 164.338 79.883)
    (attr smd)
    (fp_text reference progrun1 (at 0.381 -3.429) (layer F.SilkS))
    (fp_text value " " (at 0.508 3.937) (layer F.SilkS))
    (pad 3 smd rect (at -2.49936 2.2987) (size 0.99822 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(MOD1-Pad25)"))
    (pad 2 smd rect (at 0 2.2987) (size 0.99822 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 2.49936 2.2987) (size 0.99822 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(progrun1-Pad1)"))
  )
  (module digikey-footprints:SOT-223 (layer F.Cu) (tedit 5D28A60E)
    (at 162.306 103.124 270)
    (attr smd)
    (fp_text reference IC1 (at 0 -6.1 90) (layer F.SilkS))
    (fp_text value 3.3V (at 0.15 5.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0.127 90) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.15 270) (size 3.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3.3))
    (pad 1 smd rect (at -2.3 3.15 270) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 3.15 270) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3.3))
    (pad 3 smd rect (at 2.3 3.15 270) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module fab:fab-1X06SMD (layer F.Cu) (tedit 200000)
    (at 175.768 91.821)
    (attr smd)
    (fp_text reference FTDI1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 3.3V (at 0 0) (layer F.SilkS))
    (pad 6 smd rect (at 0 6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(FTDI1-Pad6)"))
    (pad 5 smd rect (at 0 3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(FTDI1-Pad5)"))
    (pad 4 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 /TX))
    (pad 3 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0 -3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(FTDI1-Pad2)"))
    (pad 1 smd rect (at 0 -6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 150.749 105.791 270)
    (attr smd)
    (fp_text reference C3 (at 0.762 -1.778 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 1.27 1.778 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3.3))
    (pad 1 smd rect (at -1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 168.783 100.838 90)
    (attr smd)
    (fp_text reference C2 (at 0.762 -1.778 90) (layer F.SilkS))
    (fp_text value 1uF (at 1.27 1.778 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCC3.3))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 154.813 105.918 90)
    (attr smd)
    (fp_text reference C1 (at 0.762 -1.778 90) (layer F.SilkS))
    (fp_text value 10uF (at 1.27 1.778 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
)
