(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 201)
    (zones 0)
    (modules 15)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.38 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(IC1-Pad30)")
  (net 5 "Net-(IC1-Pad29)")
  (net 6 "Net-(IC1-Pad26)")
  (net 7 "Net-(IC1-Pad25)")
  (net 8 /RST)
  (net 9 "Net-(IC1-Pad23)")
  (net 10 "Net-(IC1-Pad22)")
  (net 11 "Net-(IC1-Pad21)")
  (net 12 "Net-(IC1-Pad20)")
  (net 13 "Net-(IC1-Pad19)")
  (net 14 "Net-(IC1-Pad18)")
  (net 15 /MISO)
  (net 16 /MOSI)
  (net 17 /SCK)
  (net 18 "Net-(IC1-Pad14)")
  (net 19 "Net-(IC1-Pad13)")
  (net 20 "Net-(IC1-Pad12)")
  (net 21 "Net-(IC1-Pad11)")
  (net 22 "Net-(IC1-Pad10)")
  (net 23 "Net-(IC1-Pad9)")
  (net 24 "Net-(IC1-Pad8)")
  (net 25 "Net-(IC1-Pad7)")
  (net 26 "Net-(IC1-Pad6)")
  (net 27 "Net-(IC1-Pad5)")
  (net 28 "Net-(IC1-Pad2)")
  (net 29 "Net-(IC1-Pad1)")
  (net 30 "Net-(M4-Pad6)")
  (net 31 "Net-(M4-Pad5)")
  (net 32 "Net-(M4-Pad4)")
  (net 33 "Net-(M4-Pad2)")
  (net 34 "Net-(J2-Pad3)")
  (net 35 "Net-(J2-Pad2)")
  (net 36 "Net-(LED1-Pad1)")
  (net 37 "Net-(C1-Pad2)")
  (net 38 "Net-(C1-Pad1)")
  (net 39 "Net-(LED1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RST)
    (add_net /SCK)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad21)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad29)")
    (add_net "Net-(IC1-Pad30)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(M4-Pad2)")
    (add_net "Net-(M4-Pad4)")
    (add_net "Net-(M4-Pad5)")
    (add_net "Net-(M4-Pad6)")
    (add_net VCC)
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 125.5014 74.0918 90)
    (attr smd)
    (fp_text reference R6 (at 0.762 -1.778 90) (layer F.SilkS))
    (fp_text value 0 (at 1.27 1.778 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
  )
  (module usbc:USB-A-PCB (layer F.Cu) (tedit 5DA2A897)
    (at 113.03 72.12)
    (descr "Card-edge USB A connector.\n\nFor boards designed to be plugged directly into a USB slot. If possible, ensure that your PCB is about 2.4mm thick to fit snugly.")
    (fp_text reference J2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value USB_A (at 0 0) (layer F.SilkS) hide)
    (fp_text user >Name (at -1.27 -5.08) (layer F.SilkS))
    (fp_text user >Value (at -1.27 5.08) (layer F.Fab))
    (pad "" smd rect (at 1.55 3.5) (size 11 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
    (pad USB_M smd rect (at 2.05 1) (size 10 1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-Pad2)") (solder_mask_margin 0.1016))
    (pad USB_P smd rect (at 2.05 -1) (size 10 1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J2-Pad3)") (solder_mask_margin 0.1016))
    (pad GND smd rect (at 1.55 -3.5) (size 11 1.5) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.1016))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 122.80646 75.5523 270)
    (attr smd)
    (fp_text reference R8 (at 0.762 -1.778 90) (layer F.SilkS))
    (fp_text value 1k (at 1.27 1.778 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(LED1-Pad2)"))
    (pad 1 smd rect (at -1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module fab:fab-LED1206FAB (layer F.Cu) (tedit 200000)
    (at 124.1298 78.55966 180)
    (descr "LED1206 FAB STYLE (SMALLER PADS TO ALLOW TRACE BETWEEN)")
    (tags "LED1206 FAB STYLE (SMALLER PADS TO ALLOW TRACE BETWEEN)")
    (attr smd)
    (fp_text reference LED1 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value Red (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(LED1-Pad2)"))
    (pad 1 smd rect (at -1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
  )
  (module fab:fab-1X06SMD (layer F.Cu) (tedit 200000)
    (at 153.797 71.374)
    (attr smd)
    (fp_text reference M4 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value FTDI-SMD-HEADER (at 0 0) (layer F.SilkS))
    (pad 6 smd rect (at 0 6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(M4-Pad6)"))
    (pad 5 smd rect (at 0 3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(M4-Pad5)"))
    (pad 4 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(M4-Pad4)"))
    (pad 3 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0 -3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(M4-Pad2)"))
    (pad 1 smd rect (at 0 -6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module fab:fab-TQFP32-08THIN (layer F.Cu) (tedit 200000)
    (at 137.0584 72.898)
    (attr smd)
    (fp_text reference IC1 (at -0.7366 -5.4864) (layer F.SilkS))
    (fp_text value ATMEGA16U2-TQ (at -0.5842 0.8636) (layer F.SilkS))
    (pad 32 smd rect (at -2.79908 -4.36626) (size 0.3556 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 31 smd rect (at -1.99898 -4.2926) (size 0.3556 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 30 smd rect (at -1.19888 -4.2926) (size 0.34798 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad30)"))
    (pad 29 smd rect (at -0.39878 -4.2926) (size 0.34798 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad29)"))
    (pad 28 smd rect (at 0.39878 -4.2926) (size 0.34798 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 27 smd rect (at 1.19888 -4.2926) (size 0.3556 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 26 smd rect (at 1.99898 -4.2926) (size 0.3556 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad26)"))
    (pad 25 smd rect (at 2.79908 -4.36626) (size 0.3556 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad25)"))
    (pad 24 smd rect (at 4.36626 -2.79908) (size 1.1176 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 8 /RST))
    (pad 23 smd rect (at 4.2926 -1.99898) (size 1.27 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad23)"))
    (pad 22 smd rect (at 4.2926 -1.19888) (size 1.27 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad22)"))
    (pad 21 smd rect (at 4.2926 -0.39878) (size 1.27 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad21)"))
    (pad 20 smd rect (at 4.2926 0.39878) (size 1.27 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad20)"))
    (pad 19 smd rect (at 4.2926 1.19888) (size 1.27 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad19)"))
    (pad 18 smd rect (at 4.2926 1.99898) (size 1.27 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad18)"))
    (pad 17 smd rect (at 4.36626 2.79908) (size 1.1176 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 15 /MISO))
    (pad 16 smd rect (at 2.79908 4.36626) (size 0.3556 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 16 /MOSI))
    (pad 15 smd rect (at 1.99898 4.2926) (size 0.3556 1.27) (layers F.Cu F.Paste F.Mask)
      (net 17 /SCK))
    (pad 14 smd rect (at 1.19888 4.2926) (size 0.3556 1.27) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(IC1-Pad14)"))
    (pad 13 smd rect (at 0.39878 4.2926) (size 0.34798 1.27) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(IC1-Pad13)"))
    (pad 12 smd rect (at -0.39878 4.2926) (size 0.34798 1.27) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(IC1-Pad12)"))
    (pad 11 smd rect (at -1.19888 4.2926) (size 0.34798 1.27) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC1-Pad11)"))
    (pad 10 smd rect (at -1.99898 4.2926) (size 0.3556 1.27) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad10)"))
    (pad 9 smd rect (at -2.79908 4.36626) (size 0.3556 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad9)"))
    (pad 8 smd rect (at -4.36626 2.79908) (size 1.1176 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad8)"))
    (pad 7 smd rect (at -4.2926 1.99898) (size 1.27 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad7)"))
    (pad 6 smd rect (at -4.2926 1.19888) (size 1.27 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad6)"))
    (pad 5 smd rect (at -4.2926 0.39878) (size 1.27 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad5)"))
    (pad 4 smd rect (at -4.2926 -0.39878) (size 1.27 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at -4.2926 -1.19888) (size 1.27 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.2926 -1.99898) (size 1.27 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad2)"))
    (pad 1 smd rect (at -4.36626 -2.79908) (size 1.1176 0.3556) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(IC1-Pad1)"))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 128.143 77.216 270)
    (attr smd)
    (fp_text reference R5 (at 0.762 -1.778 90) (layer F.SilkS))
    (fp_text value 499 (at 1.27 1.778 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(M4-Pad4)"))
    (pad 1 smd rect (at -1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad9)"))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 130.556 77.216 270)
    (attr smd)
    (fp_text reference R4 (at 0.762 -1.778 90) (layer F.SilkS))
    (fp_text value 499 (at 1.27 1.778 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(M4-Pad5)"))
    (pad 1 smd rect (at -1.651 0 270) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad8)"))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 143.383 65.405 180)
    (attr smd)
    (fp_text reference R3 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 10k (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 8 /RST))
    (pad 1 smd rect (at -1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 127.381 66.421)
    (attr smd)
    (fp_text reference R2 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 22 (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad30)"))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J2-Pad2)"))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 132.588 65.7225)
    (attr smd)
    (fp_text reference R1 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 22 (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad29)"))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J2-Pad3)"))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 146.685 72.39 90)
    (attr smd)
    (fp_text reference M3 (at -0.635 -4.445 90) (layer F.SilkS))
    (fp_text value ISP (at 0 4.445 90) (layer F.SilkS))
    (pad 6 smd rect (at 2.91846 2.54 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -2.54 2.54 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 /RST))
    (pad 4 smd rect (at 2.91846 0 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 /MOSI))
    (pad 3 smd rect (at -2.54 0 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 17 /SCK))
    (pad 2 smd rect (at 2.91846 -2.54 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -2.54 -2.54 90) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 15 /MISO))
  )
  (module fab:fab-EFOBM (layer F.Cu) (tedit 200000)
    (at 128.651 71.12 180)
    (attr smd)
    (fp_text reference M2 (at 0 0) (layer F.SilkS))
    (fp_text value XTAL (at 0 0) (layer F.SilkS))
    (pad 3 smd rect (at 1.34874 0 90) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad2)"))
    (pad 2 smd rect (at 0 0 90) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.34874 0 270) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(IC1-Pad1)"))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 137.668 65.151)
    (attr smd)
    (fp_text reference C2 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 1uF (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 147.955 65.405)
    (attr smd)
    (fp_text reference C1 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(C1-Pad1)"))
  )
  (gr_line (start 108 62) (end 157 62) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 108 81) (end 108 62) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157 81) (end 108 81) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157 62) (end 157 81) (layer Edge.Cuts) (width 0.05))
  (dimension 18.104517 (width 0.12) (layer F.SilkS)
    (gr_text "18.105 mm" (at 146.834124 71.870598 -81.52885537) (layer F.SilkS))
    (feature1 (pts (xy 156.083 61.341) (xy 146.176746 62.8164)))
    (feature2 (pts (xy 158.75 79.248) (xy 148.843746 80.7234)))
    (crossbar (pts (xy 149.423769 80.637013) (xy 146.756769 62.730013)))
    (arrow1a (pts (xy 146.756769 62.730013) (xy 147.502739 63.75784)))
    (arrow1b (pts (xy 146.756769 62.730013) (xy 146.342693 63.930613)))
    (arrow2a (pts (xy 149.423769 80.637013) (xy 149.837845 79.436413)))
    (arrow2b (pts (xy 149.423769 80.637013) (xy 148.677799 79.609186)))
  )
)
