(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 235)
    (zones 0)
    (modules 20)
    (nets 44)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1 0.3)
    (user_via 1.5 1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.27 1.905)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 +5V)
  (net 4 "Net-(C5-Pad1)")
  (net 5 /Mic)
  (net 6 "Net-(J1-Pad10)")
  (net 7 "Net-(J1-Pad11)")
  (net 8 /Dat2)
  (net 9 /Dat3)
  (net 10 /CMD)
  (net 11 /Dat0)
  (net 12 "Net-(J1-Pad9)")
  (net 13 /Dat1)
  (net 14 "Net-(M1-Pad1)")
  (net 15 "Net-(M2-PadP$4)")
  (net 16 /BootstrapGND)
  (net 17 /LED)
  (net 18 /BTN)
  (net 19 "Net-(MOD1-Pad29)")
  (net 20 "Net-(MOD1-Pad30)")
  (net 21 "Net-(MOD1-Pad31)")
  (net 22 "Net-(MOD1-Pad32)")
  (net 23 "Net-(MOD1-Pad33)")
  (net 24 /RX)
  (net 25 /TX)
  (net 26 "Net-(MOD1-Pad36)")
  (net 27 "Net-(MOD1-Pad37)")
  (net 28 /CLK)
  (net 29 "Net-(MOD1-Pad12)")
  (net 30 "Net-(MOD1-Pad11)")
  (net 31 "Net-(MOD1-Pad10)")
  (net 32 "Net-(MOD1-Pad9)")
  (net 33 "Net-(MOD1-Pad8)")
  (net 34 "Net-(MOD1-Pad6)")
  (net 35 "Net-(MOD1-Pad5)")
  (net 36 "Net-(MOD1-Pad4)")
  (net 37 /EN)
  (net 38 "Net-(MOD1-Pad22)")
  (net 39 "Net-(MOD1-Pad21)")
  (net 40 "Net-(MOD1-Pad20)")
  (net 41 "Net-(MOD1-Pad19)")
  (net 42 "Net-(MOD1-Pad18)")
  (net 43 "Net-(MOD1-Pad17)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /BTN)
    (add_net /BootstrapGND)
    (add_net /CLK)
    (add_net /CMD)
    (add_net /Dat0)
    (add_net /Dat1)
    (add_net /Dat2)
    (add_net /Dat3)
    (add_net /EN)
    (add_net /LED)
    (add_net /Mic)
    (add_net /RX)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(M1-Pad1)")
    (add_net "Net-(M2-PadP$4)")
    (add_net "Net-(MOD1-Pad10)")
    (add_net "Net-(MOD1-Pad11)")
    (add_net "Net-(MOD1-Pad12)")
    (add_net "Net-(MOD1-Pad17)")
    (add_net "Net-(MOD1-Pad18)")
    (add_net "Net-(MOD1-Pad19)")
    (add_net "Net-(MOD1-Pad20)")
    (add_net "Net-(MOD1-Pad21)")
    (add_net "Net-(MOD1-Pad22)")
    (add_net "Net-(MOD1-Pad29)")
    (add_net "Net-(MOD1-Pad30)")
    (add_net "Net-(MOD1-Pad31)")
    (add_net "Net-(MOD1-Pad32)")
    (add_net "Net-(MOD1-Pad33)")
    (add_net "Net-(MOD1-Pad36)")
    (add_net "Net-(MOD1-Pad37)")
    (add_net "Net-(MOD1-Pad4)")
    (add_net "Net-(MOD1-Pad5)")
    (add_net "Net-(MOD1-Pad6)")
    (add_net "Net-(MOD1-Pad8)")
    (add_net "Net-(MOD1-Pad9)")
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 200000)
    (at 117.983 77.851 90)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference REC1 (at 0.127 -4.318 90) (layer F.SilkS))
    (fp_text value " " (at 0.762 4.445 90) (layer F.SilkS))
    (fp_text user 4 (at 4.191 2.159 90) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159 90) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159 90) (layer B.SilkS))
    (fp_text user 1 (at -3.683 -2.286 90) (layer B.SilkS))
    (pad 4 smd rect (at 3.302 2.286 90) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.302 2.286 90) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.302 -2.286 90) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 /BTN))
    (pad 1 smd rect (at -3.302 -2.286 90) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 /BTN))
  )
  (module digikey-footprints:ESP32-WROOM-32D (layer F.Cu) (tedit 5DF68CF0)
    (at 100.203 83.947 90)
    (attr smd)
    (fp_text reference MOD1 (at 0.02 -3.51 90) (layer F.SilkS))
    (fp_text value ESP32-WROOM-32 (at 0 11.88 90) (layer F.Fab))
    (fp_text user REF** (at 0.01 -5.37 90) (layer F.Fab))
    (pad 25 smd rect (at 8.5 8.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /BootstrapGND))
    (pad 26 smd rect (at 8.5 6.985 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 /Dat1))
    (pad 27 smd rect (at 8.5 5.715 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /LED))
    (pad 28 smd rect (at 8.5 4.445 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 /BTN))
    (pad 29 smd rect (at 8.5 3.175 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(MOD1-Pad29)"))
    (pad 30 smd rect (at 8.5 1.905 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(MOD1-Pad30)"))
    (pad 31 smd rect (at 8.5 0.635 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(MOD1-Pad31)"))
    (pad 32 smd rect (at 8.5 -0.635 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(MOD1-Pad32)"))
    (pad 33 smd rect (at 8.5 -1.905 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(MOD1-Pad33)"))
    (pad 34 smd rect (at 8.5 -3.175 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /RX))
    (pad 35 smd rect (at 8.5 -4.445 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /TX))
    (pad 36 smd rect (at 8.5 -5.715 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(MOD1-Pad36)"))
    (pad 37 smd rect (at 8.5 -6.985 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(MOD1-Pad37)"))
    (pad 38 smd rect (at 8.5 -8.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -8.5 8.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /Dat2))
    (pad 13 smd rect (at -8.5 6.985 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 /CLK))
    (pad 12 smd rect (at -8.5 5.715 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(MOD1-Pad12)"))
    (pad 11 smd rect (at -8.5 4.445 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(MOD1-Pad11)"))
    (pad 10 smd rect (at -8.5 3.175 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(MOD1-Pad10)"))
    (pad 9 smd rect (at -8.5 1.905 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(MOD1-Pad9)"))
    (pad 8 smd rect (at -8.5 0.635 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(MOD1-Pad8)"))
    (pad 7 smd rect (at -8.5 -0.635 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /Mic))
    (pad 6 smd rect (at -8.5 -1.905 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(MOD1-Pad6)"))
    (pad 5 smd rect (at -8.5 -3.175 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(MOD1-Pad5)"))
    (pad 4 smd rect (at -8.5 -4.445 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(MOD1-Pad4)"))
    (pad 3 smd rect (at -8.5 -5.715 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 /EN))
    (pad 2 smd rect (at -8.5 -6.985 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 24 smd rect (at 5.715 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /Dat0))
    (pad 23 smd rect (at 4.445 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /CMD))
    (pad 22 smd rect (at 3.175 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(MOD1-Pad22)"))
    (pad 21 smd rect (at 1.905 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(MOD1-Pad21)"))
    (pad 20 smd rect (at 0.635 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(MOD1-Pad20)"))
    (pad 19 smd rect (at -0.635 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(MOD1-Pad19)"))
    (pad 18 smd rect (at -1.905 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(MOD1-Pad18)"))
    (pad 17 smd rect (at -3.175 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(MOD1-Pad17)"))
    (pad 16 smd rect (at -4.445 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /Dat3))
    (pad 15 smd rect (at -5.715 9.255 180) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -8.5 -8.255 90) (size 2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-2X02SMD (layer F.Cu) (tedit 200000)
    (at 123.698 75.311 270)
    (attr smd)
    (fp_text reference M3 (at -0.635 -3.175 90) (layer F.SilkS))
    (fp_text value PINHD-2X2-SMD (at 7.493 3.175 90) (layer F.SilkS))
    (pad 4 smd rect (at 2.91846 1.27 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.54 1.27 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 25 /TX))
    (pad 2 smd rect (at 2.91846 -1.27 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -2.54 -1.27 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 24 /RX))
  )
  (module fab:fab-R1206FAB (layer B.Cu) (tedit 200000)
    (at 111.379 77.978 90)
    (attr smd)
    (fp_text reference R8 (at 0.762 1.778 270) (layer B.SilkS))
    (fp_text value 10k (at 1.27 -1.778 270) (layer B.SilkS))
    (pad 2 smd rect (at 1.651 0 90) (size 1.27 1.905) (layers B.Cu B.Paste B.Mask)
      (net 13 /Dat1))
    (pad 1 smd rect (at -1.651 0 90) (size 1.27 1.905) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 115.316 90.805 180)
    (attr smd)
    (fp_text reference R9 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 1k (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 5 /Mic))
    (pad 1 smd rect (at -1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(M2-PadP$4)"))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 100.457 94.996)
    (attr smd)
    (fp_text reference R6 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 10k (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 28 /CLK))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
  )
  (module fab:fab-R1206FAB (layer B.Cu) (tedit 200000)
    (at 109.22 83.947 270)
    (attr smd)
    (fp_text reference R5 (at 0.762 1.778 270) (layer B.SilkS))
    (fp_text value 10k (at 1.27 -1.778 270) (layer B.SilkS))
    (pad 2 smd rect (at 1.651 0 270) (size 1.27 1.905) (layers B.Cu B.Paste B.Mask)
      (net 10 /CMD))
    (pad 1 smd rect (at -1.651 0 270) (size 1.27 1.905) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
  )
  (module fab:fab-R1206FAB (layer B.Cu) (tedit 200000)
    (at 111.633 85.598 270)
    (attr smd)
    (fp_text reference R4 (at 0.762 1.778 270) (layer B.SilkS))
    (fp_text value 10k (at 1.27 -1.778 270) (layer B.SilkS))
    (pad 2 smd rect (at 1.651 0 270) (size 1.27 1.905) (layers B.Cu B.Paste B.Mask)
      (net 9 /Dat3))
    (pad 1 smd rect (at -1.651 0 270) (size 1.27 1.905) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 104.775 73.025 180)
    (attr smd)
    (fp_text reference R3 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 1k (at 1.397 0.254) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(M1-Pad1)"))
    (pad 1 smd rect (at -1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 17 /LED))
  )
  (module fab:fab-R1206FAB (layer F.Cu) (tedit 200000)
    (at 94.869 95.631 180)
    (attr smd)
    (fp_text reference R1 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 10k (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 37 /EN))
  )
  (module fab:fab-CSP-4PIN (layer F.Cu) (tedit 200000)
    (at 120.015 91.567)
    (descr "KNOWLES SPU0414HR5H-SB")
    (tags "KNOWLES SPU0414HR5H-SB")
    (attr smd)
    (fp_text reference M2 (at 0 0) (layer F.SilkS))
    (fp_text value MEMS_MIC_SPU0414HR5H-SB (at -9.017 0.254) (layer F.SilkS))
    (pad P$4 smd circle (at -0.84836 -1.22936) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(M2-PadP$4)"))
    (pad P$3 smd circle (at -0.84836 1.22936) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C5-Pad1)"))
    (pad P$2 smd circle (at 0.84836 1.22936) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad P$1 smd circle (at 0.85344 -1.21412) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 100.457 73.025 180)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference M1 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value LED (at 2.413 -1.143) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(M1-Pad1)"))
  )
  (module Connector_Card:microSD_HC_Hirose_DM3D-SF (layer B.Cu) (tedit 5DD70A23)
    (at 98.298 84.201 270)
    (descr "Micro SD, SMD, right-angle, push-pull (https://media.digikey.com/PDF/Data%20Sheets/Hirose%20PDFs/DM3D-SF.pdf)")
    (tags "Micro SD")
    (attr smd)
    (fp_text reference J1 (at -0.025 7.625 270) (layer B.SilkS))
    (fp_text value Micro_SD_Card_Det_Hirose_DM3AT (at -0.025 -6.975 270) (layer B.Fab))
    (fp_text user KEEPOUT (at -0.725 4.8 270) (layer Cmts.User))
    (fp_text user %R (at -0.025 -1.475 270) (layer B.Fab))
    (fp_text user KEEPOUT (at -0.275 0.525 270) (layer Cmts.User))
    (pad 10 smd rect (at 5.575 5.45 270) (size 1 1.55) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 11 smd rect (at 5.625 -5.225 270) (size 1.5 1.5) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad11)"))
    (pad 1 smd rect (at 3.175 -5.35 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 8 /Dat2))
    (pad 2 smd rect (at 2.075 -5.35 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 9 /Dat3))
    (pad 3 smd rect (at 0.975 -5.35 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 10 /CMD))
    (pad 4 smd rect (at -0.125 -5.35 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at -1.225 -5.35 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 28 /CLK))
    (pad 6 smd rect (at -2.325 -5.35 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -3.425 -5.35 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 11 /Dat0))
    (pad 11 smd rect (at 5.975 3.025 270) (size 0.8 1.4) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad11)"))
    (pad 9 smd rect (at -5.65 3.875 270) (size 1.45 1) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J1-Pad9)"))
    (pad 11 smd rect (at -5.975 2.375 270) (size 0.8 1.5) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad11)"))
    (pad 8 smd rect (at -4.525 -5.35 270) (size 0.7 1.75) (layers B.Cu B.Paste B.Mask)
      (net 13 /Dat1))
    (model ${KISYS3DMOD}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3D-SF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-223 (layer F.Cu) (tedit 5D28A60E)
    (at 121.793 84.836 90)
    (attr smd)
    (fp_text reference IC1 (at 0 -6.1 90) (layer F.SilkS))
    (fp_text value 3.3V (at 0.15 5.65 90) (layer F.Fab))
    (fp_text user %R (at -0.05 0.025 90) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.15 90) (size 3.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -2.3 3.15 90) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 3.15 90) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 2.3 3.15 90) (size 1.5 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 115.316 93.218)
    (attr smd)
    (fp_text reference C6 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 5 /Mic))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 121.92 95.25)
    (attr smd)
    (fp_text reference C5 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 10uF (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.651 0) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C5-Pad1)"))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 123.063 91.567 90)
    (attr smd)
    (fp_text reference C4 (at 0.762 -1.778 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.27 1.778 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 123.317 80.391 180)
    (attr smd)
    (fp_text reference C3 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 10uF (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 120.523 88.265 180)
    (attr smd)
    (fp_text reference C2 (at 0.762 -1.778) (layer F.SilkS))
    (fp_text value 1uF (at 1.27 1.778) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.651 0 180) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
  )
  (module fab:fab-C1206FAB (layer F.Cu) (tedit 200000)
    (at 115.951 86.487 90)
    (attr smd)
    (fp_text reference C1 (at 0.762 -1.778 90) (layer F.SilkS))
    (fp_text value 0.1uf (at 1.27 1.778 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -1.651 0 90) (size 1.27 1.905) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (dimension 27.178 (width 0.12) (layer F.SilkS)
    (gr_text "27.178 mm" (at 80.645 84.963 270) (layer F.SilkS))
    (feature1 (pts (xy 84.455 98.552) (xy 81.328579 98.552)))
    (feature2 (pts (xy 84.455 71.374) (xy 81.328579 71.374)))
    (crossbar (pts (xy 81.915 71.374) (xy 81.915 98.552)))
    (arrow1a (pts (xy 81.915 98.552) (xy 81.328579 97.425496)))
    (arrow1b (pts (xy 81.915 98.552) (xy 82.501421 97.425496)))
    (arrow2a (pts (xy 81.915 71.374) (xy 81.328579 72.500504)))
    (arrow2b (pts (xy 81.915 71.374) (xy 82.501421 72.500504)))
  )
  (dimension 42.672 (width 0.12) (layer F.SilkS)
    (gr_text "42.672 mm" (at 105.664 63.627) (layer F.SilkS))
    (feature1 (pts (xy 127 69.342) (xy 127 64.310579)))
    (feature2 (pts (xy 84.328 69.342) (xy 84.328 64.310579)))
    (crossbar (pts (xy 84.328 64.897) (xy 127 64.897)))
    (arrow1a (pts (xy 127 64.897) (xy 125.873496 65.483421)))
    (arrow1b (pts (xy 127 64.897) (xy 125.873496 64.310579)))
    (arrow2a (pts (xy 84.328 64.897) (xy 85.454504 65.483421)))
    (arrow2b (pts (xy 84.328 64.897) (xy 85.454504 64.310579)))
  )
)
