<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="9.271" y1="20.955" x2="38.842" y2="20.955" width="0" layer="20"/>
<wire x1="38.842" y1="20.955" x2="38.969" y2="55.296" width="0" layer="20"/>
<wire x1="38.969" y1="55.296" x2="9.398" y2="55.296" width="0" layer="20"/>
<wire x1="9.398" y1="55.296" x2="9.271" y2="20.955" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="2X02SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
<library name="ATTINY1614-SSNR">
<packages>
<package name="SOIC127P600X175-14N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PIXEL" library="fab" package="2X02SMD" value="CONN_02X2-PINHEAD-SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="fab" package="R1206FAB" value="4.99k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="ATTINY1614-SSNR" package="SOIC127P600X175-14N" value="ATTINY1614-SSNR">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" AVR tinyAVR™ 1 Microcontroller IC 8-Bit 20MHz 16KB (16K x 8) FLASH 14-SOIC "/>
<attribute name="MF" value="Microchip"/>
<attribute name="MP" value="ATTINY1614-SSNR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SO-14 Microchip"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/ATTINY1614-SSNR/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="UPDI" library="fab" package="2X02SMD" value="CONN_02X2-PINHEAD-SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="fab" package="2X03SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="LED" pad="1"/>
</signal>
<signal name="GND">
<contactref element="LED" pad="2"/>
<contactref element="UPDI" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="14"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="10"/>
<contactref element="UPDI" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="1"/>
<contactref element="UPDI" pad="4"/>
</signal>
<signal name="VDD">
<contactref element="UPDI" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="8"/>
<contactref element="PIXEL" pad="3"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="5"/>
<contactref element="PIXEL" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
