(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 79)
    (zones 0)
    (modules 5)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J2-Pad6)")
  (net 8 "Net-(J2-Pad5)")
  (net 9 "Net-(J2-Pad4)")
  (net 10 "Net-(J2-Pad2)")
  (net 11 "Net-(U1-Pad7)")
  (net 12 "Net-(U1-Pad5)")
  (net 13 "Net-(U1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net VCC)
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 139.192 69.088)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value C (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 161.036 54.356)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J1 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value "programming header" (at 2.286 15.621) (layer F.Fab))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad6)"))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 161.544 75.692)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J2 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value "programming header" (at 2.286 15.621) (layer F.Fab))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad6)"))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad5)"))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad4)"))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 151.384 67.024 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 4.99k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 608D94DE)
    (at 139.192 79.756)
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -3.5) (layer F.SilkS))
    (fp_text value Microcontroller_ATtiny412_SSFR (at 0 3.683) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 2.8 -1.905) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 2.8 -0.635) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at 2.8 0.635) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad5)"))
    (pad 5 smd rect (at 2.8 1.905) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at -2.8 1.905) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at -2.8 0.635) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad4)"))
    (pad 2 smd rect (at -2.8 -0.635) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad5)"))
    (pad 1 smd rect (at -2.8 -1.905) (size 2 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model ${FAB}/fab.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 153.924 49.784) (end 168.656 49.784) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 137.668 66.04) (end 153.924 49.784) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.112 66.04) (end 137.668 66.04) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.112 73.152) (end 134.112 66.04) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.128 73.152) (end 134.112 73.152) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.128 75.692) (end 135.128 73.152) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.064 75.692) (end 135.128 75.692) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 131.064 87.884) (end 131.064 75.692) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.48 87.884) (end 131.064 87.884) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.48 91.948) (end 157.48 87.884) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168.656 91.948) (end 157.48 91.948) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168.656 49.784) (end 168.656 91.948) (layer Edge.Cuts) (width 0.05))
)
