(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 170)
    (zones 0)
    (modules 13)
    (nets 42)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /VI_3V)
  (net 2 GND)
  (net 3 /MCU_IO15)
  (net 4 /MCU_IO14)
  (net 5 /MCU_IO27)
  (net 6 /MCU_IO25)
  (net 7 /MCU_IO33)
  (net 8 /MCU_IO32)
  (net 9 /MCU_IO21)
  (net 10 /MCU_IO19)
  (net 11 /MCU_IO18)
  (net 12 /MCU_IO5)
  (net 13 /MCU_IO17)
  (net 14 /MCU_IO16)
  (net 15 /MCU_IO4)
  (net 16 "Net-(J3-Pad6)")
  (net 17 /MCU_TX)
  (net 18 /MCU_RX)
  (net 19 /VI_5V)
  (net 20 "Net-(J3-Pad2)")
  (net 21 "Net-(SW2-Pad1)")
  (net 22 /MCU_IO0)
  (net 23 "Net-(U2-Pad32)")
  (net 24 "Net-(U2-Pad22)")
  (net 25 "Net-(U2-Pad21)")
  (net 26 "Net-(U2-Pad20)")
  (net 27 "Net-(U2-Pad19)")
  (net 28 "Net-(U2-Pad18)")
  (net 29 "Net-(U2-Pad17)")
  (net 30 "Net-(U2-Pad16)")
  (net 31 "Net-(U2-Pad11)")
  (net 32 "Net-(U2-Pad7)")
  (net 33 "Net-(U2-Pad6)")
  (net 34 "Net-(U2-Pad5)")
  (net 35 "Net-(U2-Pad4)")
  (net 36 /MCU_EN)
  (net 37 "Net-(U2-Pad14)")
  (net 38 "Net-(U2-Pad24)")
  (net 39 "Net-(U2-Pad37)")
  (net 40 "Net-(U2-Pad36)")
  (net 41 "Net-(D1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /MCU_EN)
    (add_net /MCU_IO0)
    (add_net /MCU_IO14)
    (add_net /MCU_IO15)
    (add_net /MCU_IO16)
    (add_net /MCU_IO17)
    (add_net /MCU_IO18)
    (add_net /MCU_IO19)
    (add_net /MCU_IO21)
    (add_net /MCU_IO25)
    (add_net /MCU_IO27)
    (add_net /MCU_IO32)
    (add_net /MCU_IO33)
    (add_net /MCU_IO4)
    (add_net /MCU_IO5)
    (add_net /MCU_RX)
    (add_net /MCU_TX)
    (add_net /VI_3V)
    (add_net /VI_5V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(SW2-Pad1)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad32)")
    (add_net "Net-(U2-Pad36)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
  )
  (module fab:ESP32-WROOM-32E-EDITED (layer F.Cu) (tedit 619BF0D2)
    (at 48.26 82.296 90)
    (descr "Single 2.4 GHz Wi-Fi and Bluetooth combo chip https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32_datasheet_en.pdf")
    (tags "Single 2.4 GHz Wi-Fi and Bluetooth combo  chip")
    (attr smd)
    (fp_text reference U2 (at -10.61 8.43) (layer F.SilkS))
    (fp_text value ESP32-WROOM-32 (at 0 11.5 90) (layer F.Fab))
    (fp_text user "5 mm" (at 7.8 -19.075) (layer Cmts.User))
    (fp_text user "5 mm" (at -11.2 -14.375 90) (layer Cmts.User))
    (fp_text user "5 mm" (at 11.8 -14.375 90) (layer Cmts.User))
    (fp_text user Antenna (at 0 -13 90) (layer Cmts.User))
    (fp_text user "KEEP-OUT ZONE" (at 0 -19 90) (layer Cmts.User))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 38 smd rect (at 8.5 -8.255 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 37 smd rect (at 8.5 -6.985 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U2-Pad37)"))
    (pad 36 smd rect (at 8.5 -5.715 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U2-Pad36)"))
    (pad 35 smd rect (at 8.5 -4.445 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /MCU_TX))
    (pad 34 smd rect (at 8.5 -3.175 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /MCU_RX))
    (pad 33 smd rect (at 8.5 -1.905 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /MCU_IO21))
    (pad 32 smd rect (at 8.5 -0.635 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad32)"))
    (pad 31 smd rect (at 8.5 0.635 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /MCU_IO19))
    (pad 30 smd rect (at 8.5 1.905 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /MCU_IO18))
    (pad 29 smd rect (at 8.5 3.175 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /MCU_IO5))
    (pad 28 smd rect (at 8.5 4.445 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /MCU_IO17))
    (pad 27 smd rect (at 8.5 5.715 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /MCU_IO16))
    (pad 26 smd rect (at 8.5 6.985 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /MCU_IO4))
    (pad 25 smd rect (at 8.5 8.255 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /MCU_IO0))
    (pad 24 smd rect (at 5.715 9.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U2-Pad24)"))
    (pad 23 smd rect (at 4.445 9.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /MCU_IO15))
    (pad 22 smd rect (at 3.175 9.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad22)"))
    (pad 21 smd rect (at 1.905 9.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad21)"))
    (pad 20 smd rect (at 0.635 9.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U2-Pad20)"))
    (pad 19 smd rect (at -0.635 9.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U2-Pad19)"))
    (pad 18 smd rect (at -1.905 9.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U2-Pad18)"))
    (pad 17 smd rect (at -3.175 9.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U2-Pad17)"))
    (pad 16 smd rect (at -4.445 9.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U2-Pad16)"))
    (pad 15 smd rect (at -5.715 9.255 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -8.5 8.255 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U2-Pad14)"))
    (pad 13 smd rect (at -8.5 6.985 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /MCU_IO14))
    (pad 12 smd rect (at -8.5 5.715 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /MCU_IO27))
    (pad 11 smd rect (at -8.5 4.445 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U2-Pad11)"))
    (pad 10 smd rect (at -8.5 3.175 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /MCU_IO25))
    (pad 9 smd rect (at -8.5 1.905 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /MCU_IO33))
    (pad 8 smd rect (at -8.5 0.635 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /MCU_IO32))
    (pad 7 smd rect (at -8.5 -0.635 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U2-Pad7)"))
    (pad 6 smd rect (at -8.5 -1.905 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at -8.5 -3.175 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-Pad5)"))
    (pad 4 smd rect (at -8.5 -4.445 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -8.5 -5.715 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /MCU_EN))
    (pad 2 smd rect (at -8.5 -6.985 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /VI_3V))
    (pad 1 smd rect (at -8.5 -8.255 90) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 39 smd rect (at -1 -0.755 90) (size 5 5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/ESP32-WROOM-32.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 64.262 76.422 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 1kΩ (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:LED_1206 (layer F.Cu) (tedit 595FC724)
    (at 61.214 76.422 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /MCU_IO15))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 42.386 99.004 90)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at -0.056 -6.382 90) (layer F.Fab))
    (fp_text user %R (at 0 -4.5 90) (layer F.Fab))
    (pad 1 smd rect (at -3.5 -2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.5 -2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.5 2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 36 /MCU_EN))
    (pad 2 smd rect (at 3.5 2 90) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 36 /MCU_EN))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x07_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851979)
    (at 45.466 67.31 90)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J2 (at -1.524 -2.54 270) (layer F.SilkS))
    (fp_text value Conn_01x07_Female (at 0 18.415 90) (layer F.Fab))
    (fp_text user %R (at 2.6 7.62) (layer F.Fab))
    (pad 7 smd rect (at 0 15.24 90) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /MCU_IO4))
    (pad 6 smd rect (at 0 12.7 90) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /MCU_IO16))
    (pad 5 smd rect (at 0 10.16 90) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /MCU_IO17))
    (pad 4 smd rect (at 0 7.62 90) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /MCU_IO5))
    (pad 3 smd rect (at 0 5.08 90) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /MCU_IO18))
    (pad 2 smd rect (at 0 2.54 90) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /MCU_IO19))
    (pad 1 smd rect (at 0 0 90) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /MCU_IO21))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x07_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x08_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 608519DA)
    (at 68.326 102.616 270)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J1 (at -1.524 -2.54 270) (layer F.SilkS))
    (fp_text value Conn_01x08_Female (at 7.62 9.398 180) (layer F.Fab))
    (fp_text user %R (at 2.54 8.89) (layer F.Fab))
    (pad 8 smd rect (at 0 17.78 270) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /MCU_IO32))
    (pad 7 smd rect (at 0 15.24 270) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /MCU_IO33))
    (pad 6 smd rect (at 0 12.7 270) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /MCU_IO25))
    (pad 5 smd rect (at 0 10.16 270) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /MCU_IO27))
    (pad 4 smd rect (at 0 7.62 270) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /MCU_IO14))
    (pad 3 smd rect (at 0 5.08 270) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 2.54 270) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /VI_3V))
    (pad 1 smd rect (at 0 0 270) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /VI_5V))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x08_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 42.418 106.68 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value "0.1 uF" (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /VI_3V))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 66.072 98.298)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /VI_5V))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:Switch_SPDT_C&K_AYZ0102AGRLC_7.2x3mm_P2.5mm (layer F.Cu) (tedit 5EC6693D)
    (at 66.588 67.862 180)
    (descr http://www.ckswitches.com/media/1422/js.pdf)
    (tags "switch spdt")
    (attr smd)
    (fp_text reference SW2 (at -0.01 -5.15) (layer F.SilkS))
    (fp_text value SWITCH_AYZ0102AGRLC (at -4.826 2.794) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 1.5 0 180) (size 0.9 0.9) (drill 0.85) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.5 0 180) (size 0.9 0.9) (drill 0.85) (layers *.Cu *.Mask))
    (pad 3 smd rect (at 2.5 -2.75 180) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 22 /MCU_IO0))
    (pad 2 smd rect (at 0 -2.75 180) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.5 -2.75 180) (size 1.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(SW2-Pad1)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPDT_CK-JS102011SAQN.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:SOT-223-3_TabPin2 (layer F.Cu) (tedit 58CE4E7E)
    (at 65.786 91.288 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value Regulator_Linear_ZLDO1117-3.3V-1A (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 1 /VI_3V))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /VI_3V))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 /VI_5V))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 47.498 100.552 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 10kΩ (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /VI_3V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 36 /MCU_EN))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 73.914 80.772)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J3 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 8.128 8.636 90) (layer F.Fab))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-Pad6)"))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /MCU_TX))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /MCU_RX))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /VI_5V))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J3-Pad2)"))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 66.008 83.566)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /VI_3V))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 38.608 108.966) (end 38.608 68.072) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.264 108.966) (end 38.608 108.966) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.264 95.25) (end 80.264 108.966) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.264 60.96) (end 80.264 95.25) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 78.74 60.96) (end 80.264 60.96) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 62.484 60.96) (end 78.74 60.96) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 38.608 60.96) (end 62.484 60.96) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 38.608 68.072) (end 38.608 60.96) (layer Edge.Cuts) (width 0.1))
)
