(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 86)
    (zones 0)
    (modules 10)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J2-Pad2)")
  (net 7 "Net-(J2-Pad3)")
  (net 8 "Net-(R1-Pad2)")
  (net 9 "Net-(R2-Pad1)")
  (net 10 "Net-(U1-Pad1)")
  (net 11 "Net-(U1-Pad2)")
  (net 12 "Net-(U1-Pad3)")
  (net 13 "Net-(U1-Pad4)")
  (net 14 "Net-(U1-Pad5)")
  (net 15 +3V3)
  (net 16 GND)
  (net 17 +5V)
  (net 18 "Net-(R_zero1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R_zero1-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
  )
  (module fab:SOT-23 (layer F.Cu) (tedit 60A7B52C)
    (at 137.725 110.705)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value Regulator_Linear_LM3480-3.3V-100mA (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1.2 0) (size 1.8 1) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 2 smd rect (at -1.2 0.85) (size 1.8 1) (layers F.Cu F.Paste F.Mask)
      (net 17 +5V))
    (pad 1 smd rect (at -1.2 -0.85) (size 1.8 1) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_2x02_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 608517CB)
    (at 121.27 81.28 180)
    (descr "surface-mounted straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x02 2.54mm double row")
    (attr smd)
    (fp_text reference J2 (at 0 -3.6) (layer F.SilkS))
    (fp_text value Conn_PinHeader_2x02_P2.54mm_Vertical_SMD (at 0 3.6) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -1.27 180) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 2.525 -1.27 180) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at -2.525 1.27 180) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at 2.525 1.27 180) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 60030324)
    (at 120.65 92.645 180)
    (descr "SOIC, 14 Pin, fab version")
    (tags "SOIC fab")
    (attr smd)
    (fp_text reference U1 (at 0 -5.28) (layer F.SilkS))
    (fp_text value Microcontroller_ATSAMD11C14A-SSUT (at 0 0) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.CrtYd))
    (pad 1 smd rect (at -2.475 -3.81 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -2.475 -2.54 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -2.475 -1.27 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -2.475 0 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -2.475 1.27 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -2.475 2.54 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (pad 7 smd rect (at -2.475 3.81 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 8 smd rect (at 2.475 3.81 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 9 smd rect (at 2.475 2.54 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R_zero1-Pad1)"))
    (pad 10 smd rect (at 2.475 1.27 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 11 smd rect (at 2.475 0 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 12 smd rect (at 2.475 -1.27 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 13 smd rect (at 2.475 -2.54 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (pad 14 smd rect (at 2.475 -3.81 180) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R2-Pad1)"))
    (model ${FAB}/fab.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB3_A_Molex_48393-001 (layer F.Cu) (tedit 5A142044)
    (at 113.665 53.34)
    (descr "USB 3.0, type A, right angle (http://www.molex.com/pdm_docs/sd/483930003_sd.pdf)")
    (tags "USB 3.0 type A right angle")
    (fp_text reference J1 (at 3.5 -3.6) (layer F.SilkS))
    (fp_text value USB_A (at 3.5 13) (layer F.Fab))
    (fp_text user %R (at 3.5 5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 +5V))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 4.5 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 7 0) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 GND))
    (pad 5 thru_hole circle (at 7.5 -1.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at 5.5 -1.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 3.5 -1.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 1.5 -1.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at -0.5 -1.5) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 9.9 -0.75) (size 1.2 2.4) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at -2.9 -0.75) (size 1.2 2.4) (drill oval 0.6 1.7) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 9.9 7.75) (size 1.2 2.1) (drill oval 0.6 1.4) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at -2.9 7.75) (size 1.2 2.1) (drill oval 0.6 1.4) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB3_A_Molex_48393-001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 129.23 111.22)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 -4.5) (layer F.Fab))
    (pad 2 smd rect (at 3.5 2) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 2 smd rect (at -3.5 2) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 1 smd rect (at 3.5 -2) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -3.5 -2) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 125.73 100.425 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:LED_1206 (layer F.Cu) (tedit 595FC724)
    (at 123.095 116.84 180)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value LED (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 120.015 104.045 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad2)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 119.38 110.49)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R2-Pad1)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 116.205 73.66 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_zero1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R_zero1-Pad1)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
)
