(kicad_pcb (version 20171130) (host pcbnew "(5.1.10-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 2)
    (tracks 405)
    (zones 0)
    (modules 17)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 "Net-(C_1uF1-Pad2)")
  (net 5 /A02)
  (net 6 /A03)
  (net 7 /A04)
  (net 8 /A05)
  (net 9 /A06)
  (net 10 /A07)
  (net 11 "Net-(J1-Pad2)")
  (net 12 "Net-(J1-Pad3)")
  (net 13 /SWDIO)
  (net 14 /SWDCLK)
  (net 15 "Net-(J2-Pad6)")
  (net 16 "Net-(J2-Pad8)")
  (net 17 /RESET)
  (net 18 /D10)
  (net 19 /D11)
  (net 20 /D16)
  (net 21 /D17)
  (net 22 /D18)
  (net 23 /D19)
  (net 24 "Net-(U1-Pad1)")
  (net 25 "Net-(U1-Pad2)")
  (net 26 "Net-(U1-Pad15)")
  (net 27 "Net-(U1-Pad16)")
  (net 28 "Net-(R_zero1-Pad2)")
  (net 29 "Net-(D1-Pad2)")
  (net 30 "Net-(J2-Pad7)")
  (net 31 /D08)
  (net 32 /D09)
  (net 33 "Net-(R1-Pad1)")
  (net 34 /D27)
  (net 35 /D23)
  (net 36 /D22)
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /A02)
    (add_net /A03)
    (add_net /A04)
    (add_net /A05)
    (add_net /A06)
    (add_net /A07)
    (add_net /D08)
    (add_net /D09)
    (add_net /D10)
    (add_net /D11)
    (add_net /D16)
    (add_net /D17)
    (add_net /D18)
    (add_net /D19)
    (add_net /D22)
    (add_net /D23)
    (add_net /D27)
    (add_net /RESET)
    (add_net /SWDCLK)
    (add_net /SWDIO)
    (add_net GND)
    (add_net "Net-(C_1uF1-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R_zero1-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad2)")
  )
  (module fab:TQFP-32_7x7mm_P0.8mm (layer F.Cu) (tedit 618A6EA1)
    (at 81.407 86.5505 180)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 -6.05 180) (layer F.SilkS))
    (fp_text value Microcontroller_ATSAMD21E17A-AUT (at 0 6.05 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 32 smd rect (at -2.8 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 /SWDIO))
    (pad 31 smd rect (at -2 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 /SWDCLK))
    (pad 30 smd rect (at -1.2 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 29 smd rect (at -0.4 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C_1uF1-Pad2)"))
    (pad 28 smd rect (at 0.4 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 27 smd rect (at 1.2 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R1-Pad1)"))
    (pad 26 smd rect (at 2 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 /RESET))
    (pad 25 smd rect (at 2.8 -4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 /D27))
    (pad 24 smd rect (at 4.25 -2.8 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad3)"))
    (pad 23 smd rect (at 4.25 -2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R_zero1-Pad2)"))
    (pad 22 smd rect (at 4.25 -1.2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 35 /D23))
    (pad 21 smd rect (at 4.25 -0.4 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 36 /D22))
    (pad 20 smd rect (at 4.25 0.4 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 /D19))
    (pad 19 smd rect (at 4.25 1.2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 /D18))
    (pad 18 smd rect (at 4.25 2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 /D17))
    (pad 17 smd rect (at 4.25 2.8 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 /D16))
    (pad 16 smd rect (at 2.8 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad16)"))
    (pad 15 smd rect (at 2 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad15)"))
    (pad 14 smd rect (at 1.2 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 /D11))
    (pad 13 smd rect (at 0.4 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 /D10))
    (pad 12 smd rect (at -0.4 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 32 /D09))
    (pad 11 smd rect (at -1.2 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 /D08))
    (pad 10 smd rect (at -2 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -2.8 4.25 270) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 8 smd rect (at -4.25 2.8 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /A07))
    (pad 7 smd rect (at -4.25 2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /A06))
    (pad 6 smd rect (at -4.25 1.2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /A05))
    (pad 5 smd rect (at -4.25 0.4 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /A04))
    (pad 4 smd rect (at -4.25 -0.4 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /A03))
    (pad 3 smd rect (at -4.25 -1.2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /A02))
    (pad 2 smd rect (at -4.25 -2 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at -4.25 -2.8 180) (size 1.6 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad1)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module usb_plug:USB_PLUG_TRACES (layer F.Cu) (tedit 6161FC20)
    (at 60.0964 73.6024 90)
    (fp_text reference J1 (at 0.1 5.08 90) (layer F.SilkS))
    (fp_text value USB_A (at 0.05 -6.35 90) (layer F.Fab))
    (pad 1 smd rect (at -3.6 0 90) (size 1.6 8) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 4 smd rect (at 3.6 0 90) (size 1.6 8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1 0.5 90) (size 1 7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 1 0.5 90) (size 1 7) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad3)"))
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 85.1408 116.3132 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_10uF1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 89.7636 117.7732 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_10uF2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 82.1944 101.6696 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_1uF1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C_1uF1-Pad2)"))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 91.0717 110.077 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_1uF2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:LED_1206 (layer F.Cu) (tedit 595FC724)
    (at 75.978 98.1964 180)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value LED (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module fab:PinHeader_2x05_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 60851B62)
    (at 75.9333 108.0712 270)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J2 (at 0 -4.235 90) (layer F.SilkS))
    (fp_text value Conn_PinHeader_2x05_P1.27mm_Vertical_SMD (at 0 4.235 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -2.54 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.95 -2.54 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 13 /SWDIO))
    (pad 3 smd rect (at -1.95 -1.27 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.95 -1.27 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 14 /SWDCLK))
    (pad 5 smd rect (at -1.95 0 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.95 0 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad6)"))
    (pad 7 smd rect (at -1.95 1.27 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J2-Pad7)"))
    (pad 8 smd rect (at 1.95 1.27 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad8)"))
    (pad 9 smd rect (at -1.95 2.54 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 1.95 2.54 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 17 /RESET))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 102.3239 73.6219)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J3 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 /D19))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 /D18))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /D17))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /D16))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /D11))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /D10))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 102.3239 90.0049)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J4 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /A06))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /A07))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 /D08))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 /D09))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 102.3239 106.3879)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J5 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /A05))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /A04))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /A03))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /A02))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 75.8256 101.4476)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R1-Pad1)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 89.0844 99.4156 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10K1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /SWDCLK))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 83.9028 110.3884)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10K2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /RESET))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 72.676 73.7616)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference R_zero1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R_zero1-Pad2)"))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 77.1196 116.6556)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 -4.5) (layer F.Fab))
    (pad 2 smd rect (at 3.5 2) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -3.5 2) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 3.5 -2) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /RESET))
    (pad 1 smd rect (at -3.5 -2) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /RESET))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:SOT-23 (layer F.Cu) (tedit 60A7B52C)
    (at 90.1 103.8724)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value Regulator_Linear_LM3480-3.3V-100mA (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1.2 0) (size 1.8 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.2 0.85) (size 1.8 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.2 -0.85) (size 1.8 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text o (at 87.4268 92.71) (layer F.Cu))
  (gr_text "LING\nDONG" (at 93.0148 118.0084) (layer F.Cu))
)
