(kicad_pcb (version 20171130) (host pcbnew "(5.1.12-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 98)
    (zones 0)
    (modules 12)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 1)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /A07)
  (net 2 "Net-(D1-Pad1)")
  (net 3 GND)
  (net 4 /D11)
  (net 5 +3V3)
  (net 6 /D10)
  (net 7 /D19)
  (net 8 /D18)
  (net 9 /D17)
  (net 10 /D16)
  (net 11 /A06)
  (net 12 /D08)
  (net 13 /D09)
  (net 14 "Net-(D2-Pad1)")
  (net 15 +5V)
  (net 16 /A05)
  (net 17 /A04)
  (net 18 /A03)
  (net 19 /A02)
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /A02)
    (add_net /A03)
    (add_net /A04)
    (add_net /A05)
    (add_net /A06)
    (add_net /A07)
    (add_net /D08)
    (add_net /D09)
    (add_net /D10)
    (add_net /D11)
    (add_net /D16)
    (add_net /D17)
    (add_net /D18)
    (add_net /D19)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 149.39772 49.63668)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J3 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /D19))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /D18))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /D17))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /D16))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /D11))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /D10))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 149.39772 66.08572)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J4 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /A06))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /A07))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /D08))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /D09))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:LED_1206 (layer F.Cu) (tedit 595FC724)
    (at 159.00044 67.6148 180)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /A06))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 159.06508 81.50708 180)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 -4.5) (layer F.Fab))
    (pad 2 smd rect (at 3.5 2 180) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -3.5 2 180) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 3.5 -2 180) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 /A05))
    (pad 1 smd rect (at -3.5 -2 180) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 /A05))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 159.1376 75.057)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /A05))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:LED_1206 (layer F.Cu) (tedit 595FC724)
    (at 158.9344 63.12916 180)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /A07))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module fab:PinHeader_2x02_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 608517CB)
    (at 158.78532 52.6542)
    (descr "surface-mounted straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x02 2.54mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 -3.6) (layer F.SilkS))
    (fp_text value Conn_PinHeader_2x02_P2.54mm_Vertical_SMD (at 0 3.6) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 2.525 -1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /D11))
    (pad 3 smd rect (at -2.525 1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (pad 4 smd rect (at 2.525 1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /D10))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 158.9344 59.54268 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 149.39264 82.45348)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J2 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /A05))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /A04))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /A03))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /A02))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 158.94456 87.249)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /A04))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 +3V3))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 159.09188 70.87616 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D2-Pad1)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 159.17176 92.92692)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW2 (at 0 -4.5) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 -4.5) (layer F.Fab))
    (pad 2 smd rect (at 3.5 2) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at -3.5 2) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at 3.5 -2) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /A04))
    (pad 1 smd rect (at -3.5 -2) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /A04))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
)
