(kicad_pcb (version 20171130) (host pcbnew "(5.1.12-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 124)
    (zones 0)
    (modules 14)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 1.4)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 GND)
  (net 3 /D09)
  (net 4 /D08)
  (net 5 "Net-(J3-Pad1)")
  (net 6 /D17)
  (net 7 "Net-(J3-Pad3)")
  (net 8 /D16)
  (net 9 /D10)
  (net 10 /D11)
  (net 11 /D18)
  (net 12 /D19)
  (net 13 +3V3)
  (net 14 /A07)
  (net 15 /A06)
  (net 16 "Net-(R_10K1-Pad1)")
  (net 17 "Net-(D2-Pad2)")
  (net 18 "Net-(D3-Pad2)")
  (net 19 "Net-(R_499o2-Pad1)")
  (net 20 "Net-(R_499o3-Pad1)")
  (net 21 "Net-(U1-Pad6)")
  (net 22 "Net-(U1-Pad9)")
  (net 23 "Net-(U1-Pad11)")
  (net 24 "Net-(U1-Pad5)")
  (net 25 "Net-(U1-Pad4)")
  (net 26 "Net-(U1-Pad3)")
  (net 27 "Net-(U1-Pad1)")
  (net 28 "Net-(U1-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /A06)
    (add_net /A07)
    (add_net /D08)
    (add_net /D09)
    (add_net /D10)
    (add_net /D11)
    (add_net /D16)
    (add_net /D17)
    (add_net /D18)
    (add_net /D19)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(R_10K1-Pad1)")
    (add_net "Net-(R_499o2-Pad1)")
    (add_net "Net-(R_499o3-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad9)")
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 619AD19C)
    (at 164.77488 48.00092)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J4 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /D19))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /D18))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /D17))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.4) (drill (offset 0 -0.15)) (layers F.Cu F.Paste F.Mask)
      (net 8 /D16))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.3) (drill (offset 0 0.2)) (layers F.Cu F.Paste F.Mask)
      (net 10 /D11))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /D10))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 164.77488 64.43472)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J5 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 /D09))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /D08))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /A07))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /A06))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 170.47972 57.93384 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:LED_1206 (layer F.Cu) (tedit 595FC724)
    (at 169.545 67.36436 270)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module fab:LED_1206 (layer F.Cu) (tedit 595FC724)
    (at 175.96968 68.87972)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value LED (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module fab:LED_1206 (layer F.Cu) (tedit 595FC724)
    (at 183.6354 69.00164 180)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D3 (at 0 -1.85) (layer F.SilkS))
    (fp_text value LED (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module fab:PinHeader_2x02_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 608517CB)
    (at 177.73904 49.01692)
    (descr "surface-mounted straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x02 2.54mm double row")
    (attr smd)
    (fp_text reference J3 (at 0 -3.6) (layer F.SilkS))
    (fp_text value Conn_PinHeader_2x02_P2.54mm_Vertical_SMD (at 0 3.6) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 2.525 -1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /D17))
    (pad 3 smd rect (at -2.525 1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (pad 4 smd rect (at 2.525 1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /D16))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 173.9138 57.93384 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10K1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R_10K1-Pad1)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 171.82592 76.29144)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10K2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /A06))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 171.76648 73.1012)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_499o1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /A07))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 176.01844 65.97396)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_499o2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R_499o2-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D2-Pad2)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 183.59272 65.94348 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_499o3 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R_499o3-Pad1)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 181.37644 74.24268 180)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 -4.5) (layer F.Fab))
    (pad 2 smd rect (at 3.5 2 180) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.5 2 180) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.5 -2 180) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 15 /A06))
    (pad 1 smd rect (at -3.5 -2 180) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 15 /A06))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:Microchip_RN4871 (layer F.Cu) (tedit 5A0FEF3D)
    (at 181.95984 57.8038 270)
    (descr "Microchip RN4871 footprint")
    (tags "RN4871 BLE")
    (attr smd)
    (fp_text reference U1 (at 0 -9.3 90) (layer F.SilkS))
    (fp_text value Radio_Microchip_RN4871 (at 0 4.8 90) (layer F.Fab))
    (fp_text user "On any layer" (at 0 -5.7 90) (layer Cmts.User))
    (fp_text user "No Metal, No Traces, Components" (at 0 -6.2 90) (layer Cmts.User))
    (fp_text user "KEEP-OUT ZONE" (at 1.825 -0.825) (layer Cmts.User))
    (fp_text user "KEEP-OUT ZONE" (at -2.575 -2.5) (layer Cmts.User))
    (fp_text user "KEEP-OUT ZONE" (at 0 -7.3 90) (layer Cmts.User))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 6 smd rect (at -3 3.05 270) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -1.8 3.05 270) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /D10))
    (pad 8 smd rect (at -0.6 3.05 270) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /D11))
    (pad 9 smd rect (at 0.6 3.05 270) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 1.8 3.05 270) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R_10K1-Pad1)"))
    (pad 11 smd rect (at 3 3.05 270) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad11)"))
    (pad 5 smd rect (at -4.35 1.35) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at -4.35 0.15) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at -4.35 -1.05) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at -4.35 -2.25) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -4.35 -3.45) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad1)"))
    (pad 12 smd rect (at 4.35 1.35) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R_499o2-Pad1)"))
    (pad 13 smd rect (at 4.35 0.15) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 4.35 -1.05) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 15 smd rect (at 4.35 -2.3) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R_499o3-Pad1)"))
    (pad 16 smd rect (at 4.35 -3.45) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad16)"))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/Microchip_RN4871.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
)
