(kicad_pcb (version 20171130) (host pcbnew "(5.1.12-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 295)
    (zones 0)
    (modules 19)
    (nets 22)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.5)
    (zone_clearance 0.6)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /D16)
  (net 2 +5V)
  (net 3 GND)
  (net 4 /D11)
  (net 5 /D17)
  (net 6 /O15)
  (net 7 /O14)
  (net 8 /D10)
  (net 9 /A06)
  (net 10 /A07)
  (net 11 +3V3)
  (net 12 /D08)
  (net 13 /D09)
  (net 14 /A05)
  (net 15 /A04)
  (net 16 /A03)
  (net 17 /A02)
  (net 18 /D18)
  (net 19 /D19)
  (net 20 /D22)
  (net 21 /D23)
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /A02)
    (add_net /A03)
    (add_net /A04)
    (add_net /A05)
    (add_net /A06)
    (add_net /A07)
    (add_net /D08)
    (add_net /D09)
    (add_net /D10)
    (add_net /D11)
    (add_net /D16)
    (add_net /D17)
    (add_net /D18)
    (add_net /D19)
    (add_net /D22)
    (add_net /D23)
    (add_net /O14)
    (add_net /O15)
    (add_net GND)
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD8A16)
    (at 119.38 69.174)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J3 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.5) (drill (offset 0 0.1)) (layers F.Cu F.Paste F.Mask)
      (net 5 /D17))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 /D16))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.3) (drill (offset 0 -0.2)) (layers F.Cu F.Paste F.Mask)
      (net 6 /O15))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.3) (drill (offset 0 0.2)) (layers F.Cu F.Paste F.Mask)
      (net 7 /O14))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /D11))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.5) (drill (offset 0 -0.1)) (layers F.Cu F.Paste F.Mask)
      (net 8 /D10))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD8833)
    (at 119.38 52.654)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J14 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /D23))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /D22))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 /D19))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.5) (drill (offset 0 -0.1)) (layers F.Cu F.Paste F.Mask)
      (net 18 /D18))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x03_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD85A3)
    (at 134.112 110.236)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J9 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD (at 2.6 8.3) (layer F.Fab))
    (fp_text user %R (at 2.4 2.6 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 16 /A03))
    (pad 2 smd rect (at 0 2.54) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 3 smd rect (at 0 5.08) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x03_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD8146)
    (at 142.24 65.786)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J16 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD (at 2.6 8.3) (layer F.Fab))
    (fp_text user %R (at 2.4 2.6 90) (layer F.Fab))
    (pad 3 smd rect (at 0 5.08) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 2.54) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at 0 0) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 20 /D22))
    (model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x03_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD811D)
    (at 134.112 65.786)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J13 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD (at 2.6 8.3) (layer F.Fab))
    (fp_text user %R (at 2.4 2.6 90) (layer F.Fab))
    (pad 3 smd rect (at 0 5.08) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 2.54) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at 0 0) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /D17))
    (model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x03_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD80F8)
    (at 134.366 55.626)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J17 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD (at 2.6 8.3) (layer F.Fab))
    (fp_text user %R (at 2.4 2.6 90) (layer F.Fab))
    (pad 3 smd rect (at 0 5.08) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 2.54) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at 0 0) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 19 /D19))
    (model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x03_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD80DF)
    (at 128.016 65.786)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J1 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD (at 2.6 8.3) (layer F.Fab))
    (fp_text user %R (at 2.4 2.6 90) (layer F.Fab))
    (pad 3 smd rect (at 0 5.08) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 2.54) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at 0 0) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /D16))
    (model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x03_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD80EA)
    (at 134.112 75.946)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J2 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD (at 2.6 8.3) (layer F.Fab))
    (fp_text user %R (at 2.4 2.6 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /D11))
    (pad 2 smd rect (at 0 2.54) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at 0 5.08) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD89B5)
    (at 119.38 85.714)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J4 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /A06))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /A07))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /D08))
    (pad 1 smd rect (at 0 0) (size 2.5 1.5) (drill (offset 0 0.1)) (layers F.Cu F.Paste F.Mask)
      (net 13 /D09))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 119.38 102.254)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J5 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /A05))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /A04))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /A03))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /A02))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x03_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD8130)
    (at 128.016 75.946)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J6 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD (at 2.6 8.3) (layer F.Fab))
    (fp_text user %R (at 2.4 2.6 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /D10))
    (pad 2 smd rect (at 0 2.54) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at 0 5.08) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x03_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD813B)
    (at 134.112 101.092)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J7 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD (at 2.6 8.3) (layer F.Fab))
    (fp_text user %R (at 2.4 2.6 90) (layer F.Fab))
    (pad 3 smd rect (at 0 5.08) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 2.54) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 1 smd rect (at 0 0) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /A05))
    (model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x03_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD811A)
    (at 128.016 101.092)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J8 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD (at 2.6 8.3) (layer F.Fab))
    (fp_text user %R (at 2.4 2.6 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 15 /A04))
    (pad 2 smd rect (at 0 2.54) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 3 smd rect (at 0 5.08) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x03_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD80D0)
    (at 128.016 110.236)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J10 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD (at 2.6 8.3) (layer F.Fab))
    (fp_text user %R (at 2.4 2.6 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /A02))
    (pad 2 smd rect (at 0 2.54) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 3 smd rect (at 0 5.08) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_2x02_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 61AD8AF7)
    (at 135.905 91.694)
    (descr "surface-mounted straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x02 2.54mm double row")
    (attr smd)
    (fp_text reference J11 (at 0 -3.6) (layer F.SilkS))
    (fp_text value Conn_PinHeader_2x02_P2.54mm_Vertical_SMD (at 0 3.6) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -1.27) (size 3 1) (drill (offset -0.15 0)) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 2.525 -1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /O15))
    (pad 3 smd rect (at -2.525 1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 4 smd rect (at 2.525 1.27) (size 3 1) (drill (offset 0.15 0)) (layers F.Cu F.Paste F.Mask)
      (net 7 /O14))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 127.508 85.344)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J12 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /A06))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /A07))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /D08))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /D09))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_FTDI_01x06_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 60851AE4)
    (at 145.034 86.36)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J15 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_FTDI_1x06_P2.54mm_Horizontal_SMD (at 2.286 15.621) (layer F.Fab))
    (fp_text user %R (at 2.6 6.1 90) (layer F.Fab))
    (fp_text user GND (at -1.905 0) (layer F.SilkS))
    (fp_text user CTS (at -1.905 2.54) (layer F.SilkS))
    (fp_text user VCC (at -1.905 5.08) (layer F.SilkS))
    (fp_text user TX (at -1.905 7.62) (layer F.SilkS))
    (fp_text user RX (at -1.905 10.16) (layer F.SilkS))
    (fp_text user RTS (at -1.905 12.7) (layer F.SilkS))
    (pad 1 smd rect (at 0 0) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0 2.54) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at 0 5.08) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 4 smd rect (at 0 7.62) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 +3V3))
    (pad 5 smd rect (at 0 10.16) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at 0 12.7) (size 2.5 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${FAB}/fab.3dshapes/Header_SMD_01x06_P2.54mm_Horizontal_Male.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x03_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD8103)
    (at 128.016 55.626)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J18 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD (at 2.6 8.3) (layer F.Fab))
    (fp_text user %R (at 2.4 2.6 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /D18))
    (pad 2 smd rect (at 0 2.54) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at 0 5.08) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_1x03_P2.54mm_Horizontal_SMD (layer F.Cu) (tedit 61AD8151)
    (at 140.97 75.946)
    (descr https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf)
    (tags "horizontal pin header SMD 2.54mm")
    (attr smd)
    (fp_text reference J19 (at -1.524 -2.54 180) (layer F.SilkS))
    (fp_text value Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD (at 2.6 8.3) (layer F.Fab))
    (fp_text user %R (at 2.4 2.6 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 21 /D23))
    (pad 2 smd rect (at 0 2.54) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at 0 5.08) (size 5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.8))
    (min_thickness 0.3)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.528 125.222) (xy 107.696 125.222) (xy 107.696 46.228) (xy 160.528 46.228)
      )
    )
  )
)
