(kicad_pcb (version 20171130) (host pcbnew "(5.1.12-1-10_14)")
  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 495)
    (zones 0)
    (modules 28)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.45)
    (trace_clearance 0.45)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.7)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 /SWDIO)
  (net 5 /SWDCLK)
  (net 6 "Net-(J2-Pad6)")
  (net 7 "Net-(J2-Pad7)")
  (net 8 "Net-(J2-Pad8)")
  (net 9 /RESET)
  (net 10 /TX)
  (net 11 /RX)
  (net 12 /D23)
  (net 13 /D22)
  (net 14 /A03)
  (net 15 /A02)
  (net 16 /A05)
  (net 17 /A06)
  (net 18 /A07)
  (net 19 "Net-(U1-Pad4)")
  (net 20 "Net-(U1-Pad5)")
  (net 21 /D16)
  (net 22 /D-)
  (net 23 /D+)
  (net 24 /A04)
  (net 25 "Net-(D1-Pad2)")
  (net 26 "Net-(J1-Pad6)")
  (net 27 "Net-(J1-Pad4)")
  (net 28 "Net-(D2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.45)
    (trace_width 0.45)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /A02)
    (add_net /A03)
    (add_net /A04)
    (add_net /A05)
    (add_net /A06)
    (add_net /A07)
    (add_net /D+)
    (add_net /D-)
    (add_net /D16)
    (add_net /D22)
    (add_net /D23)
    (add_net /RESET)
    (add_net /RX)
    (add_net /SWDCLK)
    (add_net /SWDIO)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 144.272 160.13836 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_10uF2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:SOIC-20_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 61ADB952)
    (at 146.086838 132.850931 45)
    (descr "SOIC, 20 Pin, fab version")
    (tags "SOIC fab")
    (attr smd)
    (fp_text reference U1 (at 0 -7.35 45) (layer F.SilkS))
    (fp_text value Microcontroller_ATSAMD11D14A-SSUT (at 0 0 45) (layer F.SilkS))
    (fp_text user %R (at 0 0 45) (layer B.CrtYd))
    (pad 1 smd rect (at -4.65 -5.715 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 /A05))
    (pad 2 smd rect (at -4.65 -4.445 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 /A06))
    (pad 3 smd rect (at -4.65 -3.175 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /A07))
    (pad 4 smd rect (at -4.65 -1.905 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -4.65 -0.635 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -4.65 0.635 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /TX))
    (pad 7 smd rect (at -4.65 1.905 45) (size 1.8 0.6) (drill (offset -0.1 0)) (layers F.Cu F.Paste F.Mask)
      (net 11 /RX))
    (pad 8 smd rect (at -4.65 3.175 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /D16))
    (pad 9 smd rect (at -4.65 4.445 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /D22))
    (pad 10 smd rect (at -4.65 5.715 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /D23))
    (pad 11 smd rect (at 4.65 5.715 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /RESET))
    (pad 12 smd rect (at 4.65 4.445 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /SWDCLK))
    (pad 13 smd rect (at 4.65 3.175 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /SWDIO))
    (pad 14 smd rect (at 4.65 1.905 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /D-))
    (pad 15 smd rect (at 4.65 0.635 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /D+))
    (pad 16 smd rect (at 4.65 -0.635 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 4.65 -1.905 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 18 smd rect (at 4.65 -3.175 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /A02))
    (pad 19 smd rect (at 4.65 -4.445 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /A03))
    (pad 20 smd rect (at 4.65 -5.715 45) (size 2 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /A04))
    (model ${FAB}/fab.3dshapes/SOIC-20_7.5x12.8mm_P1.27mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 160.02 160.052 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_10uF1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 112.708 158.724 270)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW3 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -4.5 90) (layer F.Fab))
    (pad 1 smd rect (at -3.5 -2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /D23))
    (pad 1 smd rect (at 3.5 -2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /D23))
    (pad 2 smd rect (at -3.5 2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.5 2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 123.796 158.694 270)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW9 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -4.5 90) (layer F.Fab))
    (pad 1 smd rect (at -3.5 -2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 /A05))
    (pad 1 smd rect (at 3.5 -2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 16 /A05))
    (pad 2 smd rect (at -3.5 2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.5 2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 123.796 147.884 270)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW4 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -4.5 90) (layer F.Fab))
    (pad 2 smd rect (at 3.5 2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.5 2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.5 -2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /A06))
    (pad 1 smd rect (at -3.5 -2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /A06))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_2x02_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 6196D7E1)
    (at 139.43052 144.91716)
    (descr "surface-mounted straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x02 2.54mm double row")
    (attr smd)
    (fp_text reference J3 (at 0 -3.6) (layer F.SilkS))
    (fp_text value Conn_PinHeader_2x02_P2.54mm_Vertical_SMD (at 0 3.6) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2.525 -1.27) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /TX))
    (pad 3 smd rect (at -2.525 1.27) (size 2.95 1) (drill (offset -0.1 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 2.525 1.27) (size 2.95 1) (drill (offset 0.1 0)) (layers F.Cu F.Paste F.Mask)
      (net 11 /RX))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:PinHeader_2x05_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 60851B62)
    (at 138.4046 159.87704 90)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J2 (at 0 -4.235 90) (layer F.SilkS))
    (fp_text value Conn_PinHeader_2x05_P1.27mm_Vertical_SMD (at 0 4.235 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.95 -2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 4 /SWDIO))
    (pad 3 smd rect (at -1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 5 /SWDCLK))
    (pad 5 smd rect (at -1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad6)"))
    (pad 7 smd rect (at -1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad7)"))
    (pad 8 smd rect (at 1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad8)"))
    (pad 9 smd rect (at -1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 1.95 2.54 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 9 /RESET))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 61AF0D34)
    (at 157.95 137.45 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 1.4 1.7) (drill (offset -0.3 0)) (layers F.Cu F.Paste F.Mask)
      (net 15 /A02))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad2)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:LED_1206 (layer F.Cu) (tedit 61AF0D74)
    (at 156.464 144.24 90)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -2 0 90) (size 1.6 1.7) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 141.23936 151.78684 180)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 -4.5) (layer F.Fab))
    (pad 2 smd rect (at 3.5 2 180) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.5 2 180) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.5 -2 180) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /RESET))
    (pad 1 smd rect (at -3.5 -2 180) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /RESET))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 153.13 161.29)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10K2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /RESET))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:C_1206 (layer F.Cu) (tedit 6002C54C)
    (at 146.558 160.18104 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C_1uF1 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${FAB}/fab.3dshapes/C_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 153.702 158.242 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10K1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 /SWDCLK))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 129.286 138.904 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10K3 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 /A07))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 117.766 158.754 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10K4 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /D23))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 61AEF0B5)
    (at 128.796 146.364 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10K5 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /A06))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 117.846 148.264 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10K6 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /D22))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 118.24 137.128 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10K9 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /D16))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 128.756 158.704 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R_10K10 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 /A05))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 123.796 137.216 270)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW2 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -4.5 90) (layer F.Fab))
    (pad 1 smd rect (at -3.5 -2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /A07))
    (pad 1 smd rect (at 3.5 -2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /A07))
    (pad 2 smd rect (at -3.5 2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.5 2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 112.684 147.828 270)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW5 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -4.5 90) (layer F.Fab))
    (pad 2 smd rect (at 3.5 2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.5 2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.5 -2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /D22))
    (pad 1 smd rect (at -3.5 -2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /D22))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:Button_Omron_B3SN_6x6mm (layer F.Cu) (tedit 5EC65B05)
    (at 112.684 137.216 270)
    (descr "Surface Mount Tactile Switch for High-Density Packaging")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW8 (at 0 -4.5 90) (layer F.SilkS))
    (fp_text value BUTTON_B3SN (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -4.5 90) (layer F.Fab))
    (pad 2 smd rect (at 3.5 2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.5 2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.5 -2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 21 /D16))
    (pad 1 smd rect (at -3.5 -2 270) (size 2.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 21 /D16))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_B3S-1000.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_Micro-B_Molex-105017-0001 (layer F.Cu) (tedit 61AEC72D)
    (at 130.922 123.5055 180)
    (descr http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf)
    (tags "Micro-USB SMD Typ-B")
    (attr smd)
    (fp_text reference J1 (at 0 -3.1125) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0.3 4.3375) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.6875) (layer Dwgs.User))
    (fp_text user %R (at 0 0.8875) (layer F.Fab))
    (pad 6 smd rect (at 1 1.2375 180) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at -2.5 -1.4625 180) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad6)"))
    (pad 2 smd rect (at -0.65 -1.4625 180) (size 0.3 1.35) (layers F.Cu F.Paste F.Mask)
      (net 22 /D-))
    (pad 1 smd rect (at -1.3 -1.4625 180) (size 0.3 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at 1.3 -1.4625 180) (size 0.3 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65 -1.4625 180) (size 0.3 1.35) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 -1.4625 180) (size 0.3 1.35) (layers F.Cu F.Paste F.Mask)
      (net 23 /D+))
    (pad 6 thru_hole circle (at 2.5 -1.4625 180) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at -1 1.2375 180) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J1-Pad6)"))
    (pad 6 thru_hole oval (at -3.5 1.2375) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad6)"))
    (pad 6 thru_hole oval (at 3.5 1.2375 180) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 2.9 1.2375 180) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 26 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at -2.9 1.2375 180) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 26 "Net-(J1-Pad6)"))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex-105017-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:SOT-223-3_TabPin2 (layer F.Cu) (tedit 58CE4E7E)
    (at 156.108 152.132 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0 -4.5) (layer F.SilkS))
    (fp_text value Regulator_Linear_ZLDO1117-3.3V-1A (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:LED_1206 (layer F.Cu) (tedit 61AF0D46)
    (at 157.988 127.476 90)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -2 0 90) (size 1.6 1.7) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 136.93 138.69)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module fab:R_1206 (layer F.Cu) (tedit 60020482)
    (at 153.448 125.476 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /A03))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D2-Pad2)"))
    (model ${FAB}/fab.3dshapes/R_1206.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
)
