<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT 23&lt;/b&gt;</description>
</package>
<package name="2X5_1.27MM_SMD">
</package>
<package name="R1206FAB">
</package>
<package name="1X06SMD">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="SOIC127P600X160-14N">
</package>
<package name="USB-A-PCB">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="fab" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="fab" package="2X5_1.27MM_SMD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fab" package="1X06SMD" value="CONN_06_FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="U$2" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="fab" package="SOIC127P600X160-14N" value="UC_ATSAMD11C14A-SSUT">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" ARM® Cortex®-M0+ SAM D11C Microcontroller IC 32-Bit 48MHz 16KB (16K x 8) FLASH 14-SOIC "/>
<attribute name="MF" value="Microchip"/>
<attribute name="MP" value="ATSAMD11C14A-SSUT"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOIC-14 Microchip"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/ATSAMD11C14A-SSUT/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="fab" package="USB-A-PCB" value="CONN_USBPCB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="fab" package="1X06SMD" value="CONN_06_FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="R7" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+3V3">
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="12"/>
<contactref element="J1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="X1" pad="GND"/>
<contactref element="U1" pad="11"/>
<contactref element="U$2" pad="2"/>
<contactref element="J1" pad="9"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="7"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="X1" pad="5V"/>
<contactref element="IC1" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="R7" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="USBDM">
<contactref element="X1" pad="USB_M"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="USBDP">
<contactref element="X1" pad="USB_P"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="LED">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="CLK">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="DIO">
<contactref element="U1" pad="8"/>
<contactref element="J1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U$1" pad="5"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="RX">
<contactref element="U$1" pad="4"/>
<contactref element="U1" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="U$3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
