<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="52.07" y1="89.535" x2="52.07" y2="22.86" width="0.1524" layer="20"/>
<wire x1="52.07" y1="22.86" x2="116.84" y2="22.86" width="0.1524" layer="20"/>
<wire x1="116.84" y1="22.86" x2="116.84" y2="89.535" width="0.1524" layer="20"/>
<wire x1="116.84" y1="89.535" x2="52.07" y2="89.535" width="0.1524" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="MINI-SMA">
<description>mini-SMA diode</description>
</package>
<package name="ED555DS-2DS">
</package>
<package name="R1206FAB">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="PICOW">
</package>
<package name="1X06SMD">
</package>
<package name="SLIDESWITCH-CL-SB-22A">
</package>
</packages>
</library>
<library name="HW-04-08-T-S-315-SM">
<packages>
<package name="SAMTEC_HW-04-08-T-S-315-SM">
</package>
</packages>
</library>
<library name="HW-05-XX-X-S-XXX-SM">
<packages>
<package name="SAMTEC_HW-05-XX-X-S-XXX-SM">
</package>
</packages>
</library>
<library name="HW-06-XX-X-S-XXX-SM">
<packages>
<package name="SAMTEC_HW-06-XX-X-S-XXX-SM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="fab" package="MINI-SMA" value="DIODE_SCHOTTKY_CDBM1100-G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="VALUE"/>
</element>
<element name="U$6" library="fab" package="PICOW" value="PICOW"/>
<element name="R6" library="fab" package="R1206FAB" value="5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="fab" package="R1206FAB" value="5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="fab" package="ED555DS-2DS" value="CONN_02_TERM-FABLAB">
<attribute name="NAME"/>
</element>
<element name="J5" library="HW-04-08-T-S-315-SM" package="SAMTEC_HW-04-08-T-S-315-SM" value="HW-04-08-T-S-315-SM">
<attribute name="MANUFACTURER" value="SAMTEC "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="HW-04-08-T-S-315-SM" package="SAMTEC_HW-04-08-T-S-315-SM" value="HW-04-08-T-S-315-SM">
<attribute name="MANUFACTURER" value="SAMTEC "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="HW-04-08-T-S-315-SM" package="SAMTEC_HW-04-08-T-S-315-SM" value="HW-04-08-T-S-315-SM">
<attribute name="MANUFACTURER" value="SAMTEC "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="HW-05-XX-X-S-XXX-SM" package="SAMTEC_HW-05-XX-X-S-XXX-SM" value="HW-05-XX-X-S-XXX-SM">
<attribute name="MANUFACTURER" value="Samtec"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="fab" package="ED555DS-2DS" value="CONN_02_TERM-FABLAB">
<attribute name="NAME"/>
</element>
<element name="J10" library="fab" package="ED555DS-2DS" value="CONN_02_TERM-FABLAB">
<attribute name="NAME"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$7" library="fab" package="1X06SMD" value="CONN_06_FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="U$1" library="fab" package="1X06SMD" value="CONN_06_FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="J2" library="HW-06-XX-X-S-XXX-SM" package="SAMTEC_HW-06-XX-X-S-XXX-SM" value="HW-06-XX-X-S-XXX-SM">
<attribute name="MANUFACTURER" value="Samtec"/>
<attribute name="NAME"/>
<attribute name="PARTREV" value="A"/>
<attribute name="STANDARD" value="Manufacturer recommendations"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="fab" package="SLIDESWITCH-CL-SB-22A" value="SW_SLIDE-SWITCHSMT"/>
<element name="J1" library="fab" package="ED555DS-2DS" value="CONN_02_TERM-FABLAB">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="SD-SPI-CS">
<contactref element="U$6" pad="P$17"/>
<contactref element="J2" pad="04"/>
</signal>
<signal name="GPS-TX">
<contactref element="U$6" pad="P$2"/>
<contactref element="J8" pad="03"/>
</signal>
<signal name="S$8">
</signal>
<signal name="GPS-RX">
<contactref element="U$6" pad="P$1"/>
<contactref element="J8" pad="04"/>
</signal>
<signal name="BTN-UP">
<contactref element="U$6" pad="P$6"/>
<contactref element="U$7" pad="1"/>
</signal>
<signal name="BTN-PR">
<contactref element="U$6" pad="P$7"/>
<contactref element="U$7" pad="2"/>
</signal>
<signal name="BTN-DN">
<contactref element="U$6" pad="P$9"/>
<contactref element="U$7" pad="3"/>
</signal>
<signal name="N_AGND">
<contactref element="U$6" pad="P$33"/>
</signal>
<signal name="N$9">
<contactref element="D1" pad="ANODE"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$6" pad="P$13"/>
<contactref element="U$6" pad="P$18"/>
<contactref element="U$6" pad="P$23"/>
<contactref element="U$6" pad="P$28"/>
<contactref element="U$6" pad="P$3"/>
<contactref element="U$6" pad="P$38"/>
<contactref element="U$6" pad="P$8"/>
<contactref element="J6" pad="01"/>
<contactref element="J7" pad="01"/>
<contactref element="J8" pad="02"/>
<contactref element="J10" pad="1"/>
<contactref element="J5" pad="01"/>
<contactref element="R1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U$7" pad="5"/>
<contactref element="U$1" pad="5"/>
<contactref element="J2" pad="06"/>
<contactref element="S1" pad="P$3"/>
<contactref element="S1" pad="P$6"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="SD-SPI-MISO">
<contactref element="U$6" pad="P$16"/>
<contactref element="J2" pad="03"/>
</signal>
<signal name="SD-SPI-MOSI">
<contactref element="U$6" pad="P$15"/>
<contactref element="J2" pad="02"/>
</signal>
<signal name="SD-SPI-SCK">
<contactref element="U$6" pad="P$14"/>
<contactref element="J2" pad="01"/>
</signal>
<signal name="VDD">
<contactref element="U$6" pad="P$36"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="J6" pad="02"/>
<contactref element="J7" pad="02"/>
<contactref element="J8" pad="01"/>
<contactref element="J9" pad="1"/>
<contactref element="J5" pad="02"/>
<contactref element="U$7" pad="4"/>
<contactref element="U$1" pad="4"/>
<contactref element="J2" pad="05"/>
</signal>
<signal name="VSYS">
<contactref element="U$6" pad="P$39"/>
<contactref element="D1" pad="KATHODE"/>
</signal>
<signal name="BTN-R">
<contactref element="U$6" pad="P$25"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="BTN-H">
<contactref element="U$6" pad="P$26"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="BTN-L">
<contactref element="U$6" pad="P$27"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="I2C1-SCL">
<contactref element="R7" pad="1"/>
<contactref element="U$6" pad="P$5"/>
<contactref element="J6" pad="03"/>
<contactref element="J5" pad="03"/>
<contactref element="J7" pad="03"/>
</signal>
<signal name="I2C1-SDA">
<contactref element="R6" pad="1"/>
<contactref element="U$6" pad="P$4"/>
<contactref element="J6" pad="04"/>
<contactref element="J5" pad="04"/>
<contactref element="J7" pad="04"/>
</signal>
<signal name="H-ADC0">
<contactref element="U$6" pad="P$31"/>
<contactref element="J9" pad="2"/>
</signal>
<signal name="GP14-H">
<contactref element="J3" pad="1"/>
<contactref element="U$6" pad="P$29"/>
</signal>
<signal name="N$2">
<contactref element="U$4" pad="1"/>
<contactref element="S1" pad="P$2"/>
<contactref element="S1" pad="P$5"/>
</signal>
<signal name="3V">
<contactref element="S1" pad="P$4"/>
<contactref element="S1" pad="P$1"/>
<contactref element="J1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
