<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="67.31" y1="31.75" x2="160" y2="31.75" width="0" layer="20"/>
<wire x1="160" y1="31.75" x2="160.254" y2="89.078" width="0" layer="20"/>
<wire x1="160.254" y1="89.078" x2="67.564" y2="89.078" width="0" layer="20"/>
<wire x1="67.564" y1="89.078" x2="67.31" y2="31.75" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="PICOW">
</package>
<package name="2X04_THRU">
<description>2x4 header.  

Meant for nRF24L01+, but could be used for any header or 2x4 part.

Extra-wide pads for greater durability in soldering.</description>
</package>
</packages>
</library>
<library name="Connector">
<description>&lt;b&gt;Pin Headers,Terminal blocks, D-Sub, Backplane, FFC/FPC, Socket</description>
<packages>
<package name="1X03/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="fab" package="PICOW" value="PICOW"/>
<element name="U$2" library="fab" package="2X04_THRU" value="DEVICE_NRF24L01+"/>
<element name="JP1" library="Connector" package="1X03/90" value="PINHD-1X3/90">
<attribute name="CATEGORY" value="Headers"/>
<attribute name="DESCRIPTION" value="Header, Right Angle, 3 Position"/>
<attribute name="MANUFACTURER" value="Generic"/>
<attribute name="MPN" value="Generic"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMPERATURE" value="Generic"/>
<attribute name="PART_STATUS" value="Active"/>
<attribute name="PITCH" value="0.100&quot; (2.54mm)"/>
<attribute name="ROHS_COMPLIANCE" value="Generic"/>
<attribute name="SERIES" value="Generic"/>
<attribute name="SUB-CATEGORY" value="Headers, Male Pins"/>
<attribute name="TYPE" value="Board to Board or Cable, Unshrouded, Through Hole, Right Angle"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="Connector" package="1X03/90" value="PINHD-1X3/90">
<attribute name="CATEGORY" value="Headers"/>
<attribute name="DESCRIPTION" value="Header, Right Angle, 3 Position"/>
<attribute name="MANUFACTURER" value="Generic"/>
<attribute name="MPN" value="Generic"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMPERATURE" value="Generic"/>
<attribute name="PART_STATUS" value="Active"/>
<attribute name="PITCH" value="0.100&quot; (2.54mm)"/>
<attribute name="ROHS_COMPLIANCE" value="Generic"/>
<attribute name="SERIES" value="Generic"/>
<attribute name="SUB-CATEGORY" value="Headers, Male Pins"/>
<attribute name="TYPE" value="Board to Board or Cable, Unshrouded, Through Hole, Right Angle"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="Connector" package="1X05" value="PINHD-1X5">
<attribute name="CATEGORY" value="Headers"/>
<attribute name="DESCRIPTION" value="Header, Straight, 5 Position"/>
<attribute name="MANUFACTURER" value="Generic"/>
<attribute name="MPN" value="Generic"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMPERATURE" value="Generic"/>
<attribute name="PART_STATUS" value="Active"/>
<attribute name="PITCH" value="0.100&quot; (2.54mm)"/>
<attribute name="ROHS_COMPLIANCE" value="Generic"/>
<attribute name="SERIES" value="Generic"/>
<attribute name="SUB-CATEGORY" value="Headers, Male Pins"/>
<attribute name="TYPE" value="Board to Board or Cable, Unshrouded, Through Hole, Straight"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="Connector" package="1X05" value="PINHD-1X5">
<attribute name="CATEGORY" value="Headers"/>
<attribute name="DESCRIPTION" value="Header, Straight, 5 Position"/>
<attribute name="MANUFACTURER" value="Generic"/>
<attribute name="MPN" value="Generic"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMPERATURE" value="Generic"/>
<attribute name="PART_STATUS" value="Active"/>
<attribute name="PITCH" value="0.100&quot; (2.54mm)"/>
<attribute name="ROHS_COMPLIANCE" value="Generic"/>
<attribute name="SERIES" value="Generic"/>
<attribute name="SUB-CATEGORY" value="Headers, Male Pins"/>
<attribute name="TYPE" value="Board to Board or Cable, Unshrouded, Through Hole, Straight"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="P$23"/>
<contactref element="U$1" pad="P$38"/>
<contactref element="U$1" pad="P$13"/>
<contactref element="U$1" pad="P$18"/>
<contactref element="U$1" pad="P$28"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="U$1" pad="P$8"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="CE">
<contactref element="U$2" pad="2"/>
<contactref element="U$1" pad="P$30"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="P$31"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="P$32"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="8"/>
<contactref element="U$1" pad="P$36"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="CSN">
<contactref element="U$2" pad="7"/>
<contactref element="U$1" pad="P$35"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="6"/>
<contactref element="U$1" pad="P$34"/>
</signal>
<signal name="IRQ">
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="P$33"/>
</signal>
<signal name="ESC1">
<contactref element="JP2" pad="2"/>
<contactref element="U$1" pad="P$27"/>
</signal>
<signal name="ESC2">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="P$37"/>
</signal>
<signal name="SCL">
<contactref element="JP3" pad="3"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="P$4"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="DRDY">
<contactref element="U$1" pad="P$5"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="TX">
<contactref element="JP4" pad="3"/>
<contactref element="U$1" pad="P$6"/>
</signal>
<signal name="RX">
<contactref element="JP4" pad="4"/>
<contactref element="U$1" pad="P$7"/>
</signal>
<signal name="PPS">
<contactref element="JP4" pad="5"/>
<contactref element="U$1" pad="P$9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
