(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x0001000_7fffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "PWR")
	(net 3 "ANT")
	(net 4 "Net-(J3-Pin_6)")
	(net 5 "Net-(J3-Pin_7)")
	(net 6 "GND - IN")
	(net 7 "5V")
	(net 8 "Net-(J3-Pin_1)")
	(net 9 "Net-(J3-Pin_2)")
	(net 10 "Net-(J3-Pin_5)")
	(net 11 "D1")
	(net 12 "Net-(J3-Pin_4)")
	(net 13 "Net-(J3-Pin_3)")
	(net 14 "GND - OUT")
	(net 15 "LOOP")
	(net 16 "DAC")
	(net 17 "unconnected-(M1-SWDIO-Pad17)")
	(net 18 "unconnected-(M1-SWCLK-Pad20)")
	(net 19 "unconnected-(M1-GND-Pad19)")
	(net 20 "unconnected-(M1-RESET-Pad18)")
	(net 21 "unconnected-(M1-VIN-Pad16)")
	(net 22 "unconnected-(M1-GND-Pad15)")
	(net 23 "Net-(U1-DOUT)")
	(net 24 "Net-(U2-DOUT)")
	(net 25 "Net-(U3-DOUT)")
	(net 26 "DOUT")
	(net 27 "unconnected-(M1-D2-Pad3)")
	(net 28 "unconnected-(M1-D10-Pad11)")
	(net 29 "unconnected-(M1-D4-Pad5)")
	(net 30 "unconnected-(M1-D9-Pad10)")
	(net 31 "unconnected-(M1-D5-Pad6)")
	(net 32 "unconnected-(M1-D3-Pad4)")
	(net 33 "unconnected-(M1-D8-Pad9)")
	(net 34 "unconnected-(M1-3V3-Pad12)")
	(footprint "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 86.04 109.5 -90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J7"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Power Switch"
			(at 0 5.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 232 66.5 -90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Antenna Terminal"
			(at 0 5.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:LED_ADDR_Worldsemi_WS2812B"
		(layer "F.Cu")
		(at 231.55 89)
		(descr "SMD footprint for Worldsemi WS2812B addressable LED")
		(tags "neopixel led addressable smd")
		(property "Reference" "U1"
			(at 0 -3.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LED_ADDR_Worldsemi_WS2812B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "fab:LED_ADDR_Worldsemi_WS2812B"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://cdn.sparkfun.com/datasheets/BreakoutBoards/WS2812B.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Worldsemi WS2812B, Adafruit Industries LLC ADDRESS LED SERIAL RGB 100PK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Worldsemi*WS2812B*")
		(sheetname "Root")
		(sheetfile "theremin-pcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.45 -1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -2.45 1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "Net-(U1-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 2.45 1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 2.45 -1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "D1")
			(pinfunction "DIN")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD7_3DMODEL_DIR}/fab.3dshapes/LED_ADDR_Worldsemi_WS2812B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 168.8 109 -90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J7"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "Power Switch"
			(at 0 5.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x02*")
		(sheetname "Root")
		(sheetfile "theremin-pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND - IN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND - OUT")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x08_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 204.5 97)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "USB-C Internal to Board Interface"
			(at 0 20.11 0)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x08_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Through Hole 8 positions 0.100\" (2.54mm)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x08*")
		(sheetname "Root")
		(sheetfile "theremin-pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J3-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J3-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J3-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J3-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GND - OUT")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 168.8 111.5 -90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J7"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Power Switch"
			(at 0 5.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:LED_ADDR_Worldsemi_WS2812B"
		(layer "F.Cu")
		(at 182.55 96.35)
		(descr "SMD footprint for Worldsemi WS2812B addressable LED")
		(tags "neopixel led addressable smd")
		(property "Reference" "U2"
			(at 0 -3.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LED_ADDR_Worldsemi_WS2812B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "fab:LED_ADDR_Worldsemi_WS2812B"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://cdn.sparkfun.com/datasheets/BreakoutBoards/WS2812B.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Worldsemi WS2812B, Adafruit Industries LLC ADDRESS LED SERIAL RGB 100PK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Worldsemi*WS2812B*")
		(sheetname "Root")
		(sheetfile "theremin-pcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.45 -1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "PWR")
			(pinfunction "VDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -2.45 1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(U2-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 2.45 1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 2.45 -1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "Net-(U1-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD7_3DMODEL_DIR}/fab.3dshapes/LED_ADDR_Worldsemi_WS2812B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 90.8 69 -90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J8"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "Loop Terminal"
			(at 0 5.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x02*")
		(sheetname "Root")
		(sheetfile "theremin-pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "LOOP")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "LOOP")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:LED_ADDR_Worldsemi_WS2812B"
		(layer "F.Cu")
		(at 128.45 96.35)
		(descr "SMD footprint for Worldsemi WS2812B addressable LED")
		(tags "neopixel led addressable smd")
		(property "Reference" "U3"
			(at 0 -3.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LED_ADDR_Worldsemi_WS2812B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "fab:LED_ADDR_Worldsemi_WS2812B"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://cdn.sparkfun.com/datasheets/BreakoutBoards/WS2812B.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Worldsemi WS2812B, Adafruit Industries LLC ADDRESS LED SERIAL RGB 100PK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Worldsemi*WS2812B*")
		(sheetname "Root")
		(sheetfile "theremin-pcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.45 -1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "PWR")
			(pinfunction "VDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -2.45 1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U3-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 2.45 1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 2.45 -1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(U2-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD7_3DMODEL_DIR}/fab.3dshapes/LED_ADDR_Worldsemi_WS2812B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:LED_ADDR_Worldsemi_WS2812B"
		(layer "F.Cu")
		(at 86.95 88.5)
		(descr "SMD footprint for Worldsemi WS2812B addressable LED")
		(tags "neopixel led addressable smd")
		(property "Reference" "U4"
			(at 0 -3.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LED_ADDR_Worldsemi_WS2812B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:LED_ADDR_Worldsemi_WS2812B"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://cdn.sparkfun.com/datasheets/BreakoutBoards/WS2812B.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Worldsemi WS2812B, Adafruit Industries LLC ADDRESS LED SERIAL RGB 100PK"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Worldsemi*WS2812B*")
		(sheetname "Root")
		(sheetfile "theremin-pcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.45 -1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "PWR")
			(pinfunction "VDD")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -2.45 1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "DOUT")
			(pinfunction "DOUT")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 2.45 1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 2.45 -1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U3-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD7_3DMODEL_DIR}/fab.3dshapes/LED_ADDR_Worldsemi_WS2812B.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 99.3 109.5 -90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J7"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Power Switch"
			(at 0 5.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:SeeedStudio_XIAO_RP2040"
		(layer "F.Cu")
		(at 154.485 75.22 180)
		(descr "Footprint for Seeed Studio XIAO modules")
		(tags "xiao seeed studio module")
		(property "Reference" "M1"
			(at 0 -1.27 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Module_XIAO-RP2040 - ACTUAL XIAO SAMD21!"
			(at 0.005 1.27 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:SeeedStudio_XIAO_RP2040"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RP2040 XIAO RP2040 - ARM® Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SeeedStudio?XIAO?RP2040*")
		(sheetname "Root")
		(sheetfile "theremin-pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "RESET"
			(at 0 -5.96 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SWCLK"
			(at 2.54 -8.5 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 2.545 8.89 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 2.54 -5.96 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "VIN"
			(at -2.535 8.89 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SWDIO"
			(at 0 -8.5 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0.0025 3.81 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -7.615 -7.62 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "DAC")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "1" smd rect
			(at -7.615 -7.62 180)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "DAC")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at -7.615 -5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -7.615 -5.08 180)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at -7.615 -2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(M1-D2-Pad3)")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -7.615 -2.54 180)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "unconnected-(M1-D2-Pad3)")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at -7.615 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(M1-D3-Pad4)")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -7.615 0 180)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "unconnected-(M1-D3-Pad4)")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at -7.615 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(M1-D4-Pad5)")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -7.615 2.54 180)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "unconnected-(M1-D4-Pad5)")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at -7.615 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(M1-D5-Pad6)")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -7.615 5.08 180)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "unconnected-(M1-D5-Pad6)")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at -7.615 7.62 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "ANT")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -7.615 7.62 180)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "ANT")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole circle
			(at 7.62 7.62 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "LOOP")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at 7.62 7.62 180)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "LOOP")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole circle
			(at 7.62 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(M1-D8-Pad9)")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at 7.62 5.08 180)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "unconnected-(M1-D8-Pad9)")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at 7.62 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(M1-D9-Pad10)")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 7.62 2.54 180)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "unconnected-(M1-D9-Pad10)")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(M1-D10-Pad11)")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at 7.62 0 180)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "unconnected-(M1-D10-Pad11)")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at 7.62 -2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(M1-3V3-Pad12)")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "12" smd rect
			(at 7.62 -2.54 180)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "unconnected-(M1-3V3-Pad12)")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 7.62 -5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 7.62 -5.08 180)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" thru_hole circle
			(at 7.62 -7.62 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "5V")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 7.62 -7.62 180)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "5V")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at 1.275 8.89 90)
			(size 2.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "unconnected-(M1-GND-Pad15)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -1.265 8.89 90)
			(size 2.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "unconnected-(M1-VIN-Pad16)")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "17" smd circle
			(at -1.27 -8.5 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "unconnected-(M1-SWDIO-Pad17)")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
		)
		(pad "18" smd circle
			(at -1.27 -5.96 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "unconnected-(M1-RESET-Pad18)")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "19" smd circle
			(at 1.27 -5.96 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "unconnected-(M1-GND-Pad19)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "20" smd circle
			(at 1.27 -8.5 180)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "unconnected-(M1-SWCLK-Pad20)")
			(pinfunction "SWCLK")
			(pintype "input")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste" "F.Mask" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 150.685 81.72) (xy 149.285 81.72) (xy 149.285 79.52) (xy 150.685 79.52)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste" "F.Mask" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 150.685 85.77) (xy 149.285 85.77) (xy 149.285 83.72) (xy 150.685 83.72)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste" "F.Mask" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 159.685 81.72) (xy 158.285 81.72) (xy 158.285 79.52) (xy 159.685 79.52)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste" "F.Mask" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 159.685 85.77) (xy 158.285 85.77) (xy 158.285 83.72) (xy 159.685 83.72)
				)
			)
		)
	)
	(footprint "fab:PinHeader_1x08_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 218.55 126.66 -90)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "USB-C Terminal Outer Interface"
			(at 0 20.11 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x08_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Through Hole 8 positions 0.100\" (2.54mm)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x08*")
		(sheetname "Root")
		(sheetfile "theremin-pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 8.89 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J3-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J3-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J3-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J3-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "GND - IN")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 86.04 107 -90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J10"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.25 Audio Jack"
			(at 0 5.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x02*")
		(sheetname "Root")
		(sheetfile "theremin-pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "DAC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 99.3 107 -90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J9"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "3.5mm Audio Jack"
			(at 0 5.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x02*")
		(sheetname "Root")
		(sheetfile "theremin-pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "DAC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 90.8 66.5 -90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Antenna Terminal"
			(at 0 5.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 232 69 -90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "Antenna Terminal"
			(at 0 5.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x02*")
		(sheetname "Root")
		(sheetfile "theremin-pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "ANT")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "ANT")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_circle
		(center 76.35 70.35)
		(end 77.35 70.35)
		(locked yes)
		(fill solid)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70 64)
		(end 70 114.8)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70 64)
		(end 247.8 64)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 247.8 64)
		(end 247.8 114.8)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.3 137.66)
		(end 184.3 114.8)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.1 114.8)
		(end 247.8 114.8)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.1 137.66)
		(end 184.3 137.66)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 241.45 108.45)
		(end 242.45 108.45)
		(locked yes)
		(fill solid)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 77 108.45)
		(end 78 108.45)
		(locked yes)
		(fill solid)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 190.65 128.77)
		(end 191.65 128.77)
		(locked yes)
		(fill solid)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70 114.8)
		(end 184.3 114.8)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 228.75 128.77)
		(end 229.75 128.77)
		(locked yes)
		(fill solid)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 241.45 70.35)
		(end 242.45 70.35)
		(locked yes)
		(fill solid)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.1 137.66)
		(end 235.1 114.8)
		(locked yes)
		(layer "Edge.Cuts")
	)
	(gr_text "MIT HTMAA 2024"
		(at 200 74 0)
		(layer "F.Cu")
	)
	(gr_text "KJH THERICOLOR MKII"
		(at 139.5 108.5 0)
		(layer "F.Cu")
	)
)
