(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(lib_symbols
		(symbol "fab:Conn_PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(pin_names hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
			)
			(property "Value" "Conn_PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
				(at 0 -5.08 0)
			)
			(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Male connector, single row"
				(at 0 0 0)
			)
			(property "ki_keywords" "single row male connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*PinHeader*1x02*"
				(at 0 0 0)
			)
			(symbol "Conn_PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm_1_1"
				(rectangle
					(start -1.27 -1.905)
					(end 1.27 -3.175)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 0.635)
					(end 1.27 -0.635)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
			)
		)
		(symbol "fab:Conn_PinHeader_1x08_P2.54mm_Vertical_THT_D1.4mm"
			(pin_names hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 10.16 0)
			)
			(property "Value" "Conn_PinHeader_1x08_P2.54mm_Vertical_THT_D1.4mm"
				(at 0 -12.7 0)
			)
			(property "Footprint" "fab:PinHeader_1x08_P2.54mm_Vertical_THT_D1.4mm"
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Connector Header Through Hole 8 positions 0.100\" (2.54mm)"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*PinHeader*1x08*"
				(at 0 0 0)
			)
			(symbol "Conn_PinHeader_1x08_P2.54mm_Vertical_THT_D1.4mm_1_1"
				(rectangle
					(start -1.27 -9.525)
					(end 1.27 -10.795)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 -6.985)
					(end 1.27 -8.255)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 -4.445)
					(end 1.27 -5.715)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 -1.905)
					(end 1.27 -3.175)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 0.635)
					(end 1.27 -0.635)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 3.175)
					(end 1.27 1.905)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 5.715)
					(end 1.27 4.445)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 8.255)
					(end 1.27 6.985)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 7.62 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 5.08 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_4")
					(number "4")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_5")
					(number "5")
				)
				(pin passive line
					(at 5.08 -5.08 180)
					(length 3.81)
					(name "Pin_6")
					(number "6")
				)
				(pin passive line
					(at 5.08 -7.62 180)
					(length 3.81)
					(name "Pin_7")
					(number "7")
				)
				(pin passive line
					(at 5.08 -10.16 180)
					(length 3.81)
					(name "Pin_8")
					(number "8")
				)
			)
		)
		(symbol "fab:LED_ADDR_Worldsemi_WS2812B"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -5.08 5.715 0)
			)
			(property "Value" "LED_ADDR_Worldsemi_WS2812B"
				(at 0.635 5.715 0)
			)
			(property "Footprint" "fab:LED_ADDR_Worldsemi_WS2812B"
				(at 0 0 0)
			)
			(property "Datasheet" "http://cdn.sparkfun.com/datasheets/BreakoutBoards/WS2812B.pdf"
				(at 0 0 0)
			)
			(property "Description" "Worldsemi WS2812B, Adafruit Industries LLC ADDRESS LED SERIAL RGB 100PK"
				(at 0 0 0)
			)
			(property "ki_keywords" "adressable led neopixel 3094"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*Worldsemi*WS2812B*"
				(at 0 0 0)
			)
			(symbol "LED_ADDR_Worldsemi_WS2812B_0_1"
				(rectangle
					(start -5.08 5.08)
					(end 5.08 -5.08)
					(fill
						(type background)
					)
				)
			)
			(symbol "LED_ADDR_Worldsemi_WS2812B_1_1"
				(pin power_in line
					(at 0 7.62 270)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin output line
					(at 7.62 0 180)
					(length 2.54)
					(name "DOUT")
					(number "2")
				)
				(pin power_in line
					(at 0 -7.62 90)
					(length 2.54)
					(name "VSS")
					(number "3")
				)
				(pin input line
					(at -7.62 0 0)
					(length 2.54)
					(name "DIN")
					(number "4")
				)
			)
		)
		(symbol "fab:Module_XIAO-RP2040"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "M"
				(at -10.16 16.51 0)
			)
			(property "Value" "Module_XIAO-RP2040"
				(at 3.81 16.51 0)
			)
			(property "Footprint" "fab:SeeedStudio_XIAO_RP2040"
				(at 0 0 0)
			)
			(property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/"
				(at 0 0 0)
			)
			(property "Description" "RP2040 XIAO RP2040 - ARM® Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board"
				(at 0 0 0)
			)
			(property "ki_keywords" "XIAO RP2040 102010428"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*SeeedStudio?XIAO?RP2040*"
				(at 0 0 0)
			)
			(symbol "Module_XIAO-RP2040_1_1"
				(rectangle
					(start -10.16 15.24)
					(end 10.16 -15.24)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -12.7 12.7 0)
					(length 2.54)
					(name "D0")
					(number "1")
				)
				(pin bidirectional line
					(at -12.7 -10.16 0)
					(length 2.54)
					(name "D9")
					(number "10")
				)
				(pin bidirectional line
					(at -12.7 -12.7 0)
					(length 2.54)
					(name "D10")
					(number "11")
				)
				(pin power_in line
					(at -2.54 17.78 270)
					(length 2.54)
					(name "3V3")
					(number "12")
				)
				(pin power_in line
					(at -2.54 -17.78 90)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin power_in line
					(at 0 17.78 270)
					(length 2.54)
					(name "5V")
					(number "14")
				)
				(pin power_in line
					(at 0 -17.78 90)
					(length 2.54)
					(name "GND")
					(number "15")
				)
				(pin power_in line
					(at 2.54 17.78 270)
					(length 2.54)
					(name "VIN")
					(number "16")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "SWDIO")
					(number "17")
				)
				(pin input line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "RESET")
					(number "18")
				)
				(pin power_in line
					(at 2.54 -17.78 90)
					(length 2.54)
					(name "GND")
					(number "19")
				)
				(pin bidirectional line
					(at -12.7 10.16 0)
					(length 2.54)
					(name "D1")
					(number "2")
				)
				(pin input line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "SWCLK")
					(number "20")
				)
				(pin bidirectional line
					(at -12.7 7.62 0)
					(length 2.54)
					(name "D2")
					(number "3")
				)
				(pin bidirectional line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "D3")
					(number "4")
				)
				(pin bidirectional line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "D4")
					(number "5")
				)
				(pin bidirectional line
					(at -12.7 0 0)
					(length 2.54)
					(name "D5")
					(number "6")
				)
				(pin bidirectional line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "D6")
					(number "7")
				)
				(pin bidirectional line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "D7")
					(number "8")
				)
				(pin bidirectional line
					(at -12.7 -7.62 0)
					(length 2.54)
					(name "D8")
					(number "9")
				)
			)
		)
	)
	(junction
		(at 113.03 83.82)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 111.76 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 140.97 39.37) (xy 140.97 41.91)
		)
	)
	(wire
		(pts
			(xy 195.58 31.75) (xy 200.66 31.75)
		)
	)
	(wire
		(pts
			(xy 110.49 67.31) (xy 111.76 67.31)
		)
	)
	(wire
		(pts
			(xy 111.76 67.31) (xy 114.3 67.31)
		)
	)
	(wire
		(pts
			(xy 40.64 78.74) (xy 67.31 78.74)
		)
	)
	(wire
		(pts
			(xy 110.49 69.85) (xy 111.76 69.85)
		)
	)
	(wire
		(pts
			(xy 168.91 63.5) (xy 168.91 66.04)
		)
	)
	(wire
		(pts
			(xy 187.96 39.37) (xy 187.96 41.91)
		)
	)
	(wire
		(pts
			(xy 40.64 76.2) (xy 67.31 76.2)
		)
	)
	(wire
		(pts
			(xy 92.71 21.59) (xy 92.71 24.13)
		)
	)
	(wire
		(pts
			(xy 92.71 39.37) (xy 92.71 41.91)
		)
	)
	(wire
		(pts
			(xy 187.96 21.59) (xy 187.96 24.13)
		)
	)
	(wire
		(pts
			(xy 110.49 111.76) (xy 114.3 111.76)
		)
	)
	(wire
		(pts
			(xy 41.91 39.37) (xy 41.91 41.91)
		)
	)
	(wire
		(pts
			(xy 110.49 114.3) (xy 114.3 114.3)
		)
	)
	(wire
		(pts
			(xy 111.76 69.85) (xy 111.76 67.31)
		)
	)
	(wire
		(pts
			(xy 100.33 31.75) (xy 133.35 31.75)
		)
	)
	(wire
		(pts
			(xy 140.97 21.59) (xy 140.97 24.13)
		)
	)
	(wire
		(pts
			(xy 40.64 81.28) (xy 67.31 81.28)
		)
	)
	(wire
		(pts
			(xy 40.64 73.66) (xy 67.31 73.66)
		)
	)
	(wire
		(pts
			(xy 40.64 88.9) (xy 67.31 88.9)
		)
	)
	(wire
		(pts
			(xy 110.49 100.33) (xy 114.3 100.33)
		)
	)
	(wire
		(pts
			(xy 166.37 101.6) (xy 166.37 105.41)
		)
	)
	(wire
		(pts
			(xy 41.91 21.59) (xy 41.91 24.13)
		)
	)
	(wire
		(pts
			(xy 110.49 86.36) (xy 113.03 86.36)
		)
	)
	(wire
		(pts
			(xy 40.64 86.36) (xy 67.31 86.36)
		)
	)
	(wire
		(pts
			(xy 152.4 86.36) (xy 156.21 86.36)
		)
	)
	(wire
		(pts
			(xy 152.4 88.9) (xy 156.21 88.9)
		)
	)
	(wire
		(pts
			(xy 40.64 83.82) (xy 67.31 83.82)
		)
	)
	(wire
		(pts
			(xy 50.8 106.68) (xy 53.34 106.68)
		)
	)
	(wire
		(pts
			(xy 148.59 31.75) (xy 180.34 31.75)
		)
	)
	(wire
		(pts
			(xy 110.49 83.82) (xy 113.03 83.82)
		)
	)
	(wire
		(pts
			(xy 113.03 86.36) (xy 113.03 83.82)
		)
	)
	(wire
		(pts
			(xy 152.4 71.12) (xy 156.21 71.12)
		)
	)
	(wire
		(pts
			(xy 152.4 73.66) (xy 156.21 73.66)
		)
	)
	(wire
		(pts
			(xy 50.8 104.14) (xy 53.34 104.14)
		)
	)
	(wire
		(pts
			(xy 49.53 31.75) (xy 85.09 31.75)
		)
	)
	(wire
		(pts
			(xy 113.03 83.82) (xy 114.3 83.82)
		)
	)
	(wire
		(pts
			(xy 110.49 97.79) (xy 114.3 97.79)
		)
	)
	(wire
		(pts
			(xy 29.21 31.75) (xy 34.29 31.75)
		)
	)
	(global_label "DAC"
		(shape input)
		(at 114.3 111.76 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 120.9138 111.76 0)
		)
	)
	(global_label "GND"
		(shape input)
		(at 41.91 41.91 270)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 41.91 48.7657 90)
		)
	)
	(global_label "GND - OUT"
		(shape input)
		(at 67.31 91.44 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 53.3181 91.44 0)
		)
	)
	(global_label "GND"
		(shape input)
		(at 140.97 41.91 270)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 140.97 48.7657 90)
		)
	)
	(global_label "GND - OUT"
		(shape input)
		(at 53.34 106.68 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 67.3319 106.68 0)
		)
	)
	(global_label "GND"
		(shape input)
		(at 166.37 105.41 270)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 166.37 112.2657 90)
		)
	)
	(global_label "5V"
		(shape input)
		(at 168.91 63.5 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 168.91 58.2167 90)
		)
	)
	(global_label "PWR"
		(shape input)
		(at 140.97 21.59 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 140.97 14.6134 90)
		)
	)
	(global_label "D1"
		(shape input)
		(at 152.4 73.66 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 146.9353 73.66 0)
		)
	)
	(global_label "GND"
		(shape input)
		(at 187.96 41.91 270)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 187.96 48.7657 90)
		)
	)
	(global_label "GND - IN"
		(shape input)
		(at 53.34 104.14 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 65.6386 104.14 0)
		)
	)
	(global_label "D1"
		(shape input)
		(at 29.21 31.75 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 23.7453 31.75 0)
		)
	)
	(global_label "PWR"
		(shape input)
		(at 92.71 21.59 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 92.71 14.6134 90)
		)
	)
	(global_label "PWR"
		(shape input)
		(at 187.96 21.59 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 187.96 14.6134 90)
		)
	)
	(global_label "GND"
		(shape input)
		(at 114.3 100.33 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 121.1557 100.33 0)
		)
	)
	(global_label "ANT"
		(shape input)
		(at 152.4 86.36 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 146.0281 86.36 0)
		)
	)
	(global_label "DAC"
		(shape input)
		(at 114.3 97.79 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 120.9138 97.79 0)
		)
	)
	(global_label "LOOP"
		(shape input)
		(at 114.3 83.82 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 122.2443 83.82 0)
		)
	)
	(global_label "GND"
		(shape input)
		(at 92.71 41.91 270)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 92.71 48.7657 90)
		)
	)
	(global_label "5V"
		(shape input)
		(at 41.91 21.59 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 41.91 16.3067 90)
		)
	)
	(global_label "DAC"
		(shape input)
		(at 152.4 71.12 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 145.7862 71.12 0)
		)
	)
	(global_label "DOUT"
		(shape input)
		(at 200.66 31.75 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 208.5438 31.75 0)
		)
	)
	(global_label "LOOP"
		(shape input)
		(at 152.4 88.9 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 144.4557 88.9 0)
		)
	)
	(global_label "GND - IN"
		(shape input)
		(at 40.64 91.44 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 52.9386 91.44 0)
		)
	)
	(global_label "GND"
		(shape input)
		(at 114.3 114.3 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 121.1557 114.3 0)
		)
	)
	(global_label "ANT"
		(shape input)
		(at 114.3 67.31 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 120.6719 67.31 0)
		)
	)
	(symbol
		(lib_id "fab:LED_ADDR_Worldsemi_WS2812B")
		(at 41.91 31.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 63.5 25.4314 0)
		)
		(property "Value" "LED_ADDR_Worldsemi_WS2812B"
			(at 63.5 27.9714 0)
		)
		(property "Footprint" "fab:LED_ADDR_Worldsemi_WS2812B"
			(at 41.91 31.75 0)
		)
		(property "Datasheet" "http://cdn.sparkfun.com/datasheets/BreakoutBoards/WS2812B.pdf"
			(at 41.91 31.75 0)
		)
		(property "Description" "Worldsemi WS2812B, Adafruit Industries LLC ADDRESS LED SERIAL RGB 100PK"
			(at 41.91 31.75 0)
		)
		(pin "3")
		(pin "2")
		(pin "1")
		(pin "4")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm")
		(at 105.41 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J8"
			(at 105.41 78.74 0)
		)
		(property "Value" "Loop Terminal"
			(at 105.41 81.28 0)
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 105.41 83.82 0)
		)
		(property "Datasheet" "~"
			(at 105.41 83.82 0)
		)
		(property "Description" "Male connector, single row"
			(at 105.41 83.82 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "theremin-pcb"
				(path
					(reference "J8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm")
		(at 45.72 104.14 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J7"
			(at 45.72 99.06 0)
		)
		(property "Value" "Power Switch"
			(at 45.72 101.6 0)
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 45.72 104.14 0)
		)
		(property "Datasheet" "~"
			(at 45.72 104.14 0)
		)
		(property "Description" "Male connector, single row"
			(at 45.72 104.14 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "J7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Module_XIAO-RP2040")
		(at 168.91 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "M1"
			(at 203.2 80.0414 0)
		)
		(property "Value" "Module_XIAO-RP2040 - ACTUAL XIAO SAMD21!"
			(at 203.2 82.5814 0)
		)
		(property "Footprint" "fab:SeeedStudio_XIAO_RP2040"
			(at 168.91 83.82 0)
		)
		(property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/"
			(at 168.91 83.82 0)
		)
		(property "Description" "RP2040 XIAO RP2040 - ARM® Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board"
			(at 168.91 83.82 0)
		)
		(pin "18")
		(pin "6")
		(pin "8")
		(pin "20")
		(pin "11")
		(pin "13")
		(pin "19")
		(pin "16")
		(pin "10")
		(pin "14")
		(pin "12")
		(pin "7")
		(pin "15")
		(pin "1")
		(pin "17")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "2")
		(pin "9")
		(instances
			(project ""
				(path
					(reference "M1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm")
		(at 105.41 111.76 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J10"
			(at 105.41 106.68 0)
		)
		(property "Value" "0.25 Audio Jack"
			(at 105.41 109.22 0)
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 105.41 111.76 0)
		)
		(property "Datasheet" "~"
			(at 105.41 111.76 0)
		)
		(property "Description" "Male connector, single row"
			(at 105.41 111.76 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "theremin-pcb"
				(path
					(reference "J10")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:LED_ADDR_Worldsemi_WS2812B")
		(at 92.71 31.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 114.3 25.4314 0)
		)
		(property "Value" "LED_ADDR_Worldsemi_WS2812B"
			(at 114.3 27.9714 0)
		)
		(property "Footprint" "fab:LED_ADDR_Worldsemi_WS2812B"
			(at 92.71 31.75 0)
		)
		(property "Datasheet" "http://cdn.sparkfun.com/datasheets/BreakoutBoards/WS2812B.pdf"
			(at 92.71 31.75 0)
		)
		(property "Description" "Worldsemi WS2812B, Adafruit Industries LLC ADDRESS LED SERIAL RGB 100PK"
			(at 92.71 31.75 0)
		)
		(pin "3")
		(pin "2")
		(pin "1")
		(pin "4")
		(instances
			(project "theremin-pcb"
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:LED_ADDR_Worldsemi_WS2812B")
		(at 140.97 31.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U3"
			(at 162.56 25.4314 0)
		)
		(property "Value" "LED_ADDR_Worldsemi_WS2812B"
			(at 162.56 27.9714 0)
		)
		(property "Footprint" "fab:LED_ADDR_Worldsemi_WS2812B"
			(at 140.97 31.75 0)
		)
		(property "Datasheet" "http://cdn.sparkfun.com/datasheets/BreakoutBoards/WS2812B.pdf"
			(at 140.97 31.75 0)
		)
		(property "Description" "Worldsemi WS2812B, Adafruit Industries LLC ADDRESS LED SERIAL RGB 100PK"
			(at 140.97 31.75 0)
		)
		(pin "3")
		(pin "2")
		(pin "1")
		(pin "4")
		(instances
			(project "theremin-pcb"
				(path
					(reference "U3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_1x08_P2.54mm_Vertical_THT_D1.4mm")
		(at 72.39 81.28 0)
		(mirror y)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J4"
			(at 72.39 68.58 0)
		)
		(property "Value" "USB-C Internal to Board Interface"
			(at 72.39 71.12 0)
		)
		(property "Footprint" "fab:PinHeader_1x08_P2.54mm_Vertical_THT_D1.4mm"
			(at 72.39 81.28 0)
		)
		(property "Datasheet" "~"
			(at 72.39 81.28 0)
		)
		(property "Description" "Connector Header Through Hole 8 positions 0.100\" (2.54mm)"
			(at 72.39 81.28 0)
		)
		(pin "7")
		(pin "5")
		(pin "6")
		(pin "3")
		(pin "2")
		(pin "8")
		(pin "1")
		(pin "4")
		(instances
			(project ""
				(path
					(reference "J4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm")
		(at 105.41 67.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J1"
			(at 105.41 62.23 0)
		)
		(property "Value" "Antenna Terminal"
			(at 105.41 64.77 0)
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 105.41 67.31 0)
		)
		(property "Datasheet" "~"
			(at 105.41 67.31 0)
		)
		(property "Description" "Male connector, single row"
			(at 105.41 67.31 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "theremin-pcb"
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:LED_ADDR_Worldsemi_WS2812B")
		(at 187.96 31.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U4"
			(at 209.55 25.4314 0)
		)
		(property "Value" "LED_ADDR_Worldsemi_WS2812B"
			(at 209.55 27.9714 0)
		)
		(property "Footprint" "fab:LED_ADDR_Worldsemi_WS2812B"
			(at 187.96 31.75 0)
		)
		(property "Datasheet" "http://cdn.sparkfun.com/datasheets/BreakoutBoards/WS2812B.pdf"
			(at 187.96 31.75 0)
		)
		(property "Description" "Worldsemi WS2812B, Adafruit Industries LLC ADDRESS LED SERIAL RGB 100PK"
			(at 187.96 31.75 0)
		)
		(pin "3")
		(pin "2")
		(pin "1")
		(pin "4")
		(instances
			(project "theremin-pcb"
				(path
					(reference "U4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_1x08_P2.54mm_Vertical_THT_D1.4mm")
		(at 35.56 81.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J3"
			(at 35.56 68.58 0)
		)
		(property "Value" "USB-C Terminal Outer Interface"
			(at 35.56 71.12 0)
		)
		(property "Footprint" "fab:PinHeader_1x08_P2.54mm_Vertical_THT_D1.4mm"
			(at 35.56 81.28 0)
		)
		(property "Datasheet" "~"
			(at 35.56 81.28 0)
		)
		(property "Description" "Connector Header Through Hole 8 positions 0.100\" (2.54mm)"
			(at 35.56 81.28 0)
		)
		(pin "1")
		(pin "2")
		(pin "7")
		(pin "6")
		(pin "5")
		(pin "8")
		(pin "3")
		(pin "4")
		(instances
			(project ""
				(path
					(reference "J3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm")
		(at 105.41 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J9"
			(at 105.41 92.71 0)
		)
		(property "Value" "3.5mm Audio Jack"
			(at 105.41 95.25 0)
		)
		(property "Footprint" "fab:PinHeader_1x02_P2.54mm_Vertical_THT_D1.4mm"
			(at 105.41 97.79 0)
		)
		(property "Datasheet" "~"
			(at 105.41 97.79 0)
		)
		(property "Description" "Male connector, single row"
			(at 105.41 97.79 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "theremin-pcb"
				(path
					(reference "J9")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
