(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x0001000_7fffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "../../week05/")
		)
	)
	(net 0 "")
	(net 1 "PWR_GND")
	(net 2 "A0")
	(net 3 "PWR_5V")
	(net 4 "A1")
	(net 5 "A2")
	(net 6 "A3")
	(net 7 "A6")
	(net 8 "A7")
	(net 9 "A8")
	(net 10 "A9")
	(net 11 "A10")
	(net 12 "PWR_3V3")
	(net 13 "SDA")
	(net 14 "SCL")
	(net 15 "Net-(J10-Pin_5)")
	(footprint "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
		(layer "F.Cu")
		(at 161.08 108 -90)
		(descr "https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf")
		(tags "horizontal pin header SMD 2.54mm")
		(property "Reference" "J6"
			(at -2.5 -3.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 26.6 7.42 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x03*")
		(sheetname "Root")
		(sheetfile "RP_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2 2.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 2.54 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "PWR_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 5.08 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "A7")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
		(layer "F.Cu")
		(at 120.5 108 -90)
		(descr "https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf")
		(tags "horizontal pin header SMD 2.54mm")
		(property "Reference" "J3"
			(at -3 -3.42 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 26.6 7.42 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x03*")
		(sheetname "Root")
		(sheetfile "RP_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2 1.58 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 2.54 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "PWR_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 5.08 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "A2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
		(layer "F.Cu")
		(at 187.08 108 -90)
		(descr "https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf")
		(tags "horizontal pin header SMD 2.54mm")
		(property "Reference" "J8"
			(at -1.524 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 26.6 7.42 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x03*")
		(sheetname "Root")
		(sheetfile "RP_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2.4 2.6 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 2.54 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "PWR_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 5.08 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "A9")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
		(layer "F.Cu")
		(at 198.42 108 -90)
		(descr "https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf")
		(tags "horizontal pin header SMD 2.54mm")
		(property "Reference" "J9"
			(at -1.524 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 26.5 7.42 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x03*")
		(sheetname "Root")
		(sheetfile "RP_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2.4 2.6 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 2.54 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "PWR_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 5.08 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "A10")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
		(layer "F.Cu")
		(at 147.54 108 -90)
		(descr "https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf")
		(tags "horizontal pin header SMD 2.54mm")
		(property "Reference" "J5"
			(at -1.524 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 26.6 7.42 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x03*")
		(sheetname "Root")
		(sheetfile "RP_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2.4 2.6 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 2.54 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "PWR_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 5.08 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "A6")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x05_P2.54mm_Horizontal_SMD"
		(layer "F.Cu")
		(at 193.7 62.4)
		(descr "https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf")
		(tags "horizontal pin header SMD 2.54mm")
		(property "Reference" "J10"
			(at -1.524 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_1x05_P2.54mm_Horizontal_SMD"
			(at 25.5 13.335 0)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x05_P2.54mm_Horizontal_SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x05*")
		(sheetname "Root")
		(sheetfile "RP_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2.54 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 2.54)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "PWR_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 5.08)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "PWR_3V3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0 7.62)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "SDA")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 10.16)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(J10-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(model "${FAB}/fab.3dshapes/Header_SMD_01x05_P2.54mm_Horizontal_Male.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:SeeedStudio_XIAO_SocketSMD"
		(layer "F.Cu")
		(at 147.97 70.58)
		(descr "Footprint for Seeed Studio XIAO modules, SMD socket (female header)")
		(tags "xiao seeed studio module socket female header")
		(property "Reference" "M2"
			(at 0.0025 -2.149 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Module_XIAO-RP2040_SocketSMD"
			(at 14.53 -16.58 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:SeeedStudio_XIAO_SocketSMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RP2040 XIAO RP2040 - ARM® Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board SMD Socket (Female Header)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SeeedStudio?XIAO?SocketSMD*")
		(sheetname "Root")
		(sheetfile "RP_Breakout.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -9.27 -7.62)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "A0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -5.97 -5.08)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "A1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -9.27 -2.54)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "A2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -5.97 0)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "A3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -9.27 2.54)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "SDA")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -5.97 5.08)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "SCL")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -9.27 7.62)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "A6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at 9.27 7.62)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "A7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at 5.97 5.08)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "A8")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 9.27 2.54)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "A9")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at 5.97 0)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "A10")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at 9.27 -2.54)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "PWR_3V3")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 5.97 -5.08)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "PWR_GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 9.27 -7.62)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_5V")
			(pinfunction "5V")
			(pintype "power_in")
		)
	)
	(footprint "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
		(layer "F.Cu")
		(at 107 108 -90)
		(descr "https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf")
		(tags "horizontal pin header SMD 2.54mm")
		(property "Reference" "J2"
			(at -1.524 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 26.6 7.42 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x03*")
		(sheetname "Root")
		(sheetfile "RP_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2.4 2.6 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 2.54 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "PWR_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 5.08 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "A1")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
		(layer "F.Cu")
		(at 95.55 108 -90)
		(descr "https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf")
		(tags "horizontal pin header SMD 2.54mm")
		(property "Reference" "J1"
			(at -1.524 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 26.6 7.42 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x03*")
		(sheetname "Root")
		(sheetfile "RP_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2.4 2.6 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 2.54 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "PWR_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 5.08 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "A0")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
		(layer "F.Cu")
		(at 134.04 108 -90)
		(descr "https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf")
		(tags "horizontal pin header SMD 2.54mm")
		(property "Reference" "J4"
			(at -1.524 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 26.6 7.42 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x03*")
		(sheetname "Root")
		(sheetfile "RP_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2.4 2.6 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 2.54 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "PWR_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 5.08 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "A3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:Jumper_1206"
		(layer "F.Cu")
		(at 175.3 74 180)
		(descr "Jumper, based on SMD 1206 resistor")
		(tags "jumper smd 1206")
		(property "Reference" "JP1"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jumper_1206"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:Jumper_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper based on 0 Ohm 1206 resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper*")
		(sheetname "Root")
		(sheetfile "RP_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(J10-Pin_5)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "SCL")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
		(layer "F.Cu")
		(at 174.66 108 -90)
		(descr "https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf")
		(tags "horizontal pin header SMD 2.54mm")
		(property "Reference" "J7"
			(at -1.524 -2.54 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 26.6 7.42 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x03_P2.54mm_Horizontal_SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x03*")
		(sheetname "Root")
		(sheetfile "RP_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2.4 2.6 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 2.54 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "PWR_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 5.08 270)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "A8")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "$(FAB)/fab.3dshapes/Header_SMD_01x03_P2.54mm_Horizontal_Male.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 86 60)
		(end 200.5 114.5)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "KJH"
		(at 96 70 45)
		(layer "F.Cu")
	)
)
