<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="109.22" y1="93.98" x2="109.22" y2="16.51" width="0.4064" layer="20"/>
<wire x1="109.22" y1="93.98" x2="71.12" y2="93.98" width="0.4064" layer="20"/>
<wire x1="71.12" y1="93.98" x2="71.12" y2="16.51" width="0.4064" layer="20"/>
<wire x1="71.12" y1="16.51" x2="109.22" y2="16.51" width="0.4064" layer="20"/>
<hole x="74.93" y="90.17" drill="3.2"/>
<hole x="105.41" y="90.17" drill="3.2"/>
<hole x="74.93" y="20.32" drill="3.2"/>
<hole x="105.41" y="20.32" drill="3.2"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="R1206FAB">
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="2X02SMD">
</package>
<package name="MINI-SMA">
<description>mini-SMA diode</description>
</package>
<package name="SOIC127P599X175-9N">
</package>
<package name="XIAO_ESP32_S3">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="1X06SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="fab" package="6MM_SWITCH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="fab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="fab" package="2X02SMD" value="CONN_02X2-PINHEAD-SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="fab" package="C1206FAB" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="fab" package="C1206FAB" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="fab" package="MINI-SMA" value="DIODE_SCHOTTKY_CDBM1100-G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="fab" package="2X02SMD" value="CONN_02X2-PINHEAD-SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$6" library="fab" package="SOIC127P599X175-9N" value="TB67H451FNG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="fab" package="C1206FAB" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="fab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$7" library="fab" package="XIAO_ESP32_S3" value="XIAO_ESP32_S3">
</element>
<element name="U2" library="fab" package="SOT223" value="VR_REGULATOR_SOT223">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fab" package="1X06SMD" value="CONN_06_FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U$4" pad="1"/>
<contactref element="U$7" pad="P$10"/>
</signal>
<signal name="N$7">
<contactref element="S1" pad="2"/>
<contactref element="U$7" pad="P$8"/>
</signal>
<signal name="N$19">
<contactref element="C6" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="D1" pad="KATHODE"/>
<contactref element="U$6" pad="4"/>
<contactref element="U$7" pad="P$14"/>
</signal>
<signal name="N$15">
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="S1" pad="4"/>
<contactref element="U$6" pad="9"/>
<contactref element="U$6" pad="1"/>
<contactref element="U$6" pad="7"/>
<contactref element="C4" pad="1"/>
<contactref element="U$7" pad="P$27"/>
<contactref element="U$7" pad="P$26"/>
<contactref element="U$7" pad="P$24"/>
<contactref element="U$7" pad="P$13"/>
<contactref element="U$7" pad="P$23"/>
<contactref element="U$7" pad="P$15"/>
<contactref element="U$7" pad="P$21"/>
<contactref element="U$7" pad="P$25"/>
<contactref element="U2" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U$5" pad="3"/>
<contactref element="U$5" pad="4"/>
<contactref element="U$6" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="U$6" pad="3"/>
<contactref element="U$7" pad="P$3"/>
</signal>
<signal name="N$12">
<contactref element="U$6" pad="2"/>
<contactref element="U$7" pad="P$4"/>
</signal>
<signal name="N$13">
<contactref element="U$6" pad="8"/>
<contactref element="U$5" pad="1"/>
<contactref element="U$5" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U$6" pad="5"/>
<contactref element="U$3" pad="4"/>
<contactref element="U$3" pad="3"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="N$16">
<contactref element="D1" pad="ANODE"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$7" pad="P$5"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="U$7" pad="P$6"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U$7" pad="P$12"/>
<contactref element="U$1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
