(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "SDA")
	(net 2 "SCL")
	(net 3 "GND")
	(net 4 "5V")
	(net 5 "D7")
	(net 6 "Net-(BZ1-+)")
	(net 7 "D1")
	(net 8 "D10")
	(net 9 "D9")
	(net 10 "Net-(D2-K)")
	(net 11 "/D6")
	(net 12 "/D3")
	(net 13 "/D2")
	(net 14 "3.3V")
	(net 15 "unconnected-(M1-D0-Pad1)")
	(footprint "fab:SeeedStudio_XIAO_SocketSMD"
		(layer "F.Cu")
		(at 134.14 51.145)
		(descr "Footprint for Seeed Studio XIAO modules, SMD socket (female header)")
		(tags "xiao seeed studio module socket female header")
		(property "Reference" "M1"
			(at 0.0025 -2.149 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Module_XIAO-ESP32C3_SocketSMD"
			(at 0.0025 0.391 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:SeeedStudio_XIAO_SocketSMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://wiki.seeedstudio.com/XIAO_ESP32C3_Getting_Started/"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESP32-C3 Transceiver; 802.11 a/b/g/n (Wi-Fi, WiFi, WLAN), Bluetooth® Smart 4.x Low Energy (BLE) 2.4GHz Evaluation Board SMD Socket Female Header"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SeeedStudio?XIAO?SocketSMD*")
		(sheetname "Root")
		(sheetfile "FishFeeder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.0025 2.931 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -9.27 -7.62)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "unconnected-(M1-D0-Pad1)")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -5.97 -5.08)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -9.27 -2.54)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -5.97 0)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "/D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -9.27 2.54)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "SDA")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -5.97 5.08)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "SCL")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -9.27 7.62)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at 9.27 7.62)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "D1")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at 5.97 5.08)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "D7")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 9.27 2.54)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "D9")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at 5.97 0)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "D10")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at 9.27 -2.54)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "3.3V")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 5.97 -5.08)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 9.27 -7.62)
			(size 2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "5V")
			(pinfunction "5V")
			(pintype "power_in")
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 143.5 66)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R1"
			(at 0 -1.85 360)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 1.9 360)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:R_1206"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FishFeeder.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "D7")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "3.3V")
			(pintype "passive")
		)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "OLED:128x64OLED"
		(layer "F.Cu")
		(at 108.54 51.1)
		(property "Reference" "J3"
			(at 0 0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "OLED_4_PIN"
			(at -7.747 -7.62 0)
			(layer "F.Fab")
		)
		(property "Footprint" "OLED:128x64OLED"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "FishFeeder.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at -3.62 -10.6 90)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -1.08 -10.6 90)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 1.46 -10.6 90)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 4 -10.6 90)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "SDA")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 107.5 32.5)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R4"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "0k"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:R_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FishFeeder.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "GND")
			(pintype "passive")
		)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Buzzer_Beeper:Buzzer_12x9.5RM7.6"
		(layer "F.Cu")
		(at 174.7 65)
		(descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
		(tags "buzzer")
		(property "Reference" "BZ1"
			(at 3.8 -7.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "Buzzer"
			(at 3.8 7.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Buzzer_Beeper:Buzzer_12x9.5RM7.6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Buzzer, polarized"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Buzzer*")
		(sheetname "Root")
		(sheetfile "FishFeeder.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at -0.01 -2.54 0)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -0.01 -2.54 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 3.8 -4 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(BZ1-+)")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.6 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Buzzer_Beeper.3dshapes/Buzzer_12x9.5RM7.6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 162 51 90)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R2"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "68"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:R_1206"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FishFeeder.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 90)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 90)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "GND")
			(pintype "passive")
		)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline"
		(layer "F.Cu")
		(at 117.595 79.615)
		(descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "U1"
			(at 1.27 -3.56 0)
			(layer "F.SilkS")
		)
		(property "Value" "DS18B20"
			(at 1.27 2.79 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-92_Inline"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/DS18B20.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Programmable Resolution 1-Wire Digital Thermometer TO-92"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO*92*")
		(sheetname "Root")
		(sheetfile "FishFeeder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -0.5 0)
			(size 1.24 1.97)
			(drill 0.75
				(offset 0 0.015)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 1.27 0)
			(size 1.54 1.54)
			(drill 0.75
				(offset 0 -0.02)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "D7")
			(pinfunction "DQ")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole oval
			(at 3 0)
			(size 1.43 1.48)
			(drill 0.75
				(offset -0.005 0.01)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "3.3V")
			(pinfunction "V_{DD}")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 159 61.5)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R3"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:R_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "FishFeeder.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "D9")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(BZ1-+)")
			(pintype "passive")
		)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D5.0mm_Horizontal_O6.35mm_Z15.0mm"
		(layer "F.Cu")
		(at 168.5 55.04 90)
		(descr "LED, diameter 5.0mm, horizontal offset 6.35mm, z-position of LED center 15.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 1.27 -1.96 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 16.01 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D5.0mm_Horizontal_O6.35mm_Z15.0mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "FishFeeder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 9.85 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "D10")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm_Horizontal_O6.35mm_Z15.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 152.5 65.475)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J5"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "SG90_Motor_3_PIN"
			(at 0 7.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "FishFeeder.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "D1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 88 22)
		(end 193 88.5)
		(fill none)
		(layer "Edge.Cuts")
	)
)
