(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(M1-D2-Pad3)")
	(net 2 "unconnected-(M1-5V-Pad14)")
	(net 3 "PWR_3V3")
	(net 4 "unconnected-(M1-SWDIO-Pad17)")
	(net 5 "unconnected-(M1-GND-Pad19)")
	(net 6 "PWR_GND")
	(net 7 "unconnected-(M1-D1-Pad2)")
	(net 8 "unconnected-(M1-VIN-Pad16)")
	(net 9 "CS")
	(net 10 "unconnected-(M1-SWCLK-Pad20)")
	(net 11 "unconnected-(M1-RESET-Pad18)")
	(net 12 "unconnected-(J1-Pin_7-Pad7)")
	(net 13 "unconnected-(J1-Pin_8-Pad8)")
	(net 14 "SCL")
	(net 15 "SDL")
	(net 16 "T_SENSE")
	(net 17 "unconnected-(J5-Pin_1-Pad1)")
	(net 18 "unconnected-(J1-Pin_6-Pad6)")
	(net 19 "unconnected-(J1-Pin_5-Pad5)")
	(net 20 "unconnected-(J2-DAT1-Pad8)")
	(net 21 "unconnected-(J2-SHIELD-Pad9)")
	(net 22 "unconnected-(J2-DAT2-Pad1)")
	(net 23 "unconnected-(J3-Pin_2-Pad2)")
	(net 24 "unconnected-(J3-Pin_6-Pad6)")
	(net 25 "unconnected-(J3-Pin_7-Pad7)")
	(net 26 "unconnected-(J3-Pin_8-Pad8)")
	(net 27 "SDA")
	(net 28 "MISO")
	(net 29 "SCK")
	(net 30 "RX")
	(net 31 "MOSI")
	(net 32 "TX")
	(net 33 "Net-(U2-VLED+-Pad10)")
	(net 34 "unconnected-(U2-~{INT}-Pad13)")
	(net 35 "unconnected-(U2-NC-Pad5)")
	(net 36 "unconnected-(U2-NC-Pad7)")
	(net 37 "unconnected-(U2-NC-Pad8)")
	(net 38 "unconnected-(U2-NC-Pad14)")
	(net 39 "unconnected-(U2-NC-Pad6)")
	(net 40 "unconnected-(U2-NC-Pad1)")
	(footprint "fab:PinHeader_1x08_P2.54mm_Horizontal_SMD"
		(layer "F.Cu")
		(at 83.5 83.4 180)
		(descr "https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf")
		(tags "horizontal pin header SMD 2.54mm")
		(property "Reference" "J3"
			(at -1.524 -2.54 360)
			(layer "F.SilkS")
		)
		(property "Value" "Headers for GPS"
			(at -4.5 20.955 360)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x08_P2.54mm_Horizontal_SMD"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x08*")
		(sheetname "Root")
		(sheetfile "starpcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2.54 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 2.54 180)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "unconnected-(J3-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 5.08 180)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "PWR_GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0 7.62 180)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 10.16 180)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "SDA")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0 12.7 180)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "unconnected-(J3-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0 15.24 180)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "unconnected-(J3-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0 17.78 180)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "unconnected-(J3-Pin_8-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${FAB}/fab.3dshapes/Header_SMD_01x08_P2.54mm_Horizontal_Male.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 119.5 93)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R1"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.9 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "fab:R_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "Root")
		(sheetfile "starpcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_3V3")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "T_SENSE")
			(pintype "passive")
		)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 121.8 101.48)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R2"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.99k"
			(at 11.5 2.16 0)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:R_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "Root")
		(sheetfile "starpcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_3V3")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "SCL")
			(pintype "passive")
		)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:MicroSD_Amphenol_114-00841-68"
		(layer "F.Cu")
		(at 103.2 99.5)
		(descr "Wurth Elektronik MicroSD Card Holder with Lid 693072010801 http://katalog.we-online.de/em/datasheet/693072010801.pdf")
		(tags "socket slot microsd sdcard card")
		(property "Reference" "J2"
			(at -3.62 -3.71 0)
			(layer "F.SilkS")
		)
		(property "Value" "Micro_SD_Socket"
			(at -0.2 4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:MicroSD_Amphenol_114-00841-68"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa188.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zero-Drift, Precision, Low-Noise, Rail-to-Rail Output, 36-V Operational Amplifier, TSOT-23-5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*MicroSD*")
		(sheetname "Root")
		(sheetfile "starpcb.kicad_sch")
		(attr smd)
		(fp_text user "KEEP CLEAR"
			(at -0.93 -5.95 0)
			(layer "F.Fab")
		)
		(fp_text user "CLEAR"
			(at -0.85 -9.99 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 3.2 0)
			(size 0.7 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "unconnected-(J2-DAT2-Pad1)")
			(pinfunction "DAT2")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at 2.1 0)
			(size 0.7 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "CS")
			(pinfunction "DAT3/CD")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at 1 0)
			(size 0.7 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "MOSI")
			(pinfunction "CMD")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -0.1 0)
			(size 0.7 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at -1.2 0)
			(size 0.7 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "SCK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -2.3 0)
			(size 0.7 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "PWR_GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at -3.4 0)
			(size 0.7 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "MISO")
			(pinfunction "DAT0")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -4.5 0)
			(size 0.7 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "unconnected-(J2-DAT1-Pad8)")
			(pinfunction "DAT1")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -6.3 -7.6)
			(size 0.8 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "unconnected-(J2-SHIELD-Pad9)")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -6 -9.3)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "unconnected-(J2-SHIELD-Pad9)")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -5.9 -0.1)
			(size 1.3 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "unconnected-(J2-SHIELD-Pad9)")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 5.4 -10.8)
			(size 1 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "unconnected-(J2-SHIELD-Pad9)")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 5.65 -0.1)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "unconnected-(J2-SHIELD-Pad9)")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 6 -8.35)
			(size 0.8 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "unconnected-(J2-SHIELD-Pad9)")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connectors_Card.3dshapes/MicroSd_Wurth_693072010801.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x08_P2.54mm_Horizontal_SMD"
		(layer "F.Cu")
		(at 124.5 65.3)
		(descr "https://s3.amazonaws.com/catalogspreads-pdf/PAGE112-113%20.100%20MALE%20HDR.pdf")
		(tags "horizontal pin header SMD 2.54mm")
		(property "Reference" "J1"
			(at -1.524 -2.54 180)
			(layer "F.SilkS")
		)
		(property "Value" "MPU-6050_1x08_P2.54mm"
			(at 0.1 20.955 0)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x08_P2.54mm_Horizontal_SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x08*")
		(sheetname "Root")
		(sheetfile "starpcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2.54 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 2.54)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "PWR_GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 5.08)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0 7.62)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "SDL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 10.16)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "unconnected-(J1-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0 12.7)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "unconnected-(J1-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0 15.24)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "unconnected-(J1-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0 17.78)
			(size 2.5 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "unconnected-(J1-Pin_8-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(model "${FAB}/fab.3dshapes/Header_SMD_01x08_P2.54mm_Horizontal_Male.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:SeeedStudio_XIAO_RP2040"
		(layer "F.Cu")
		(at 103.38 74.96)
		(descr "Footprint for Seeed Studio XIAO modules")
		(tags "xiao seeed studio module")
		(property "Reference" "M1"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Module_XIAO-RP2040"
			(at 0.005 1.27 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:SeeedStudio_XIAO_RP2040"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RP2040 XIAO RP2040 - ARM® Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SeeedStudio?XIAO?RP2040*")
		(sheetname "Root")
		(sheetfile "starpcb.kicad_sch")
		(attr through_hole)
		(fp_text user "RESET"
			(at 0 -5.96 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "VIN"
			(at -2.535 8.89 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 2.545 8.89 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SWCLK"
			(at 2.54 -8.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SWDIO"
			(at 0 -8.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 2.54 -5.96 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0.0025 3.81 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -7.615 -7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "T_SENSE")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "1" smd rect
			(at -7.615 -7.62)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "T_SENSE")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at -7.615 -5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(M1-D1-Pad2)")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -7.615 -5.08)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "unconnected-(M1-D1-Pad2)")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at -7.615 -2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "unconnected-(M1-D2-Pad3)")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -7.615 -2.54)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "unconnected-(M1-D2-Pad3)")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at -7.615 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "CS")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -7.615 0)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "CS")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at -7.615 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "SDA")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -7.615 2.54)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "SDA")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at -7.615 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "SCL")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -7.615 5.08)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "SCL")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at -7.615 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "TX")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -7.615 7.62)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "TX")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole circle
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "RX")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at 7.62 7.62)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "RX")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole circle
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "SCK")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at 7.62 5.08)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "SCK")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "MISO")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 7.62 2.54)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "MISO")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "MOSI")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at 7.62 0)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "MOSI")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at 7.62 -2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "PWR_3V3")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "12" smd rect
			(at 7.62 -2.54)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_3V3")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 7.62 -5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "PWR_GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 7.62 -5.08)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "PWR_GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" thru_hole circle
			(at 7.62 -7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "unconnected-(M1-5V-Pad14)")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 7.62 -7.62)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "unconnected-(M1-5V-Pad14)")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at 1.275 8.89 270)
			(size 2.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "PWR_GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -1.265 8.89 270)
			(size 2.4 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "unconnected-(M1-VIN-Pad16)")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "17" smd circle
			(at -1.27 -8.5)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "unconnected-(M1-SWDIO-Pad17)")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
		)
		(pad "18" smd circle
			(at -1.27 -5.96)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "unconnected-(M1-RESET-Pad18)")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "19" smd circle
			(at 1.27 -5.96)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "unconnected-(M1-GND-Pad19)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "20" smd circle
			(at 1.27 -8.5)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "unconnected-(M1-SWCLK-Pad20)")
			(pinfunction "SWCLK")
			(pintype "input")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste" "F.Mask" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 98.18 64.41) (xy 99.58 64.41) (xy 99.58 66.46) (xy 98.18 66.46)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste" "F.Mask" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 98.18 68.46) (xy 99.58 68.46) (xy 99.58 70.66) (xy 98.18 70.66)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste" "F.Mask" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 107.18 64.41) (xy 108.58 64.41) (xy 108.58 66.46) (xy 107.18 66.46)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Paste" "F.Mask" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 107.18 68.46) (xy 108.58 68.46) (xy 108.58 70.66) (xy 107.18 70.66)
				)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 124 108)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "TH1"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "Thermistor_NTC"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:R_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.fi/datasheet/2/18/AAS-920-324F-Thermometrics-NTC-SMD-032717-web-1018802.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Temperature dependent resistor, Amphenol NHQ103B375T10, negative temperature coefficient, NTC Thermistor 10k 1206 (3216 Metric)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*1206*")
		(sheetname "Root")
		(sheetfile "starpcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "T_SENSE")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "PWR_GND")
			(pintype "passive")
		)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "OptoDevice:Maxim_OLGA-14_3.3x5.6mm_P0.8mm"
		(layer "F.Cu")
		(at 83.2 95.6)
		(descr "https://pdfserv.maximintegrated.com/land_patterns/90-0602.PDF")
		(tags "OLGA-14 OESIP-14")
		(property "Reference" "U2"
			(at 0.22 -4.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "HR Sensor MAX30102"
			(at 1.25 4.17 180)
			(layer "F.Fab")
		)
		(property "Footprint" "OptoDevice:Maxim_OLGA-14_3.3x5.6mm_P0.8mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX30102.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Heart Rate Sensor, 14-OLGA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Maxim*OLGA*3.3x5.6mm*P0.8mm*")
		(sheetname "Root")
		(sheetfile "starpcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.01 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 -2.4)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "unconnected-(U2-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -1.2 -1.6)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.2 -0.8)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -1.2 0)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "PWR_GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -1.2 0.8)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "unconnected-(U2-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "6" smd roundrect
			(at -1.2 1.6)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "unconnected-(U2-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd roundrect
			(at -1.2 2.4)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "unconnected-(U2-NC-Pad7)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "8" smd roundrect
			(at 1.2 2.4)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "unconnected-(U2-NC-Pad8)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "9" smd roundrect
			(at 1.2 1.6)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U2-VLED+-Pad10)")
			(pinfunction "VLED+")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 1.2 0.8)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U2-VLED+-Pad10)")
			(pinfunction "VLED+")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at 1.2 0)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "PWR_3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at 1.2 -0.8)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "PWR_GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd roundrect
			(at 1.2 -1.6)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "unconnected-(U2-~{INT}-Pad13)")
			(pinfunction "~{INT}")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 1.2 -2.4)
			(size 0.75 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "unconnected-(U2-NC-Pad14)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(model "${KICAD8_3DMODEL_DIR}/OptoDevice.3dshapes/Maxim_OLGA-14_3.3x5.6mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 133.3 105)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R3"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.99k"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:R_1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "Root")
		(sheetfile "starpcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "PWR_3V3")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "SDA")
			(pintype "passive")
		)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_1x01_P2.54mm_Vertical_THT_D2mm"
		(layer "F.Cu")
		(at 72.5 106)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J5"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_1x01_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 3.1 0)
			(layer "F.Fab")
		)
		(property "Footprint" "fab:PinHeader_1x01_P2.54mm_Vertical_THT_D2mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Connector pin header 2.54mm pitch vertical tht"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x01*")
		(sheetname "Root")
		(sheetfile "starpcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -0.6 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5 5)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(J5-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
)
