(kicad_sch
	(version 20231120)
	(generator "eeschema")
	(generator_version "8.0")
	(paper "A4")
	(lib_symbols
		(symbol "Sensor:MAX30102"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at 7.62 15.24 0)
			)
			(property "Value" "MAX30102"
				(at 7.62 12.7 0)
			)
			(property "Footprint" "OptoDevice:Maxim_OLGA-14_3.3x5.6mm_P0.8mm"
				(at 0 -2.54 0)
			)
			(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX30102.pdf"
				(at 0 0 0)
			)
			(property "Description" "Heart Rate Sensor, 14-OLGA"
				(at 0 0 0)
			)
			(property "ki_keywords" "Heart Rate"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Maxim*OLGA*3.3x5.6mm*P0.8mm*"
				(at 0 0 0)
			)
			(symbol "MAX30102_0_1"
				(rectangle
					(start -7.62 10.16)
					(end 7.62 -10.16)
					(fill
						(type background)
					)
				)
			)
			(symbol "MAX30102_1_1"
				(pin no_connect line
					(at -7.62 5.08 0)
					(length 2.54) hide
					(name "NC")
					(number "1")
				)
				(pin passive line
					(at 0 12.7 270)
					(length 2.54) hide
					(name "VLED+")
					(number "10")
				)
				(pin power_in line
					(at -5.08 12.7 270)
					(length 2.54)
					(name "VDD")
					(number "11")
				)
				(pin power_in line
					(at 2.54 -12.7 90)
					(length 2.54)
					(name "GND")
					(number "12")
				)
				(pin output line
					(at 10.16 0 180)
					(length 2.54)
					(name "~{INT}")
					(number "13")
				)
				(pin no_connect line
					(at 7.62 2.54 180)
					(length 2.54) hide
					(name "NC")
					(number "14")
				)
				(pin input line
					(at -10.16 2.54 0)
					(length 2.54)
					(name "SCL")
					(number "2")
				)
				(pin bidirectional line
					(at -10.16 0 0)
					(length 2.54)
					(name "SDA")
					(number "3")
				)
				(pin power_in line
					(at -2.54 -12.7 90)
					(length 2.54)
					(name "PGND")
					(number "4")
				)
				(pin no_connect line
					(at 7.62 -7.62 180)
					(length 2.54) hide
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 7.62 -5.08 180)
					(length 2.54) hide
					(name "NC")
					(number "6")
				)
				(pin no_connect line
					(at -7.62 -2.54 0)
					(length 2.54) hide
					(name "NC")
					(number "7")
				)
				(pin no_connect line
					(at 7.62 5.08 180)
					(length 2.54) hide
					(name "NC")
					(number "8")
				)
				(pin power_in line
					(at 0 12.7 270)
					(length 2.54)
					(name "VLED+")
					(number "9")
				)
			)
		)
		(symbol "fab:Conn_PinHeader_1x01_P2.54mm_Vertical_THT_D1.4mm"
			(pin_names
				(offset 1.016) hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
			)
			(property "Value" "Conn_PinHeader_1x01_P2.54mm_Vertical_THT_D1.4mm"
				(at 0 -2.54 0)
			)
			(property "Footprint" "fab:PinHeader_1x01_P2.54mm_Vertical_THT_D1.4mm"
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Connector pin header 2.54mm pitch vertical tht"
				(at 0 0 0)
			)
			(property "ki_keywords" "Connector pin header 2.54mm pitch vertical tht"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*PinHeader*1x01*"
				(at 0 0 0)
			)
			(symbol "Conn_PinHeader_1x01_P2.54mm_Vertical_THT_D1.4mm_1_1"
				(rectangle
					(start -1.27 0.635)
					(end 1.27 -0.635)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
			)
		)
		(symbol "fab:Conn_PinHeader_1x08_P2.54mm_Horizontal_SMD"
			(pin_names hide)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 10.16 0)
			)
			(property "Value" "Conn_PinHeader_1x08_P2.54mm_Horizontal_SMD"
				(at 0 -12.7 0)
			)
			(property "Footprint" "fab:PinHeader_1x08_P2.54mm_Horizontal_SMD"
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Male connector, single row"
				(at 0 0 0)
			)
			(property "ki_keywords" "single row male connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*PinHeader*1x08*"
				(at 0 0 0)
			)
			(symbol "Conn_PinHeader_1x08_P2.54mm_Horizontal_SMD_1_1"
				(rectangle
					(start -1.27 -9.525)
					(end 1.27 -10.795)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 -6.985)
					(end 1.27 -8.255)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 -4.445)
					(end 1.27 -5.715)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 -1.905)
					(end 1.27 -3.175)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 0.635)
					(end 1.27 -0.635)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 3.175)
					(end 1.27 1.905)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 5.715)
					(end 1.27 4.445)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start -1.27 8.255)
					(end 1.27 6.985)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at 5.08 7.62 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 5.08 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_4")
					(number "4")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_5")
					(number "5")
				)
				(pin passive line
					(at 5.08 -5.08 180)
					(length 3.81)
					(name "Pin_6")
					(number "6")
				)
				(pin passive line
					(at 5.08 -7.62 180)
					(length 3.81)
					(name "Pin_7")
					(number "7")
				)
				(pin passive line
					(at 5.08 -10.16 180)
					(length 3.81)
					(name "Pin_8")
					(number "8")
				)
			)
		)
		(symbol "fab:Micro_SD_Socket"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at -13.97 15.24 0)
			)
			(property "Value" "Micro_SD_Socket"
				(at 1.27 15.24 0)
			)
			(property "Footprint" "fab:MicroSD_Amphenol_114-00841-68"
				(at 0 0 0)
			)
			(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa188.pdf"
				(at 0 0 0)
			)
			(property "Description" "Zero-Drift, Precision, Low-Noise, Rail-to-Rail Output, 36-V Operational Amplifier, TSOT-23-5"
				(at 0 0 0)
			)
			(property "ki_keywords" "single opamp zero-drift 114-00841-68"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*MicroSD*"
				(at 0 0 0)
			)
			(symbol "Micro_SD_Socket_0_1"
				(rectangle
					(start -13.97 13.97)
					(end 13.97 -13.97)
					(fill
						(type background)
					)
				)
			)
			(symbol "Micro_SD_Socket_1_1"
				(pin bidirectional line
					(at -17.78 -7.62 0)
					(length 3.81)
					(name "DAT2")
					(number "1")
				)
				(pin bidirectional line
					(at -17.78 -10.16 0)
					(length 3.81)
					(name "DAT3/CD")
					(number "2")
				)
				(pin input line
					(at -17.78 5.08 0)
					(length 3.81)
					(name "CMD")
					(number "3")
				)
				(pin power_in line
					(at 0 17.78 270)
					(length 3.81)
					(name "VDD")
					(number "4")
				)
				(pin input line
					(at -17.78 2.54 0)
					(length 3.81)
					(name "CLK")
					(number "5")
				)
				(pin power_in line
					(at 0 -17.78 90)
					(length 3.81)
					(name "VSS")
					(number "6")
				)
				(pin bidirectional line
					(at -17.78 -2.54 0)
					(length 3.81)
					(name "DAT0")
					(number "7")
				)
				(pin bidirectional line
					(at -17.78 -5.08 0)
					(length 3.81)
					(name "DAT1")
					(number "8")
				)
				(pin passive line
					(at 17.78 -10.16 180)
					(length 3.81)
					(name "SHIELD")
					(number "9")
				)
			)
		)
		(symbol "fab:Module_XIAO-RP2040"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "M"
				(at -10.16 16.51 0)
			)
			(property "Value" "Module_XIAO-RP2040"
				(at 3.81 16.51 0)
			)
			(property "Footprint" "fab:SeeedStudio_XIAO_RP2040"
				(at 0 0 0)
			)
			(property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/"
				(at 0 0 0)
			)
			(property "Description" "RP2040 XIAO RP2040 - ARM® Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board"
				(at 0 0 0)
			)
			(property "ki_keywords" "XIAO RP2040 102010428"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*SeeedStudio?XIAO?RP2040*"
				(at 0 0 0)
			)
			(symbol "Module_XIAO-RP2040_1_1"
				(rectangle
					(start -10.16 15.24)
					(end 10.16 -15.24)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -12.7 12.7 0)
					(length 2.54)
					(name "D0")
					(number "1")
				)
				(pin bidirectional line
					(at -12.7 -10.16 0)
					(length 2.54)
					(name "D9")
					(number "10")
				)
				(pin bidirectional line
					(at -12.7 -12.7 0)
					(length 2.54)
					(name "D10")
					(number "11")
				)
				(pin power_in line
					(at -2.54 17.78 270)
					(length 2.54)
					(name "3V3")
					(number "12")
				)
				(pin power_in line
					(at -2.54 -17.78 90)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin power_in line
					(at 0 17.78 270)
					(length 2.54)
					(name "5V")
					(number "14")
				)
				(pin power_in line
					(at 0 -17.78 90)
					(length 2.54)
					(name "GND")
					(number "15")
				)
				(pin power_in line
					(at 2.54 17.78 270)
					(length 2.54)
					(name "VIN")
					(number "16")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "SWDIO")
					(number "17")
				)
				(pin input line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "RESET")
					(number "18")
				)
				(pin power_in line
					(at 2.54 -17.78 90)
					(length 2.54)
					(name "GND")
					(number "19")
				)
				(pin bidirectional line
					(at -12.7 10.16 0)
					(length 2.54)
					(name "D1")
					(number "2")
				)
				(pin input line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "SWCLK")
					(number "20")
				)
				(pin bidirectional line
					(at -12.7 7.62 0)
					(length 2.54)
					(name "D2")
					(number "3")
				)
				(pin bidirectional line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "D3")
					(number "4")
				)
				(pin bidirectional line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "D4")
					(number "5")
				)
				(pin bidirectional line
					(at -12.7 0 0)
					(length 2.54)
					(name "D5")
					(number "6")
				)
				(pin bidirectional line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "D6")
					(number "7")
				)
				(pin bidirectional line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "D7")
					(number "8")
				)
				(pin bidirectional line
					(at -12.7 -7.62 0)
					(length 2.54)
					(name "D8")
					(number "9")
				)
			)
		)
		(symbol "fab:PWR_3V3"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "PWR_3V3"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+3V3\""
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "PWR_3V3_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "PWR_3V3_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0) hide
					(name "PWR_3V3")
					(number "1")
				)
			)
		)
		(symbol "fab:PWR_GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "PWR_GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "PWR_GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "PWR_GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0) hide
					(name "PWR_GND")
					(number "1")
				)
			)
		)
		(symbol "fab:R_1206"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.54 0 90)
			)
			(property "Value" "R_1206"
				(at -2.54 0 90)
			)
			(property "Footprint" "fab:R_1206"
				(at 0 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor RC1206FR-074M99L RC1206FR-07499KL RC1206FR-0749K9L RC1206FR-0749R9L RC1206FR-074R99L ERJ-8BWJR100V RC1206FR-070RL RC1206FR-071RL RC1206FR-0710RL RC1206FR-07100RL RC1206FR-07499RL RC1206FR-071KL RC1206FR-074K99L RC1206FR-0710KL RC1206FR-07100KL RC1206FR-071ML RC1206FR-0710ML PT1206FR-070R1L"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*R*1206*"
				(at 0 0 0)
			)
			(symbol "R_1206_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type background)
					)
				)
			)
			(symbol "R_1206_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
		(symbol "fab:Thermistor_NTC"
			(pin_numbers hide)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "TH"
				(at -3.81 0 90)
			)
			(property "Value" "Thermistor_NTC"
				(at 2.54 0 90)
			)
			(property "Footprint" "fab:R_1206"
				(at 0 0 0)
			)
			(property "Datasheet" "https://www.mouser.fi/datasheet/2/18/AAS-920-324F-Thermometrics-NTC-SMD-032717-web-1018802.pdf"
				(at 0 0 0)
			)
			(property "Description" "Temperature dependent resistor, Amphenol NHQ103B375T10, negative temperature coefficient, NTC Thermistor 10k 1206 (3216 Metric)"
				(at 0 0 0)
			)
			(property "ki_keywords" "thermistor NTC resistor sensor NHQ103B375T10"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*1206*"
				(at 0 0 0)
			)
			(symbol "Thermistor_NTC_0_1"
				(arc
					(start -3.048 2.159)
					(mid -3.0505 2.3165)
					(end -3.175 2.413)
					(fill
						(type none)
					)
				)
				(arc
					(start -3.048 2.159)
					(mid -2.9736 1.9794)
					(end -2.794 1.905)
					(fill
						(type none)
					)
				)
				(arc
					(start -3.048 2.794)
					(mid -2.9736 2.6144)
					(end -2.794 2.54)
					(fill
						(type none)
					)
				)
				(arc
					(start -2.794 1.905)
					(mid -2.6144 1.9794)
					(end -2.54 2.159)
					(fill
						(type none)
					)
				)
				(arc
					(start -2.794 2.54)
					(mid -2.434 2.5608)
					(end -2.159 2.794)
					(fill
						(type none)
					)
				)
				(arc
					(start -2.794 3.048)
					(mid -2.9736 2.9736)
					(end -3.048 2.794)
					(fill
						(type none)
					)
				)
				(arc
					(start -2.54 2.794)
					(mid -2.6144 2.9736)
					(end -2.794 3.048)
					(fill
						(type none)
					)
				)
				(rectangle
					(start -1.016 2.54)
					(end 1.016 -2.54)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -2.54 2.159) (xy -2.54 2.794)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 2.54) (xy -1.778 1.524) (xy 1.778 -1.524) (xy 1.778 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 -3.683) (xy -2.54 -1.397) (xy -2.794 -2.159) (xy -2.286 -2.159) (xy -2.54 -1.397) (xy -2.54 -1.651)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -1.778 -1.397) (xy -1.778 -3.683) (xy -2.032 -2.921) (xy -1.524 -2.921) (xy -1.778 -3.683)
						(xy -1.778 -3.429)
					)
					(fill
						(type outline)
					)
				)
			)
			(symbol "Thermistor_NTC_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
		)
	)
	(junction
		(at 80.01 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 33.02 116.84)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 104.14 50.8) (xy 105.41 50.8)
		)
	)
	(wire
		(pts
			(xy 33.02 104.14) (xy 33.02 105.41)
		)
	)
	(wire
		(pts
			(xy 33.02 115.57) (xy 33.02 116.84)
		)
	)
	(wire
		(pts
			(xy 33.02 129.54) (xy 33.02 128.27)
		)
	)
	(wire
		(pts
			(xy 33.02 116.84) (xy 33.02 118.11)
		)
	)
	(wire
		(pts
			(xy 39.37 116.84) (xy 33.02 116.84)
		)
	)
	(wire
		(pts
			(xy 80.01 67.31) (xy 82.55 67.31)
		)
	)
	(global_label "SDA"
		(shape input)
		(at 69.85 46.99 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 63.2967 46.99 0)
		)
	)
	(global_label "SDL"
		(shape input)
		(at 38.1 41.91 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 44.5928 41.91 0)
		)
	)
	(global_label "MOSI"
		(shape input)
		(at 105.41 43.18 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 97.8286 43.18 0)
		)
	)
	(global_label "SCL"
		(shape input)
		(at 68.58 99.06 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 62.0872 99.06 0)
		)
	)
	(global_label "SCK"
		(shape input)
		(at 69.85 57.15 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 63.1153 57.15 0)
		)
	)
	(global_label "T_SENSE"
		(shape input)
		(at 69.85 36.83 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 58.8821 36.83 0)
		)
	)
	(global_label "SCL"
		(shape input)
		(at 38.1 78.74 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 44.5928 78.74 0)
		)
	)
	(global_label "SCK"
		(shape input)
		(at 105.41 45.72 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 98.6753 45.72 0)
		)
	)
	(global_label "SCL"
		(shape input)
		(at 69.85 49.53 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 63.3572 49.53 0)
		)
	)
	(global_label "TX"
		(shape input)
		(at 69.85 52.07 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 64.6877 52.07 0)
		)
	)
	(global_label "T_SENSE"
		(shape input)
		(at 39.37 116.84 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 50.3379 116.84 0)
		)
	)
	(global_label "CS"
		(shape input)
		(at 69.85 44.45 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 64.3853 44.45 0)
		)
	)
	(global_label "SCL"
		(shape input)
		(at 38.1 39.37 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 44.5928 39.37 0)
		)
	)
	(global_label "SDA"
		(shape input)
		(at 55.88 99.06 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 49.3267 99.06 0)
		)
	)
	(global_label "RX"
		(shape input)
		(at 69.85 54.61 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 64.3853 54.61 0)
		)
	)
	(global_label "MOSI"
		(shape input)
		(at 69.85 62.23 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 62.2686 62.23 0)
		)
	)
	(global_label "SDA"
		(shape input)
		(at 87.63 93.98 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 81.0767 93.98 0)
		)
	)
	(global_label "MISO"
		(shape input)
		(at 69.85 59.69 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 62.2686 59.69 0)
		)
	)
	(global_label "CS"
		(shape input)
		(at 105.41 58.42 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 99.9453 58.42 0)
		)
	)
	(global_label "SDA"
		(shape input)
		(at 38.1 81.28 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 44.6533 81.28 0)
		)
	)
	(global_label "MISO"
		(shape input)
		(at 104.14 50.8 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 96.5586 50.8 0)
		)
	)
	(global_label "SCL"
		(shape input)
		(at 87.63 91.44 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 81.1372 91.44 0)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_1x08_P2.54mm_Horizontal_SMD")
		(at 33.02 78.74 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J3"
			(at 33.02 66.04 0)
		)
		(property "Value" "Headers for GPS"
			(at 29.21 78.74 90)
		)
		(property "Footprint" "fab:PinHeader_1x08_P2.54mm_Horizontal_SMD"
			(at 33.02 78.74 0)
		)
		(property "Datasheet" "~"
			(at 33.02 78.74 0)
		)
		(property "Description" "Male connector, single row"
			(at 33.02 78.74 0)
		)
		(pin "8")
		(pin "6")
		(pin "3")
		(pin "1")
		(pin "7")
		(pin "5")
		(pin "4")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "J3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_GND")
		(at 38.1 76.2 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR05"
			(at 44.45 76.2 0)
		)
		(property "Value" "PWR_GND"
			(at 41.91 76.1999 90)
		)
		(property "Footprint" ""
			(at 38.1 76.2 0)
		)
		(property "Datasheet" ""
			(at 38.1 76.2 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 38.1 76.2 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_3V3")
		(at 55.88 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR014"
			(at 55.88 92.71 0)
		)
		(property "Value" "PWR_3V3"
			(at 55.88 83.82 0)
		)
		(property "Footprint" ""
			(at 55.88 88.9 0)
		)
		(property "Datasheet" ""
			(at 55.88 88.9 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3V3\""
			(at 55.88 88.9 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR014")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_3V3")
		(at 92.71 81.28 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR010"
			(at 92.71 85.09 0)
		)
		(property "Value" "PWR_3V3"
			(at 92.71 76.2 0)
		)
		(property "Footprint" ""
			(at 92.71 81.28 0)
		)
		(property "Datasheet" ""
			(at 92.71 81.28 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3V3\""
			(at 92.71 81.28 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR010")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:R_1206")
		(at 55.88 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 58.42 92.7099 0)
		)
		(property "Value" "4.99k"
			(at 58.42 95.2499 0)
		)
		(property "Footprint" "fab:R_1206"
			(at 55.88 93.98 90)
		)
		(property "Datasheet" "~"
			(at 55.88 93.98 0)
		)
		(property "Description" "Resistor"
			(at 55.88 93.98 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "starpcb"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_3V3")
		(at 80.01 31.75 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR08"
			(at 80.01 35.56 0)
		)
		(property "Value" "PWR_3V3"
			(at 80.01 26.67 0)
		)
		(property "Footprint" ""
			(at 80.01 31.75 0)
		)
		(property "Datasheet" ""
			(at 80.01 31.75 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3V3\""
			(at 80.01 31.75 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR08")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_GND")
		(at 38.1 36.83 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 44.45 36.83 0)
		)
		(property "Value" "PWR_GND"
			(at 41.91 36.8299 90)
		)
		(property "Footprint" ""
			(at 38.1 36.83 0)
		)
		(property "Datasheet" ""
			(at 38.1 36.83 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 38.1 36.83 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_1x01_P2.54mm_Vertical_THT_D1.4mm")
		(at 140.97 101.6 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J5"
			(at 140.97 96.52 0)
		)
		(property "Value" "Conn_PinHeader_1x01_P2.54mm_Vertical_THT_D1.4mm"
			(at 140.97 99.06 0)
		)
		(property "Footprint" "fab:PinHeader_1x01_P2.54mm_Vertical_THT_D2mm"
			(at 140.97 101.6 0)
		)
		(property "Datasheet" "~"
			(at 140.97 101.6 0)
		)
		(property "Description" "Connector pin header 2.54mm pitch vertical tht"
			(at 140.97 101.6 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "J5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:R_1206")
		(at 33.02 110.49 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 35.56 109.2199 0)
		)
		(property "Value" "10k"
			(at 35.56 111.7599 0)
		)
		(property "Footprint" "fab:R_1206"
			(at 33.02 110.49 90)
		)
		(property "Datasheet" "~"
			(at 33.02 110.49 0)
		)
		(property "Description" "Resistor"
			(at 33.02 110.49 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_3V3")
		(at 123.19 30.48 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR09"
			(at 123.19 34.29 0)
		)
		(property "Value" "PWR_3V3"
			(at 123.19 25.4 0)
		)
		(property "Footprint" ""
			(at 123.19 30.48 0)
		)
		(property "Datasheet" ""
			(at 123.19 30.48 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3V3\""
			(at 123.19 30.48 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR09")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_GND")
		(at 33.02 129.54 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR012"
			(at 33.02 135.89 0)
		)
		(property "Value" "PWR_GND"
			(at 35.814 133.858 0)
		)
		(property "Footprint" ""
			(at 33.02 129.54 0)
		)
		(property "Datasheet" ""
			(at 33.02 129.54 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 33.02 129.54 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR012")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_GND")
		(at 100.33 106.68 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR03"
			(at 100.33 113.03 0)
		)
		(property "Value" "PWR_GND"
			(at 103.124 110.998 0)
		)
		(property "Footprint" ""
			(at 100.33 106.68 0)
		)
		(property "Datasheet" ""
			(at 100.33 106.68 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 100.33 106.68 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_GND")
		(at 95.25 106.68 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR011"
			(at 95.25 113.03 0)
		)
		(property "Value" "PWR_GND"
			(at 91.186 110.744 0)
		)
		(property "Footprint" ""
			(at 95.25 106.68 0)
		)
		(property "Datasheet" ""
			(at 95.25 106.68 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 95.25 106.68 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR011")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Thermistor_NTC")
		(at 33.02 123.19 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "TH1"
			(at 35.56 122.2374 0)
		)
		(property "Value" "Thermistor_NTC"
			(at 35.56 124.7774 0)
		)
		(property "Footprint" "fab:R_1206"
			(at 33.02 123.19 0)
		)
		(property "Datasheet" "https://www.mouser.fi/datasheet/2/18/AAS-920-324F-Thermometrics-NTC-SMD-032717-web-1018802.pdf"
			(at 33.02 123.19 0)
		)
		(property "Description" "Temperature dependent resistor, Amphenol NHQ103B375T10, negative temperature coefficient, NTC Thermistor 10k 1206 (3216 Metric)"
			(at 33.02 123.19 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "TH1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_3V3")
		(at 33.02 104.14 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR013"
			(at 33.02 107.95 0)
		)
		(property "Value" "PWR_3V3"
			(at 33.02 99.06 0)
		)
		(property "Footprint" ""
			(at 33.02 104.14 0)
		)
		(property "Datasheet" ""
			(at 33.02 104.14 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3V3\""
			(at 33.02 104.14 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR013")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_GND")
		(at 123.19 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 123.19 72.39 0)
		)
		(property "Value" "PWR_GND"
			(at 123.19 71.12 0)
		)
		(property "Footprint" ""
			(at 123.19 66.04 0)
		)
		(property "Datasheet" ""
			(at 123.19 66.04 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 123.19 66.04 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_3V3")
		(at 38.1 71.12 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 34.29 71.12 0)
		)
		(property "Value" "PWR_3V3"
			(at 41.91 71.1199 90)
		)
		(property "Footprint" ""
			(at 38.1 71.12 0)
		)
		(property "Datasheet" ""
			(at 38.1 71.12 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3V3\""
			(at 38.1 71.12 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_3V3")
		(at 68.58 88.9 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR015"
			(at 68.58 92.71 0)
		)
		(property "Value" "PWR_3V3"
			(at 68.58 83.82 0)
		)
		(property "Footprint" ""
			(at 68.58 88.9 0)
		)
		(property "Datasheet" ""
			(at 68.58 88.9 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3V3\""
			(at 68.58 88.9 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR015")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Module_XIAO-RP2040")
		(at 82.55 49.53 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "M1"
			(at 81.026 22.352 0)
		)
		(property "Value" "Module_XIAO-RP2040"
			(at 82.55 19.812 0)
		)
		(property "Footprint" "fab:SeeedStudio_XIAO_RP2040"
			(at 82.55 49.53 0)
		)
		(property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/"
			(at 82.55 49.53 0)
		)
		(property "Description" "RP2040 XIAO RP2040 - ARM® Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board"
			(at 82.55 49.53 0)
		)
		(pin "13")
		(pin "12")
		(pin "10")
		(pin "4")
		(pin "5")
		(pin "9")
		(pin "14")
		(pin "3")
		(pin "6")
		(pin "2")
		(pin "20")
		(pin "8")
		(pin "15")
		(pin "18")
		(pin "16")
		(pin "17")
		(pin "11")
		(pin "19")
		(pin "7")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "M1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Micro_SD_Socket")
		(at 123.19 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J2"
			(at 146.05 52.1014 0)
		)
		(property "Value" "Micro_SD_Socket"
			(at 146.05 54.6414 0)
		)
		(property "Footprint" "fab:MicroSD_Amphenol_114-00841-68"
			(at 123.19 48.26 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/opa188.pdf"
			(at 123.19 48.26 0)
		)
		(property "Description" "Zero-Drift, Precision, Low-Noise, Rail-to-Rail Output, 36-V Operational Amplifier, TSOT-23-5"
			(at 123.19 48.26 0)
		)
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(pin "3")
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_GND")
		(at 80.01 67.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 80.01 73.66 0)
		)
		(property "Value" "PWR_GND"
			(at 80.01 72.39 0)
		)
		(property "Footprint" ""
			(at 80.01 67.31 0)
		)
		(property "Datasheet" ""
			(at 80.01 67.31 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 80.01 67.31 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_1x08_P2.54mm_Horizontal_SMD")
		(at 33.02 41.91 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J1"
			(at 33.02 29.21 0)
		)
		(property "Value" "MPU-6050_1x08_P2.54mm"
			(at 29.21 41.656 90)
		)
		(property "Footprint" "fab:PinHeader_1x08_P2.54mm_Horizontal_SMD"
			(at 33.02 41.91 0)
		)
		(property "Datasheet" "~"
			(at 33.02 41.91 0)
		)
		(property "Description" "Male connector, single row"
			(at 33.02 41.91 0)
		)
		(pin "8")
		(pin "4")
		(pin "1")
		(pin "3")
		(pin "2")
		(pin "7")
		(pin "5")
		(pin "6")
		(instances
			(project ""
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_3V3")
		(at 38.1 34.29 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR07"
			(at 34.29 34.29 0)
		)
		(property "Value" "PWR_3V3"
			(at 41.91 34.2899 90)
		)
		(property "Footprint" ""
			(at 38.1 34.29 0)
		)
		(property "Datasheet" ""
			(at 38.1 34.29 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+3V3\""
			(at 38.1 34.29 0)
		)
		(pin "1")
		(instances
			(project "starpcb"
				(path
					(reference "#PWR07")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:R_1206")
		(at 68.58 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 71.12 92.7099 0)
		)
		(property "Value" "4.99k"
			(at 71.12 95.2499 0)
		)
		(property "Footprint" "fab:R_1206"
			(at 68.58 93.98 90)
		)
		(property "Datasheet" "~"
			(at 68.58 93.98 0)
		)
		(property "Description" "Resistor"
			(at 68.58 93.98 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "starpcb"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Sensor:MAX30102")
		(at 97.79 93.98 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "U2"
			(at 97.282 114.554 0)
		)
		(property "Value" "HR Sensor MAX30102"
			(at 97.028 116.332 0)
		)
		(property "Footprint" "OptoDevice:Maxim_OLGA-14_3.3x5.6mm_P0.8mm"
			(at 97.79 96.52 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX30102.pdf"
			(at 97.79 93.98 0)
		)
		(property "Description" "Heart Rate Sensor, 14-OLGA"
			(at 97.79 93.98 0)
		)
		(pin "1")
		(pin "6")
		(pin "2")
		(pin "10")
		(pin "11")
		(pin "13")
		(pin "5")
		(pin "14")
		(pin "8")
		(pin "9")
		(pin "3")
		(pin "4")
		(pin "7")
		(pin "12")
		(instances
			(project ""
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
)
