(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Digistump ATtiny-backups/")
		)
	)
	(net 0 "")
	(net 1 "+5V")
	(net 2 "GND")
	(net 3 "Net-(D1-Pad2)")
	(net 4 "Net-(D2-Pad1)")
	(net 5 "Net-(D3-Pad1)")
	(net 6 "Net-(J1-Pad1)")
	(net 7 "Net-(J1-Pad2)")
	(net 8 "Net-(J1-Pad3)")
	(net 9 "Net-(J2-Pad1)")
	(net 10 "Net-(J2-Pad2)")
	(net 11 "Net-(J2-Pad3)")
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 128.407 145.287 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D3"
			(at 3.049 -0.117 0)
			(layer "F.SilkS")
		)
		(property "Value" "3V6"
			(at 0 2.1 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Digistump ATtiny.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D3-Pad1)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "!My_Custom_Library:USB-A-PCB"
		(layer "F.Cu")
		(at 116.332 144.018)
		(property "Reference" "U2"
			(at -8.25 -7.75 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "USB-PCB"
			(at 4.5 -7.75 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Digistump ATtiny.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at 0 3.75)
			(size 7 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+5V")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at 0 1)
			(size 6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(D2-Pad1)")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at 0 -1)
			(size 6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(D3-Pad1)")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at 0 -3.75)
			(size 7 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 147.955 146.436 90)
		(descr "LED, diameter 3.0mm, 2 pins")
		(tags "LED diameter 3.0mm 2 pins")
		(property "Reference" "D1"
			(at -2.281 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at -2.027 0 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Digistump ATtiny.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D1-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 128.905 140.589 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 1.651 2.032 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k5"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Digistump ATtiny.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 4 "Net-(D2-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 1 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 132.461 142.875)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "68R"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Digistump ATtiny.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 5 "Net-(D3-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 8 "Net-(J1-Pad3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 132.207 145.415)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at -0.227064 2.032 0)
			(layer "F.SilkS")
		)
		(property "Value" "68R"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Digistump ATtiny.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 4 "Net-(D2-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 7 "Net-(J1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8W_5.3x5.3mm_P1.27mm"
		(layer "F.Cu")
		(at 139.573 144.145)
		(descr "8-Lead Plastic Small Outline (SM) - 5.28 mm Body [SOIC] (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "U1"
			(at -0.127 -1.524 0)
			(layer "F.SilkS")
		)
		(property "Value" "ATtiny85"
			(at 0 3.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Digistump ATtiny.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.65 -1.905)
			(size 1.7 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(J1-Pad1)")
			(pinfunction "~{RESET}/PB5")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -3.65 -0.635)
			(size 1.7 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(J1-Pad2)")
			(pinfunction "XTAL1/PB3")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -3.65 0.635)
			(size 1.7 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(J1-Pad3)")
			(pinfunction "XTAL2/PB4")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -3.65 1.905)
			(size 1.7 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 3.65 1.905)
			(size 1.7 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(J2-Pad1)")
			(pinfunction "AREF/PB0")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at 3.65 0.635)
			(size 1.7 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(J2-Pad2)")
			(pinfunction "PB1")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at 3.65 -0.635)
			(size 1.7 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(J2-Pad3)")
			(pinfunction "PB2")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at 3.65 -1.905)
			(size 1.7 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8W_5.3x5.3mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 135.89 147.828 90)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "REF**"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "DIP-8_W7.62mm"
			(at 3.81 9.95 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "8" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 125.105 146.811 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D2"
			(at 0.001 2.042 270)
			(layer "F.SilkS")
		)
		(property "Value" "3V6"
			(at 0 2.1 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Digistump ATtiny.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(D2-Pad1)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 147.955 141.351 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at -0.254 2.032 0)
			(layer "F.SilkS")
		)
		(property "Value" "330R"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Digistump ATtiny.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 1.9144 -0.762 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 3 "Net-(D1-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2083333333)
			(net 10 "Net-(J2-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 125.095 140.97 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at -0.508 1.915 270)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.85 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "Digistump ATtiny.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1886792453)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1886792453)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 112.414 138.049)
		(end 150.222 150.049)
		(fill no)
		(layer "Edge.Cuts")
	)
	(embedded_fonts no)
)
