(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber/")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-A)")
	(net 2 "/DBG1")
	(net 3 "Net-(D2-A)")
	(net 4 "/DBG2")
	(net 5 "Net-(D3-A)")
	(net 6 "/DBG3")
	(net 7 "/SCL")
	(net 8 "/SDA")
	(net 9 "GND")
	(net 10 "/V_MTR")
	(net 11 "unconnected-(M1-SWCLK-Pad20)")
	(net 12 "Net-(D4-A)")
	(net 13 "Net-(D5-A)")
	(net 14 "unconnected-(M1-SWDIO-Pad17)")
	(net 15 "Net-(J2-Pin_1)")
	(net 16 "unconnected-(M1-RESET-Pad18)")
	(net 17 "Net-(J3-Pin_2)")
	(net 18 "Net-(J3-Pin_1)")
	(net 19 "Net-(J4-Pin_2)")
	(net 20 "Net-(J4-Pin_1)")
	(net 21 "Net-(M1-D6)")
	(net 22 "Net-(M1-D7)")
	(net 23 "Net-(M1-D8)")
	(net 24 "Net-(M1-D9)")
	(net 25 "Net-(D6-A)")
	(net 26 "Net-(M1-D10)")
	(net 27 "Net-(M1-D3)")
	(net 28 "Net-(Q1-G)")
	(net 29 "Net-(U1-RS)")
	(net 30 "Net-(U2-RS)")
	(net 31 "Net-(SW1-B)")
	(net 32 "5V")
	(net 33 "3V3")
	(footprint "fab:Button_CnK_PTS636.0_6x3.5mm"
		(layer "F.Cu")
		(at 119.8 95.6)
		(descr "Light Touch Switch")
		(tags "button btn switch touch")
		(property "Reference" "SW2"
			(at 0 -2.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "Switch_Tactile_CnK"
			(at 0 3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ckswitches.com/media/2779/pts636.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, C&K PTS636 SM25F SMTR LFS, Tactile Switch SPST-NO Top Actuated Surface Mount"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Button?CnK*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4 0)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(M1-D9)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4 0)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Switch_CnK-PTS636SM25FSMTR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:LED_1206"
		(layer "F.Cu")
		(at 98.5 72 90)
		(descr "LED SMD 1206, hand soldering")
		(tags "LED 1206")
		(property "Reference" "D5"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "GREEN"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LED*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.8 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 90)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 90)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/LED-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 96 77.5)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R9"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(SW1-B)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:R_2010"
		(layer "F.Cu")
		(at 107 84.5 90)
		(descr "Resistor SMD 2010, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 2010")
		(property "Reference" "R4"
			(at -0.01 -2.55 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.25"
			(at 0.01 2.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Motor driver sense resistor generic"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*2010*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.5 0 90)
			(size 1.6 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(U1-RS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.5 0 90)
			(size 1.6 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-2010.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 135 90 -90)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R11"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(M1-D10)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 103 77.5 180)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R8"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "100K"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:TerminalBlock_OnShore_1x02_P3.50mm_Horizontal"
		(layer "F.Cu")
		(at 107 95.45)
		(descr "2 Position Wire to Board Terminal Block Horizontal with Board 0.138\" (3.50mm) Through Hole")
		(tags "THT Terminal Block pitch 3.5mm")
		(property "Reference" "J3"
			(at 2 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "OUT2"
			(at 1.7 5.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "www.on-shore.com/wp-content/uploads/ED555XDS.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TERM BLK 2POS SIDE ENT 3.5MM PCB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TerminalBlock*1x02*P3.50mm*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.75 2.9 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 93.75 95.45)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" thru_hole circle
			(at 0 -0.45)
			(size 3.3 3.3)
			(drill 3.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "fab:TerminalBlock_OnShore_1x02_P3.50mm_Horizontal"
		(layer "F.Cu")
		(at 85.5 95)
		(descr "2 Position Wire to Board Terminal Block Horizontal with Board 0.138\" (3.50mm) Through Hole")
		(tags "THT Terminal Block pitch 3.5mm")
		(property "Reference" "J2"
			(at 1.9 -3.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "V_MTR"
			(at 1.7 5.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "www.on-shore.com/wp-content/uploads/ED555XDS.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TERM BLK 2POS SIDE ENT 3.5MM PCB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TerminalBlock*1x02*P3.50mm*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.75 2.9 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 95.55 61.75 -90)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R7"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/SDA")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(D5-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:R_2010"
		(layer "F.Cu")
		(at 129 87)
		(descr "Resistor SMD 2010, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 2010")
		(property "Reference" "R5"
			(at -0.01 -2.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.25"
			(at 0.01 2.72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Motor driver sense resistor generic"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*2010*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.35 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.5 0)
			(size 1.6 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Net-(U2-RS)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.5 0)
			(size 1.6 2.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-2010.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:PinHeader_01x04_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 88.55 59.95)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "DISPLAY"
			(at 3.45 9.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x04*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.45 4.33 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/SDA")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "5V")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/PinHeader-01x04_P2.54mm_Vertical_THT.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:LED_1206"
		(layer "F.Cu")
		(at 142.6 68.1 90)
		(descr "LED SMD 1206, hand soldering")
		(tags "LED 1206")
		(property "Reference" "D6"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "RED"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LED*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.8 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 90)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 90)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/LED-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:SeeedStudio_XIAO_RP2040"
		(layer "F.Cu")
		(at 127.725 68.61)
		(descr "Footprint for Seeed Studio XIAO modules")
		(tags "xiao seeed studio module")
		(property "Reference" "M1"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "XIAO-RP2040"
			(at 0.005 1.27 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RP2040 XIAO RP2040 - ARM® Dual-Core Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SeeedStudio?XIAO?RP2040*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr through_hole)
		(fp_text user "SWDIO"
			(at 0 -8.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "RESET"
			(at 0 -5.96 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 2.54 -5.96 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "VIN"
			(at -2.535 8.89 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SWCLK"
			(at 2.54 -8.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 2.545 8.89 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0.0025 3.81 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -7.615 -7.62)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/DBG1")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -7.615 -5.08)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/DBG2")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -7.615 -2.54)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/DBG3")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -7.615 0)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(M1-D3)")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -7.615 2.54)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/SDA")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -7.615 5.08)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/SCL")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -7.615 7.62)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(M1-D6)")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at 7.62 7.62)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(M1-D7)")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at 7.62 5.08)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(M1-D8)")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 7.62 2.54)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(M1-D9)")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at 7.62 0)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(M1-D10)")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at 7.62 -2.54)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "3V3")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 7.62 -5.08)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 7.62 -7.62)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "5V")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at 1.275 8.89 270)
			(size 2.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -1.265 8.89 270)
			(size 2.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "5V")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "17" smd circle
			(at -1.27 -8.5)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(M1-SWDIO-Pad17)")
			(pinfunction "SWDIO")
			(pintype "bidirectional+no_connect")
		)
		(pad "18" smd circle
			(at -1.27 -5.96)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(M1-RESET-Pad18)")
			(pinfunction "RESET")
			(pintype "input+no_connect")
		)
		(pad "19" smd circle
			(at 1.27 -5.96)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "20" smd circle
			(at 1.27 -8.5)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(M1-SWCLK-Pad20)")
			(pinfunction "SWCLK")
			(pintype "input+no_connect")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Mask" "F.Paste" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 122.525 58.06) (xy 123.925 58.06) (xy 123.925 60.11) (xy 122.525 60.11)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Mask" "F.Paste" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 122.525 62.11) (xy 123.925 62.11) (xy 123.925 64.31) (xy 122.525 64.31)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Mask" "F.Paste" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 131.525 58.06) (xy 132.925 58.06) (xy 132.925 60.11) (xy 131.525 60.11)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Mask" "F.Paste" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 131.525 62.11) (xy 132.925 62.11) (xy 132.925 64.31) (xy 131.525 64.31)
				)
			)
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Seeed_XIAO-nRF52840_Sense.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 180)
			)
		)
	)
	(footprint "fab:HSOP-8"
		(layer "F.Cu")
		(at 121.595 85.1 -90)
		(descr "HSOP-8")
		(tags "hsop-8 smd")
		(property "Reference" "U2"
			(at 0 -3.6 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Motor2"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/TB67H451FNG_datasheet_en_20201126.pdf?did=68598&prodName=TB67H451FNG"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50V/3A BRUSHED MOTOR DRIVER Toshiba TB67H451FNG,EL"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*HSOP?8*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.9 -1.905 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -2.9 -0.635 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(M1-D8)")
			(pinfunction "IN2")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -2.9 0.635 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(M1-D7)")
			(pinfunction "IN1")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.9 1.905 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "3V3")
			(pinfunction "VREF")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 2.9 1.905 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/V_MTR")
			(pinfunction "VM")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 2.9 0.635 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(J3-Pin_1)")
			(pinfunction "OUT1")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 2.9 -0.635 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Net-(U2-RS)")
			(pinfunction "RS")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 2.9 -1.905 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(J3-Pin_2)")
			(pinfunction "OUT2")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 0 0 270)
			(size 2.7 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pinfunction "PAD")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "fab:TerminalBlock_OnShore_1x02_P3.50mm_Horizontal"
		(layer "F.Cu")
		(at 98.5 95.45)
		(descr "2 Position Wire to Board Terminal Block Horizontal with Board 0.138\" (3.50mm) Through Hole")
		(tags "THT Terminal Block pitch 3.5mm")
		(property "Reference" "J4"
			(at 1.9 -3.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "OUT1"
			(at 1.7 5.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "www.on-shore.com/wp-content/uploads/ED555XDS.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TERM BLK 2POS SIDE ENT 3.5MM PCB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TerminalBlock*1x02*P3.50mm*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.75 2.9 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J4-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0)
			(size 3 3)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J4-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x02_P3.50mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 141.4 62.9)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R12"
			(at 1 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(D6-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:MountingHole_M3"
		(layer "F.Cu")
		(at 140.4 58.1)
		(property "Reference" "REF**"
			(at 0 3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_M3"
			(at 0 -3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "M3"
			(at -2.9 -1.9 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "M3"
			(at 2.2 -1.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" thru_hole circle
			(at 0.1 0)
			(size 3.3 3.3)
			(drill 3.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "fab:CP_Elec_100uF_Panasonic_EEE-FN1E101UL"
		(layer "F.Cu")
		(at 100 85 -90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 10.0x10.0mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C1"
			(at -5 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 4.3 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://api.pim.na.industrial.panasonic.com/file_stream/main/fileversion/19782"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, SMD, radial"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CP*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.6 0 270)
			(size 3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/V_MTR")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.6 0 270)
			(size 3 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Capacitor_Panasonic-EEE-FN1E101UL.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:LED_1206"
		(layer "F.Cu")
		(at 109 66 180)
		(descr "LED SMD 1206, hand soldering")
		(tags "LED 1206")
		(property "Reference" "D3"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "BLUE"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LED*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.8 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/DBG3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/LED-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:MountingHole_M3"
		(layer "F.Cu")
		(at 140 95)
		(property "Reference" "REF**"
			(at 0 3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_M3"
			(at 0 -3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "M3"
			(at -1 3.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "M3"
			(at 2.2 -1.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" thru_hole circle
			(at 0.5 0)
			(size 3.3 3.3)
			(drill 3.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "fab:LED_1206"
		(layer "F.Cu")
		(at 95 72 90)
		(descr "LED SMD 1206, hand soldering")
		(tags "LED 1206")
		(property "Reference" "D4"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "GREEN"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LED*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.8 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 90)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 90)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/LED-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 102.5 66)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R3"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -3.275 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "3V3")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D3-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:PinHeader_01x03_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 115 60.46)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J5"
			(at -0.5 -1.96 0)
			(layer "F.SilkS")
		)
		(property "Value" "DEBUG"
			(at 0 8.1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x03*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.3 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/DBG1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/DBG2")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/DBG3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/PinHeader-01x03_P2.54mm_Vertical_THT.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:SOT-23-3"
		(layer "F.Cu")
		(at 92.3 84.5)
		(descr "SOT-23-3, Standard")
		(tags "SOT-23-3")
		(property "Reference" "Q1"
			(at 0 -2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "SQ2351ES-T1_BE3"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NDS356AP-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "P-Channel mosfet NDS356AP in SOT-23 package"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SOT?23*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.2 -0.95)
			(size 1 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.2 0.95)
			(size 1 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(J2-Pin_1)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.2 0)
			(size 1 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/V_MTR")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:LED_1206"
		(layer "F.Cu")
		(at 108.7 62.5 180)
		(descr "LED SMD 1206, hand soldering")
		(tags "LED 1206")
		(property "Reference" "D2"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "BLUE"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LED*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.8 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/DBG2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/LED-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 135 84 90)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R10"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 90)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 90)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(M1-D9)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 92.5 66.5 -90)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R6"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 270)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/SCL")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 270)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(D4-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:Switch_Slide_Top_CnK_JS102011SCQN_8.5x3.5mm"
		(layer "F.Cu")
		(at 87.25 79 90)
		(descr "https://www.ckswitches.com/media/1422/js.pdf")
		(tags "switch slide top spdt smd JS102011SCQN")
		(property "Reference" "SW1"
			(at 0.01 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "Switch_Slide_Top_CnK"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ckswitches.com/media/1422/js.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Slide Switch SPDT Surface Mount"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Switch*CnK?JS102011JCQN*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -3 -3.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.5 2.75 90)
			(size 1 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2.75 90)
			(size 1 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(SW1-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.5 2.75 90)
			(size 1 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "5V")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Switch_CnK-JS102011SCQN.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 102.5 62.5)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R2"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "3V3")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(D2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:LED_1206"
		(layer "F.Cu")
		(at 108.5 59 180)
		(descr "LED SMD 1206, hand soldering")
		(tags "LED 1206")
		(property "Reference" "D1"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "BLUE"
			(at -1 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LED*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.8 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/DBG1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/LED-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:HSOP-8"
		(layer "F.Cu")
		(at 113.095 85.1 -90)
		(descr "HSOP-8")
		(tags "hsop-8 smd")
		(property "Reference" "U1"
			(at 0 -3.6 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Motor1"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/TB67H451FNG_datasheet_en_20201126.pdf?did=68598&prodName=TB67H451FNG"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50V/3A BRUSHED MOTOR DRIVER Toshiba TB67H451FNG,EL"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*HSOP?8*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.9 -1.905 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at -2.9 -0.635 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(M1-D6)")
			(pinfunction "IN2")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -2.9 0.635 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(M1-D3)")
			(pinfunction "IN1")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.9 1.905 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "3V3")
			(pinfunction "VREF")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 2.9 1.905 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/V_MTR")
			(pinfunction "VM")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 2.9 0.635 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(J4-Pin_1)")
			(pinfunction "OUT1")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 2.9 -0.635 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(U1-RS)")
			(pinfunction "RS")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 2.9 -1.905 270)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(J4-Pin_2)")
			(pinfunction "OUT2")
			(pintype "output")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 0 0 270)
			(size 2.7 2.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "GND")
			(pinfunction "PAD")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 102.5 59)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R1"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at -5 2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.5 5 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "3V3")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:Button_CnK_PTS636.0_6x3.5mm"
		(layer "F.Cu")
		(at 131.5 95.5 180)
		(descr "Light Touch Switch")
		(tags "button btn switch touch")
		(property "Reference" "SW3"
			(at 0 -2.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "Switch_Tactile_CnK"
			(at 0 3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ckswitches.com/media/2779/pts636.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, C&K PTS636 SM25F SMTR LFS, Tactile Switch SPST-NO Top Actuated Surface Mount"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Button?CnK*")
		(sheetname "/")
		(sheetfile "HTMAA.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.8 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4 0 180)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(M1-D10)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 4 0 180)
			(size 2.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Switch_CnK-PTS636SM25FSMTR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 82.4 58.2)
		(mid 83.27868 56.07868)
		(end 85.4 55.2)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 141.27868 55.2)
		(mid 143.4 56.07868)
		(end 144.27868 58.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.4 96.5)
		(end 82.4 58.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.27868 99.5)
		(end 85.4 99.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.4 55.2)
		(end 141.2787 55.2)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 85.4 99.5)
		(mid 83.27868 98.62132)
		(end 82.4 96.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.27868 58.2)
		(end 144.27868 96.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.27868 96.5)
		(mid 143.4 98.62132)
		(end 141.27868 99.5)
		(layer "Edge.Cuts")
	)
	(gr_text "${REFERENCE}"
		(at 124.1 50.32 90)
		(layer "F.Fab")
	)
	(dimension
		(type orthogonal)
		(layer "F.Cu")
		(pts
			(xy 85.4 55.2) (xy 85.4 99.5)
		)
		(height -19.9)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "44.3"
			(at 63.7 77.35 90)
			(layer "F.Cu")
		)
	)
	(dimension
		(type orthogonal)
		(layer "F.Cu")
		(pts
			(xy 82.4 96.5) (xy 145.3 97.3)
		)
		(height 15.6)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "62.9"
			(at 113.85 110.3 0)
			(layer "F.Cu")
		)
	)
	(zone
		(net 9)
		(net_name "GND")
		(layer "F.Cu")
		(name "GND")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 81.9 53.3) (xy 80.6 101.8) (xy 148 101.3) (xy 148 53.2)
			)
		)
	)
	(embedded_fonts no)
)
