(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "fab:LED_1206"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED_1206"
				(at 0 -2.54 0)
			)
			(property "Footprint" "fab:LED_1206"
				(at 0 0 0)
			)
			(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode 1206 SML-LX1206IC-TR SML-LX1206GC-TR 5988230107F 150120BS75000 QBLP650-IW HIR11-21C/L11/TR8"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*LED*1206*"
				(at 0 0 0)
			)
			(symbol "LED_1206_0_1"
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1206_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:Module_XIAO-ESP32C3"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "M"
				(at -10.16 16.51 0)
			)
			(property "Value" "Module_XIAO-ESP32C3"
				(at 3.81 16.51 0)
			)
			(property "Footprint" "fab:SeeedStudio_XIAO_ESP32C3"
				(at 0 0 0)
			)
			(property "Datasheet" "https://wiki.seeedstudio.com/XIAO_ESP32C3_Getting_Started/"
				(at -2.54 0 0)
			)
			(property "Description" "ESP32-C3 Transceiver; 802.11 a/b/g/n (Wi-Fi, WiFi, WLAN), Bluetooth® Smart 4.x Low Energy (BLE) 2.4GHz Evaluation Board"
				(at 0 0 0)
			)
			(property "ki_keywords" "SEEED STUDIO XIAO ESP32C3 WIFI+B 113991054"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*SeeedStudio?XIAO?ESP32C*"
				(at 0 0 0)
			)
			(symbol "Module_XIAO-ESP32C3_1_1"
				(rectangle
					(start -10.16 15.24)
					(end 10.16 -15.24)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -12.7 12.7 0)
					(length 2.54)
					(name "D0")
					(number "1")
				)
				(pin bidirectional line
					(at -12.7 10.16 0)
					(length 2.54)
					(name "D1")
					(number "2")
				)
				(pin bidirectional line
					(at -12.7 7.62 0)
					(length 2.54)
					(name "D2")
					(number "3")
				)
				(pin bidirectional line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "D3")
					(number "4")
				)
				(pin bidirectional line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "D4")
					(number "5")
				)
				(pin bidirectional line
					(at -12.7 0 0)
					(length 2.54)
					(name "D5")
					(number "6")
				)
				(pin bidirectional line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "D6")
					(number "7")
				)
				(pin bidirectional line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "D7")
					(number "8")
				)
				(pin bidirectional line
					(at -12.7 -7.62 0)
					(length 2.54)
					(name "D8")
					(number "9")
				)
				(pin bidirectional line
					(at -12.7 -10.16 0)
					(length 2.54)
					(name "D9")
					(number "10")
				)
				(pin bidirectional line
					(at -12.7 -12.7 0)
					(length 2.54)
					(name "D10")
					(number "11")
				)
				(pin power_in line
					(at -2.54 17.78 270)
					(length 2.54)
					(name "3V3")
					(number "12")
				)
				(pin power_in line
					(at -2.54 -17.78 90)
					(length 2.54)
					(name "BAT_GND")
					(number "15")
				)
				(pin power_in line
					(at 0 17.78 270)
					(length 2.54)
					(name "5V")
					(number "14")
				)
				(pin power_in line
					(at 0 -17.78 90)
					(length 2.54)
					(name "THERMAL")
					(number "23")
				)
				(pin power_in line
					(at 2.54 17.78 270)
					(length 2.54)
					(name "BAT_VIN")
					(number "16")
				)
				(pin power_in line
					(at 2.54 -17.78 90)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin power_in line
					(at 5.08 -17.78 90)
					(length 2.54)
					(name "GND")
					(number "21")
				)
				(pin input line
					(at 12.7 5.08 180)
					(length 2.54)
					(name "EN")
					(number "18")
				)
				(pin input line
					(at 12.7 0 180)
					(length 2.54)
					(name "MTDI")
					(number "17")
				)
				(pin output line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "MTDO")
					(number "22")
				)
				(pin input line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "MTMS")
					(number "19")
				)
				(pin input line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "MTCK")
					(number "20")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:R_1206"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.54 0 90)
			)
			(property "Value" "R_1206"
				(at -2.54 0 90)
			)
			(property "Footprint" "fab:R_1206"
				(at 0 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor RC1206FR-074M99L RC1206FR-07499KL RC1206FR-0749K9L RC1206FR-0749R9L RC1206FR-074R99L ERJ-8BWJR100V RC1206FR-070RL RC1206FR-071RL RC1206FR-0710RL RC1206FR-07100RL RC1206FR-07499RL RC1206FR-071KL RC1206FR-074K99L RC1206FR-0710KL RC1206FR-07100KL RC1206FR-071ML RC1206FR-0710ML PT1206FR-070R1L"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*R*1206*"
				(at 0 0 0)
			)
			(symbol "R_1206_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type background)
					)
				)
			)
			(symbol "R_1206_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:Switch_Slide_Top_CnK"
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 0 4.318 0)
			)
			(property "Value" "Switch_Slide_Top_CnK"
				(at 0 -5.08 0)
			)
			(property "Footprint" "fab:Switch_Slide_Top_CnK_JS102011SCQN_8.5x3.5mm"
				(at 0 0 0)
			)
			(property "Datasheet" "https://www.ckswitches.com/media/1422/js.pdf"
				(at 0 0 0)
			)
			(property "Description" "Slide Switch SPDT Surface Mount"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch single-pole double-throw spdt ON-ON JS102011JCQN JS102011SCQN top smd"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*Switch*CnK?JS102011JCQN*"
				(at 0 0 0)
			)
			(symbol "Switch_Slide_Top_CnK_0_0"
				(circle
					(center -2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 -2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
			)
			(symbol "Switch_Slide_Top_CnK_0_1"
				(polyline
					(pts
						(xy -1.524 0.254) (xy 1.651 2.286)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 2.54)
					(radius 0.508)
					(fill
						(type none)
					)
				)
			)
			(symbol "Switch_Slide_Top_CnK_1_1"
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "B")
					(number "2")
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 2.54)
					(name "C")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:Switch_Tactile_CUIDevices"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 1.905 3.175 0)
			)
			(property "Value" "Switch_Tactile_CUIDevices"
				(at 0 0 0)
			)
			(property "Footprint" "fab:Button_CUIDevices_TS04-66-43-BK-260-SMT_6.0x6.0mm"
				(at 0 0 0)
			)
			(property "Datasheet" "https://www.cuidevices.com/product/resource/ts04.pdf"
				(at 0 0 0)
			)
			(property "Description" "SWITCH TACTILE SPST-NO 0.05A 15V"
				(at 0 0 0)
			)
			(property "ki_keywords" "btn button tactile switch low profile TS04-66-43-BK-260-SMT"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*Button?CUIDevices?TS04?66?43?BK?260*"
				(at 0 0 0)
			)
			(symbol "Switch_Tactile_CUIDevices_0_1"
				(polyline
					(pts
						(xy -2.54 1.27) (xy 2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center -1.905 0)
					(radius 0.635)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 1.905 0)
					(radius 0.635)
					(fill
						(type none)
					)
				)
			)
			(symbol "Switch_Tactile_CUIDevices_1_1"
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin input line
					(at -5.08 0 0)
					(length 2.54)
					(hide yes)
					(name "")
					(number "2")
				)
				(pin input line
					(at 5.08 0 180)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin input line
					(at 5.08 0 180)
					(length 2.54)
					(hide yes)
					(name "")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:Switch_Tactile_Omron"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 1.27 2.54 0)
			)
			(property "Value" "Switch_Tactile_Omron"
				(at 0 -1.524 0)
			)
			(property "Footprint" "fab:Button_Omron_B3SN_6.0x6.0mm"
				(at 0 0 0)
			)
			(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3sn.pdf"
				(at 0 0 0)
			)
			(property "Description" "Push button switch, Omron, B3SN, Sealed Tactile Switch (SMT), SPST-NO Top Actuated Surface Mount"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button button tactile spst single pole single throw B3SN-3112P"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*Button*"
				(at 0 0 0)
			)
			(symbol "Switch_Tactile_Omron_0_1"
				(circle
					(center -2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 3.048)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.27) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GNDREF"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GNDREF"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GNDREF\" , reference supply ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GNDREF_0_1"
				(polyline
					(pts
						(xy -0.635 -1.905) (xy 0.635 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.127 -2.54) (xy 0.127 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GNDREF_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 87.63 57.15)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 157.48 43.18) (xy 157.48 83.82)
		)
	)
	(wire
		(pts
			(xy 106.68 50.8) (xy 111.76 50.8)
		)
	)
	(wire
		(pts
			(xy 121.92 54.61) (xy 127 54.61)
		)
	)
	(wire
		(pts
			(xy 142.24 91.44) (xy 142.24 82.55)
		)
	)
	(wire
		(pts
			(xy 109.22 57.15) (xy 127 57.15)
		)
	)
	(wire
		(pts
			(xy 87.63 52.07) (xy 87.63 57.15)
		)
	)
	(wire
		(pts
			(xy 142.24 91.44) (xy 167.64 91.44)
		)
	)
	(wire
		(pts
			(xy 87.63 57.15) (xy 99.06 57.15)
		)
	)
	(wire
		(pts
			(xy 142.24 43.18) (xy 142.24 46.99)
		)
	)
	(wire
		(pts
			(xy 142.24 43.18) (xy 157.48 43.18)
		)
	)
	(wire
		(pts
			(xy 167.64 73.66) (xy 167.64 91.44)
		)
	)
	(wire
		(pts
			(xy 157.48 83.82) (xy 165.1 83.82)
		)
	)
	(wire
		(pts
			(xy 121.92 50.8) (xy 121.92 54.61)
		)
	)
	(wire
		(pts
			(xy 87.63 50.8) (xy 99.06 50.8)
		)
	)
	(symbol
		(lib_id "fab:Switch_Slide_Top_CnK")
		(at 165.1 78.74 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW2"
			(at 168.91 77.4699 90)
		)
		(property "Value" "Switch_Slide_Top_CnK"
			(at 168.91 80.0099 90)
		)
		(property "Footprint" "fab:Switch_Slide_Top_CnK_JS102011SCQN_8.5x3.5mm"
			(at 165.1 78.74 0)
		)
		(property "Datasheet" "https://www.ckswitches.com/media/1422/js.pdf"
			(at 165.1 78.74 0)
		)
		(property "Description" "Slide Switch SPDT Surface Mount"
			(at 165.1 78.74 0)
		)
		(pin "2")
		(pin "3")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "SW2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:R_1206")
		(at 116.84 50.8 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R2"
			(at 116.84 44.45 90)
		)
		(property "Value" "R_1206"
			(at 116.84 46.99 90)
		)
		(property "Footprint" "fab:R_1206"
			(at 116.84 50.8 90)
		)
		(property "Datasheet" "1002?"
			(at 116.84 50.8 0)
		)
		(property "Description" "Resistor"
			(at 116.84 50.8 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Switch_Tactile_CUIDevices")
		(at 199.39 95.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW3"
			(at 199.39 87.63 0)
		)
		(property "Value" "Switch_Tactile_CUIDevices"
			(at 199.39 90.17 0)
		)
		(property "Footprint" "fab:Button_CUIDevices_TS04-66-43-BK-260-SMT_6.0x6.0mm"
			(at 199.39 95.25 0)
		)
		(property "Datasheet" "https://www.cuidevices.com/product/resource/ts04.pdf"
			(at 199.39 95.25 0)
		)
		(property "Description" "SWITCH TACTILE SPST-NO 0.05A 15V"
			(at 199.39 95.25 0)
		)
		(pin "3")
		(pin "2")
		(pin "1")
		(pin "4")
		(instances
			(project ""
				(path
					(reference "SW3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GNDREF")
		(at 87.63 50.8 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 81.28 50.8 0)
		)
		(property "Value" "GNDREF"
			(at 83.82 50.7999 90)
		)
		(property "Footprint" ""
			(at 87.63 50.8 0)
		)
		(property "Datasheet" ""
			(at 87.63 50.8 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GNDREF\" , reference supply ground"
			(at 87.63 50.8 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Module_XIAO-ESP32C3")
		(at 139.7 64.77 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "M1"
			(at 144.3833 44.45 0)
		)
		(property "Value" "Module_XIAO-ESP32C3"
			(at 144.3833 46.99 0)
		)
		(property "Footprint" "fab:SeeedStudio_XIAO_ESP32C3"
			(at 139.7 64.77 0)
		)
		(property "Datasheet" "https://wiki.seeedstudio.com/XIAO_ESP32C3_Getting_Started/"
			(at 137.16 64.77 0)
		)
		(property "Description" "ESP32-C3 Transceiver; 802.11 a/b/g/n (Wi-Fi, WiFi, WLAN), Bluetooth® Smart 4.x Low Energy (BLE) 2.4GHz Evaluation Board"
			(at 139.7 64.77 0)
		)
		(pin "14")
		(pin "17")
		(pin "22")
		(pin "9")
		(pin "11")
		(pin "12")
		(pin "1")
		(pin "15")
		(pin "10")
		(pin "13")
		(pin "4")
		(pin "20")
		(pin "21")
		(pin "5")
		(pin "3")
		(pin "6")
		(pin "2")
		(pin "7")
		(pin "23")
		(pin "16")
		(pin "8")
		(pin "18")
		(pin "19")
		(instances
			(project ""
				(path
					(reference "M1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GNDREF")
		(at 87.63 57.15 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 81.28 57.15 0)
		)
		(property "Value" "GNDREF"
			(at 83.82 57.1499 90)
		)
		(property "Footprint" ""
			(at 87.63 57.15 0)
		)
		(property "Datasheet" ""
			(at 87.63 57.15 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GNDREF\" , reference supply ground"
			(at 87.63 57.15 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Switch_Tactile_Omron")
		(at 104.14 57.15 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW1"
			(at 105.4101 58.42 90)
		)
		(property "Value" "Switch_Tactile_Omron"
			(at 102.8701 58.42 90)
		)
		(property "Footprint" "fab:Button_Omron_B3SN_6.0x6.0mm"
			(at 104.14 57.15 0)
		)
		(property "Datasheet" "https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3sn.pdf"
			(at 104.14 57.15 0)
		)
		(property "Description" "Push button switch, Omron, B3SN, Sealed Tactile Switch (SMT), SPST-NO Top Actuated Surface Mount"
			(at 104.14 57.15 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:LED_1206")
		(at 102.87 50.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D1"
			(at 101.2698 44.45 0)
		)
		(property "Value" "LED_1206"
			(at 101.2698 46.99 0)
		)
		(property "Footprint" "fab:LED_1206"
			(at 102.87 50.8 0)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
			(at 102.87 50.8 0)
		)
		(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
			(at 102.87 50.8 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
