(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_57555555)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "/Volumes/NO NAME/")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-A)")
	(net 2 "Net-(D1-GK)")
	(net 3 "Net-(D1-BK)")
	(net 4 "Net-(D1-RK)")
	(net 5 "unconnected-(M1-GP26-Pad31)")
	(net 6 "unconnected-(M1-GP11-Pad15)")
	(net 7 "unconnected-(M1-GP27-Pad32)")
	(net 8 "unconnected-(M1-GP8-Pad11)")
	(net 9 "unconnected-(M1-GP16-Pad21)")
	(net 10 "unconnected-(M1-GP5-Pad7)")
	(net 11 "unconnected-(M1-RUN-Pad30)")
	(net 12 "unconnected-(M1-ADC_VREF-Pad35)")
	(net 13 "unconnected-(M1-3V3_EN-Pad37)")
	(net 14 "unconnected-(M1-GP7-Pad10)")
	(net 15 "unconnected-(M1-GP21-Pad27)")
	(net 16 "unconnected-(M1-GP4-Pad6)")
	(net 17 "Net-(M1-GP2)")
	(net 18 "unconnected-(M1-VBUS-Pad40)")
	(net 19 "unconnected-(M1-GP9-Pad12)")
	(net 20 "unconnected-(M1-GP3-Pad5)")
	(net 21 "unconnected-(M1-VSYS-Pad39)")
	(net 22 "unconnected-(M1-GP20-Pad26)")
	(net 23 "Net-(M1-GP1)")
	(net 24 "unconnected-(M1-GP17-Pad22)")
	(net 25 "unconnected-(M1-GP18-Pad24)")
	(net 26 "unconnected-(M1-GP12-Pad16)")
	(net 27 "unconnected-(M1-GP14-Pad19)")
	(net 28 "unconnected-(M1-GP22-Pad29)")
	(net 29 "unconnected-(M1-GP13-Pad17)")
	(net 30 "unconnected-(M1-GP15-Pad20)")
	(net 31 "unconnected-(M1-GP10-Pad14)")
	(net 32 "unconnected-(M1-GP19-Pad25)")
	(net 33 "unconnected-(M1-GP28-Pad34)")
	(net 34 "Net-(M1-GP0)")
	(net 35 "unconnected-(M1-3V3_OUT-Pad36)")
	(net 36 "unconnected-(M1-GP6-Pad9)")
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 122.8344 88.0872 180)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R2"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "R_1206"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "bluetooth.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(M1-GP2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(D1-RK)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 122.5804 79.6036 180)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R3"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "R_1206"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "bluetooth.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(M1-GP0)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(D1-BK)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "fab:RaspberryPi_PicoW_Combined"
		(layer "F.Cu")
		(at 140.6906 104.648)
		(descr "Footprint for Raspberry Pi Pico W, SMD and THT Combined")
		(tags "raspberry pi pico w smd tht combined")
		(property "Reference" "M1"
			(at 0.0025 -2.54 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Module_RaspberryPi_PicoW_Combined"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RP2040 Transceiver; 802.11 b/g/n (Wi-Fi, WiFi, WLAN), Bluetooth® 5 2.4GHz Evaluation Board"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RaspberryPi?PicoW*")
		(sheetname "/")
		(sheetfile "bluetooth.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -10.795 -24.13)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(M1-GP0)")
			(pinfunction "GP0")
			(pintype "bidirectional")
		)
		(pad "1" thru_hole circle
			(at -8.89 -24.13)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(M1-GP0)")
			(pinfunction "GP0")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -10.795 -21.59)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(M1-GP1)")
			(pinfunction "GP1")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at -8.89 -21.59)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(M1-GP1)")
			(pinfunction "GP1")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -10.795 -19.05)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole circle
			(at -8.89 -19.05)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -10.795 -16.51)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(M1-GP2)")
			(pinfunction "GP2")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at -8.89 -16.51)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(M1-GP2)")
			(pinfunction "GP2")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -10.795 -13.97)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(M1-GP3-Pad5)")
			(pinfunction "GP3")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at -8.89 -13.97)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(M1-GP3-Pad5)")
			(pinfunction "GP3")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -10.795 -11.43)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(M1-GP4-Pad6)")
			(pinfunction "GP4")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at -8.89 -11.43)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(M1-GP4-Pad6)")
			(pinfunction "GP4")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -10.795 -8.89)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "unconnected-(M1-GP5-Pad7)")
			(pinfunction "GP5")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at -8.89 -8.89)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(M1-GP5-Pad7)")
			(pinfunction "GP5")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -10.795 -6.35)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -8.89 -6.35)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -10.795 -3.819556)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "unconnected-(M1-GP6-Pad9)")
			(pinfunction "GP6")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole circle
			(at -8.89 -3.81)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(M1-GP6-Pad9)")
			(pinfunction "GP6")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -10.795 -1.27)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(M1-GP7-Pad10)")
			(pinfunction "GP7")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at -8.89 -1.27)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(M1-GP7-Pad10)")
			(pinfunction "GP7")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -10.795 1.27)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "unconnected-(M1-GP8-Pad11)")
			(pinfunction "GP8")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at -8.89 1.27)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(M1-GP8-Pad11)")
			(pinfunction "GP8")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -10.795 3.81)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(M1-GP9-Pad12)")
			(pinfunction "GP9")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at -8.89 3.81)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(M1-GP9-Pad12)")
			(pinfunction "GP9")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at -10.795 6.35)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at -8.89 6.35)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -10.795 8.89)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "unconnected-(M1-GP10-Pad14)")
			(pinfunction "GP10")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole circle
			(at -8.89 8.89)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(M1-GP10-Pad14)")
			(pinfunction "GP10")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -10.795 11.43)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "unconnected-(M1-GP11-Pad15)")
			(pinfunction "GP11")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole circle
			(at -8.89 11.43)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(M1-GP11-Pad15)")
			(pinfunction "GP11")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at -10.795 13.97)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(M1-GP12-Pad16)")
			(pinfunction "GP12")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole circle
			(at -8.89 13.97)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(M1-GP12-Pad16)")
			(pinfunction "GP12")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -10.795 16.51)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "unconnected-(M1-GP13-Pad17)")
			(pinfunction "GP13")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole circle
			(at -8.89 16.51)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(M1-GP13-Pad17)")
			(pinfunction "GP13")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at -10.795 19.05)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at -8.89 19.05)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at -10.795 21.59)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "unconnected-(M1-GP14-Pad19)")
			(pinfunction "GP14")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole circle
			(at -8.89 21.59)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(M1-GP14-Pad19)")
			(pinfunction "GP14")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at -10.795 24.13)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "unconnected-(M1-GP15-Pad20)")
			(pinfunction "GP15")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole circle
			(at -8.89 24.13)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(M1-GP15-Pad20)")
			(pinfunction "GP15")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole circle
			(at 8.89 24.13)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(M1-GP16-Pad21)")
			(pinfunction "GP16")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 10.795 24.13)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "unconnected-(M1-GP16-Pad21)")
			(pinfunction "GP16")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole circle
			(at 8.89 21.59)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(M1-GP17-Pad22)")
			(pinfunction "GP17")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 10.795 21.59)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "unconnected-(M1-GP17-Pad22)")
			(pinfunction "GP17")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole circle
			(at 8.89 19.05)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at 10.795 19.05)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at 8.89 16.51)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(M1-GP18-Pad24)")
			(pinfunction "GP18")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 10.795 16.51)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "unconnected-(M1-GP18-Pad24)")
			(pinfunction "GP18")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole circle
			(at 8.89 13.97)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(M1-GP19-Pad25)")
			(pinfunction "GP19")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 10.795 13.97)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "unconnected-(M1-GP19-Pad25)")
			(pinfunction "GP19")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole circle
			(at 8.89 11.43)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(M1-GP20-Pad26)")
			(pinfunction "GP20")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 10.795 11.43)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(M1-GP20-Pad26)")
			(pinfunction "GP20")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole circle
			(at 8.89 8.89)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(M1-GP21-Pad27)")
			(pinfunction "GP21")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 10.795 8.89)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "unconnected-(M1-GP21-Pad27)")
			(pinfunction "GP21")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole circle
			(at 8.89 6.35)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 10.795 6.35)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "29" thru_hole circle
			(at 8.89 3.81)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(M1-GP22-Pad29)")
			(pinfunction "GP22")
			(pintype "bidirectional")
		)
		(pad "29" smd rect
			(at 10.795 3.81)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "unconnected-(M1-GP22-Pad29)")
			(pinfunction "GP22")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole circle
			(at 8.89 1.27)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(M1-RUN-Pad30)")
			(pinfunction "RUN")
			(pintype "input")
		)
		(pad "30" smd rect
			(at 10.795 1.27)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(M1-RUN-Pad30)")
			(pinfunction "RUN")
			(pintype "input")
		)
		(pad "31" thru_hole circle
			(at 8.89 -1.27)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(M1-GP26-Pad31)")
			(pinfunction "GP26")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at 10.786443 -1.297864)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "unconnected-(M1-GP26-Pad31)")
			(pinfunction "GP26")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole circle
			(at 8.89 -3.81)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(M1-GP27-Pad32)")
			(pinfunction "GP27")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at 10.795 -3.81)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "unconnected-(M1-GP27-Pad32)")
			(pinfunction "GP27")
			(pintype "bidirectional")
		)
		(pad "33" thru_hole circle
			(at 8.89 -6.35)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 10.795 -6.35)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "34" thru_hole circle
			(at 8.89 -8.89)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(M1-GP28-Pad34)")
			(pinfunction "GP28")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at 10.795 -8.89)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "unconnected-(M1-GP28-Pad34)")
			(pinfunction "GP28")
			(pintype "bidirectional")
		)
		(pad "35" thru_hole circle
			(at 8.89 -11.43)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(M1-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF")
			(pintype "input")
		)
		(pad "35" smd rect
			(at 10.795 -11.43)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "unconnected-(M1-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF")
			(pintype "input")
		)
		(pad "36" thru_hole circle
			(at 8.89 -13.97)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(M1-3V3_OUT-Pad36)")
			(pinfunction "3V3_OUT")
			(pintype "power_in")
		)
		(pad "36" smd rect
			(at 10.795 -13.97)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "unconnected-(M1-3V3_OUT-Pad36)")
			(pinfunction "3V3_OUT")
			(pintype "power_in")
		)
		(pad "37" thru_hole circle
			(at 8.89 -16.51)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(M1-3V3_EN-Pad37)")
			(pinfunction "3V3_EN")
			(pintype "input")
		)
		(pad "37" smd rect
			(at 10.795 -16.51)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "unconnected-(M1-3V3_EN-Pad37)")
			(pinfunction "3V3_EN")
			(pintype "input")
		)
		(pad "38" thru_hole circle
			(at 8.89 -19.05)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "38" smd rect
			(at 10.795 -19.05)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "39" thru_hole circle
			(at 8.89 -21.59)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(M1-VSYS-Pad39)")
			(pinfunction "VSYS")
			(pintype "power_in")
		)
		(pad "39" smd rect
			(at 10.795 -21.59)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(M1-VSYS-Pad39)")
			(pinfunction "VSYS")
			(pintype "power_in")
		)
		(pad "40" thru_hole circle
			(at 8.89 -24.13)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(M1-VBUS-Pad40)")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "40" smd rect
			(at 10.795 -24.13)
			(size 3.81 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(M1-VBUS-Pad40)")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "fab:LED_RGB_CreeLED_CLV1A-FKB"
		(layer "F.Cu")
		(at 114.4524 84.1756 90)
		(descr "RGB LED 3.2x2.7mm http://www.avagotech.com/docs/AV02-0610EN")
		(tags "LED 3227")
		(property "Reference" "D1"
			(at 0 -2.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED_RGB_CreeLED_PLCC4"
			(at 0 2.6 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://assets.cree-led.com/a/ds/h/HB-CLV1A-FKB.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "LED RGB 4PLCC SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CreeLED?CLV1A?FKB*")
		(sheetname "/")
		(sheetfile "bluetooth.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.75 -0.75 270)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(D1-RK)")
			(pinfunction "RK")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.75 0.75 270)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.75 0.75 270)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(D1-BK)")
			(pinfunction "BK")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.75 -0.75 270)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(D1-GK)")
			(pinfunction "GK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/fab.3dshapes/LED_RGB_CreeLED_CLV1A-FKB.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 122.5804 83.058 180)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R1"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "R_1206"
			(at 1.3716 1.8796 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "bluetooth.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 0 180)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(M1-GP1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5 0 180)
			(size 1.2 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(D1-GK)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Resistor-1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(gr_rect
		(start 112.1664 78.232)
		(end 133.4516 89.2048)
		(fill no)
		(layer "Edge.Cuts")
	)
	(embedded_fonts no)
)
