(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "fab:LED_RGB_CreeLED_PLCC4"
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 10.16 0)
			)
			(property "Value" "LED_RGB_CreeLED_PLCC4"
				(at 0 -10.16 0)
			)
			(property "Footprint" "fab:LED_RGB_CreeLED_CLV1A-FKB"
				(at 0 0 0)
			)
			(property "Datasheet" "https://assets.cree-led.com/a/ds/h/HB-CLV1A-FKB.pdf"
				(at 0 0 0)
			)
			(property "Description" "LED RGB 4PLCC SMD"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED RGB diode common anode RABG CLV1A-FKB-CK1VW1DE1BB7C3C3"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*CreeLED?CLV1A?FKB*"
				(at 0 0 0)
			)
			(symbol "LED_RGB_CreeLED_PLCC4_0_0"
				(text "R"
					(at -1.905 3.81 0)
				)
				(text "G"
					(at -1.905 -1.27 0)
				)
				(text "B"
					(at -1.905 -6.35 0)
				)
			)
			(symbol "LED_RGB_CreeLED_PLCC4_0_1"
				(rectangle
					(start -2.54 8.89)
					(end 2.54 -8.89)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -1.27 6.35) (xy -1.27 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 6.35) (xy -1.27 3.81) (xy -1.27 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 5.08) (xy -2.54 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 1.27) (xy -1.27 -1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy -2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -3.81) (xy -1.27 -6.35)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -3.81) (xy -1.27 -6.35)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -5.08) (xy -2.54 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -5.08) (xy 1.27 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.016 6.35) (xy 0.508 7.874) (xy -0.254 7.874) (xy 0.508 7.874) (xy 0.508 7.112)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.016 1.27) (xy 0.508 2.794) (xy -0.254 2.794) (xy 0.508 2.794) (xy 0.508 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.016 -3.81) (xy 0.508 -2.286) (xy -0.254 -2.286) (xy 0.508 -2.286) (xy 0.508 -3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 6.35) (xy 1.524 7.874) (xy 0.762 7.874) (xy 1.524 7.874) (xy 1.524 7.112)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 1.524 2.794) (xy 0.762 2.794) (xy 1.524 2.794) (xy 1.524 2.032)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -3.81) (xy 1.524 -2.286) (xy 0.762 -2.286) (xy 1.524 -2.286) (xy 1.524 -3.048)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 6.35) (xy 1.27 3.81) (xy -1.27 5.08) (xy 1.27 6.35)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 1.27 6.35)
					(end 1.27 6.35)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 5.08) (xy -1.27 5.08)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 1.27 3.81)
					(end 1.27 6.35)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 1.27) (xy 1.27 -1.27) (xy -1.27 0) (xy 1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 1.27 1.27)
					(end 1.27 1.27)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 2.54 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 1.27 -1.27)
					(end 1.27 1.27)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -3.81) (xy 1.27 -6.35) (xy -1.27 -5.08) (xy 1.27 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -5.08) (xy 2.032 -5.08) (xy 2.032 5.08) (xy 1.27 5.08)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 0)
					(radius 0.254)
					(fill
						(type outline)
					)
				)
			)
			(symbol "LED_RGB_CreeLED_PLCC4_1_1"
				(pin passive line
					(at -5.08 5.08 0)
					(length 2.54)
					(name "RK")
					(number "1")
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "GK")
					(number "4")
				)
				(pin passive line
					(at -5.08 -5.08 0)
					(length 2.54)
					(name "BK")
					(number "3")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:Module_RaspberryPi_PicoW_Combined"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "M"
				(at 0 0 0)
			)
			(property "Value" "Module_RaspberryPi_PicoW_Combined"
				(at 0 0 0)
			)
			(property "Footprint" "fab:RaspberryPi_PicoW_Combined"
				(at 0 0 0)
			)
			(property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf"
				(at 0 0 0)
			)
			(property "Description" "RP2040 Transceiver; 802.11 b/g/n (Wi-Fi, WiFi, WLAN), Bluetooth® 5 2.4GHz Evaluation Board"
				(at 0 0 0)
			)
			(property "ki_keywords" "Raspberry Pi Pico RP2040 SC0918"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*RaspberryPi?PicoW*"
				(at 0 0 0)
			)
			(symbol "Module_RaspberryPi_PicoW_Combined_1_1"
				(rectangle
					(start -10.16 25.4)
					(end 10.16 -25.4)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -12.7 17.78 0)
					(length 2.54)
					(name "GP0")
					(number "1")
				)
				(pin bidirectional line
					(at -12.7 15.24 0)
					(length 2.54)
					(name "GP1")
					(number "2")
				)
				(pin bidirectional line
					(at -12.7 12.7 0)
					(length 2.54)
					(name "GP2")
					(number "4")
				)
				(pin bidirectional line
					(at -12.7 10.16 0)
					(length 2.54)
					(name "GP3")
					(number "5")
				)
				(pin bidirectional line
					(at -12.7 7.62 0)
					(length 2.54)
					(name "GP4")
					(number "6")
				)
				(pin bidirectional line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "GP5")
					(number "7")
				)
				(pin bidirectional line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "GP6")
					(number "9")
				)
				(pin bidirectional line
					(at -12.7 0 0)
					(length 2.54)
					(name "GP7")
					(number "10")
				)
				(pin bidirectional line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "GP8")
					(number "11")
				)
				(pin bidirectional line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "GP9")
					(number "12")
				)
				(pin bidirectional line
					(at -12.7 -7.62 0)
					(length 2.54)
					(name "GP10")
					(number "14")
				)
				(pin bidirectional line
					(at -12.7 -10.16 0)
					(length 2.54)
					(name "GP11")
					(number "15")
				)
				(pin bidirectional line
					(at -12.7 -12.7 0)
					(length 2.54)
					(name "GP12")
					(number "16")
				)
				(pin bidirectional line
					(at -12.7 -15.24 0)
					(length 2.54)
					(name "GP13")
					(number "17")
				)
				(pin bidirectional line
					(at -12.7 -17.78 0)
					(length 2.54)
					(name "GP14")
					(number "19")
				)
				(pin bidirectional line
					(at -12.7 -20.32 0)
					(length 2.54)
					(name "GP15")
					(number "20")
				)
				(pin power_in line
					(at -5.08 27.94 270)
					(length 2.54)
					(name "VBUS")
					(number "40")
				)
				(pin power_in line
					(at -2.54 27.94 270)
					(length 2.54)
					(name "VSYS")
					(number "39")
				)
				(pin passive line
					(at 0 -27.94 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "13")
				)
				(pin passive line
					(at 0 -27.94 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "18")
				)
				(pin passive line
					(at 0 -27.94 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "23")
				)
				(pin passive line
					(at 0 -27.94 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "28")
				)
				(pin power_in line
					(at 0 -27.94 90)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin passive line
					(at 0 -27.94 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "33")
				)
				(pin passive line
					(at 0 -27.94 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "38")
				)
				(pin passive line
					(at 0 -27.94 90)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "8")
				)
				(pin power_in line
					(at 2.54 27.94 270)
					(length 2.54)
					(name "3V3_OUT")
					(number "36")
				)
				(pin input line
					(at 12.7 15.24 180)
					(length 2.54)
					(name "3V3_EN")
					(number "37")
				)
				(pin input line
					(at 12.7 12.7 180)
					(length 2.54)
					(name "ADC_VREF")
					(number "35")
				)
				(pin input line
					(at 12.7 10.16 180)
					(length 2.54)
					(name "RUN")
					(number "30")
				)
				(pin bidirectional line
					(at 12.7 2.54 180)
					(length 2.54)
					(name "GP28")
					(number "34")
				)
				(pin bidirectional line
					(at 12.7 0 180)
					(length 2.54)
					(name "GP27")
					(number "32")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "GP26")
					(number "31")
				)
				(pin bidirectional line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "GP22")
					(number "29")
				)
				(pin bidirectional line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "GP21")
					(number "27")
				)
				(pin bidirectional line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "GP20")
					(number "26")
				)
				(pin bidirectional line
					(at 12.7 -12.7 180)
					(length 2.54)
					(name "GP19")
					(number "25")
				)
				(pin bidirectional line
					(at 12.7 -15.24 180)
					(length 2.54)
					(name "GP18")
					(number "24")
				)
				(pin bidirectional line
					(at 12.7 -17.78 180)
					(length 2.54)
					(name "GP17")
					(number "22")
				)
				(pin bidirectional line
					(at 12.7 -20.32 180)
					(length 2.54)
					(name "GP16")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:R_1206"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.54 0 90)
			)
			(property "Value" "R_1206"
				(at -2.54 0 90)
			)
			(property "Footprint" "fab:R_1206"
				(at 0 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor RC1206FR-074M99L RC1206FR-07499KL RC1206FR-0749K9L RC1206FR-0749R9L RC1206FR-074R99L ERJ-8BWJR100V RC1206FR-070RL RC1206FR-071RL RC1206FR-0710RL RC1206FR-07100RL RC1206FR-07499RL RC1206FR-071KL RC1206FR-074K99L RC1206FR-0710KL RC1206FR-07100KL RC1206FR-071ML RC1206FR-0710ML PT1206FR-070R1L"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*R*1206*"
				(at 0 0 0)
			)
			(symbol "R_1206_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type background)
					)
				)
			)
			(symbol "R_1206_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
	)
	(wire
		(pts
			(xy 110.49 128.27) (xy 110.49 83.82)
		)
	)
	(wire
		(pts
			(xy 91.44 68.58) (xy 91.44 67.31)
		)
	)
	(wire
		(pts
			(xy 120.65 82.55) (xy 127 82.55)
		)
	)
	(wire
		(pts
			(xy 118.11 68.58) (xy 118.11 87.63)
		)
	)
	(wire
		(pts
			(xy 91.44 83.82) (xy 100.33 83.82)
		)
	)
	(wire
		(pts
			(xy 82.55 88.9) (xy 100.33 88.9)
		)
	)
	(wire
		(pts
			(xy 82.55 62.23) (xy 120.65 62.23)
		)
	)
	(wire
		(pts
			(xy 82.55 68.58) (xy 82.55 62.23)
		)
	)
	(wire
		(pts
			(xy 91.44 78.74) (xy 91.44 83.82)
		)
	)
	(wire
		(pts
			(xy 82.55 78.74) (xy 82.55 88.9)
		)
	)
	(wire
		(pts
			(xy 119.38 85.09) (xy 127 85.09)
		)
	)
	(wire
		(pts
			(xy 91.44 67.31) (xy 119.38 67.31)
		)
	)
	(wire
		(pts
			(xy 120.65 62.23) (xy 120.65 82.55)
		)
	)
	(wire
		(pts
			(xy 119.38 67.31) (xy 119.38 85.09)
		)
	)
	(wire
		(pts
			(xy 118.11 87.63) (xy 127 87.63)
		)
	)
	(wire
		(pts
			(xy 100.33 68.58) (xy 118.11 68.58)
		)
	)
	(wire
		(pts
			(xy 139.7 128.27) (xy 110.49 128.27)
		)
	)
	(symbol
		(lib_id "fab:Module_RaspberryPi_PicoW_Combined")
		(at 139.7 100.33 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "M1"
			(at 141.8433 128.27 0)
		)
		(property "Value" "Module_RaspberryPi_PicoW_Combined"
			(at 141.8433 130.81 0)
		)
		(property "Footprint" "fab:RaspberryPi_PicoW_Combined"
			(at 139.7 100.33 0)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf"
			(at 139.7 100.33 0)
		)
		(property "Description" "RP2040 Transceiver; 802.11 b/g/n (Wi-Fi, WiFi, WLAN), Bluetooth® 5 2.4GHz Evaluation Board"
			(at 139.7 100.33 0)
		)
		(pin "1")
		(pin "2")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "9")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "17")
		(pin "19")
		(pin "20")
		(pin "40")
		(pin "39")
		(pin "13")
		(pin "18")
		(pin "23")
		(pin "28")
		(pin "3")
		(pin "33")
		(pin "38")
		(pin "8")
		(pin "36")
		(pin "37")
		(pin "35")
		(pin "30")
		(pin "34")
		(pin "32")
		(pin "31")
		(pin "29")
		(pin "27")
		(pin "26")
		(pin "25")
		(pin "24")
		(pin "22")
		(pin "21")
		(instances
			(project ""
				(path
					(reference "M1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:R_1206")
		(at 100.33 73.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 102.87 72.3899 0)
		)
		(property "Value" "R_1206"
			(at 102.87 74.9299 0)
		)
		(property "Footprint" "fab:R_1206"
			(at 100.33 73.66 90)
		)
		(property "Datasheet" "~"
			(at 100.33 73.66 0)
		)
		(property "Description" "Resistor"
			(at 100.33 73.66 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "bluetooth"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:R_1206")
		(at 91.44 73.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 93.98 72.3899 0)
		)
		(property "Value" "R_1206"
			(at 93.98 74.9299 0)
		)
		(property "Footprint" "fab:R_1206"
			(at 91.44 73.66 90)
		)
		(property "Datasheet" "~"
			(at 91.44 73.66 0)
		)
		(property "Description" "Resistor"
			(at 91.44 73.66 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:R_1206")
		(at 82.55 73.66 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 85.09 72.3899 0)
		)
		(property "Value" "R_1206"
			(at 85.09 74.9299 0)
		)
		(property "Footprint" "fab:R_1206"
			(at 82.55 73.66 90)
		)
		(property "Datasheet" "~"
			(at 82.55 73.66 0)
		)
		(property "Description" "Resistor"
			(at 82.55 73.66 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "bluetooth"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:LED_RGB_CreeLED_PLCC4")
		(at 105.41 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 105.41 69.85 0)
		)
		(property "Value" "LED_RGB_CreeLED_PLCC4"
			(at 105.41 72.39 0)
		)
		(property "Footprint" "fab:LED_RGB_CreeLED_CLV1A-FKB"
			(at 105.41 83.82 0)
		)
		(property "Datasheet" "https://assets.cree-led.com/a/ds/h/HB-CLV1A-FKB.pdf"
			(at 105.41 83.82 0)
		)
		(property "Description" "LED RGB 4PLCC SMD"
			(at 105.41 83.82 0)
		)
		(pin "1")
		(pin "4")
		(pin "3")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
