(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+3.3V")
	(net 3 "/SDA")
	(net 4 "/SCL")
	(net 5 "unconnected-(M2-RESET-Pad18)")
	(net 6 "/TOUCH2")
	(net 7 "unconnected-(M2-P28{slash}D2-Pad3)")
	(net 8 "unconnected-(M2-SWCLK-Pad20)")
	(net 9 "/TOUCH5")
	(net 10 "unconnected-(M2-P29{slash}D3-Pad4)")
	(net 11 "/TOUCH3")
	(net 12 "/TOUCH4")
	(net 13 "unconnected-(M2-SWDIO-Pad17)")
	(net 14 "/TOUCH1")
	(net 15 "/TOUCH0")
	(net 16 "unconnected-(M2-P0{slash}D6-Pad7)")
	(net 17 "unconnected-(M2-GND-Pad19)")
	(net 18 "unconnected-(M2-VIN-Pad16)")
	(net 19 "unconnected-(M2-5V-Pad14)")
	(net 20 "unconnected-(M2-GND-Pad15)")
	(footprint "footprints:Display_128x64_096_I2C"
		(layer "F.Cu")
		(at 139.573 91.694)
		(descr "Display 0.96\" OLED 128x64 pixel with SSD1306 controller and I2C interface")
		(tags "display OLED SSD1306 128x64")
		(property "Reference" "J4"
			(at -6.985 24.13 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at -7.874 4.699 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "design_xiao.kicad_sch")
		(attr through_hole)
		(fp_text user "GND"
			(at -3.81 2.413 0)
			(layer "F.SilkS")
		)
		(fp_text user "VDD"
			(at -1.27 2.413 0)
			(layer "F.SilkS")
		)
		(fp_text user "SDA"
			(at 3.937 2.413 0)
			(layer "F.SilkS")
		)
		(fp_text user "SCL"
			(at 1.27 2.413 0)
			(layer "F.SilkS")
		)
		(pad "" np_thru_hole oval
			(at -11.176 0.635)
			(size 3.8 2.9)
			(drill oval 3.8 2.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at -11.176 23.749)
			(size 3.8 2.9)
			(drill oval 3.8 2.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 11.176 0.635)
			(size 3.8 2.9)
			(drill oval 3.8 2.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 11.176 23.749)
			(size 3.8 2.9)
			(drill oval 3.8 2.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at -3.81 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -1.27 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3.3V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 1.27 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 3.81 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/SDA")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 124.46 83.439 -90)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R4"
			(at -3.683 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 3.683 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "design_xiao.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 270)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/SDA")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 270)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 127.254 85.344 -90)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R5"
			(at -3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 3.556 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "design_xiao.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 270)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/SCL")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 270)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:SeeedStudio_XIAO_RP2040"
		(layer "F.Cu")
		(at 139.7 79.121)
		(descr "Footprint for Seeed Studio XIAO modules")
		(tags "xiao seeed studio module")
		(property "Reference" "M2"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Module_XIAO-RP2040"
			(at 0.005 1.27 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RP2040 XIAO RP2040 - ARM® Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SeeedStudio?XIAO?RP2040*")
		(sheetname "/")
		(sheetfile "design_xiao.kicad_sch")
		(attr through_hole)
		(fp_text user "GND"
			(at 2.54 -5.96 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SWDIO"
			(at 0 -8.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "VIN"
			(at -2.535 8.89 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "RESET"
			(at 0 -5.96 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 2.545 8.89 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "SWCLK"
			(at 2.54 -8.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0.0025 3.81 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -7.615 -7.62)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/TOUCH5")
			(pinfunction "P26/D0")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -7.615 -5.08)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/TOUCH3")
			(pinfunction "P27/D1")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -7.615 -2.54)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "unconnected-(M2-P28{slash}D2-Pad3)")
			(pinfunction "P28/D2")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -7.615 0)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "unconnected-(M2-P29{slash}D3-Pad4)")
			(pinfunction "P29/D3")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -7.615 2.54)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/SDA")
			(pinfunction "P6/D4")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -7.615 5.08)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/SCL")
			(pinfunction "P7/D5")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -7.615 7.62)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(M2-P0{slash}D6-Pad7)")
			(pinfunction "P0/D6")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at 7.62 7.62)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/TOUCH4")
			(pinfunction "P1/D7")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at 7.62 5.08)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/TOUCH2")
			(pinfunction "P2/D8")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 7.62 2.54)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "/TOUCH1")
			(pinfunction "P4/D9")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at 7.62 0)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "/TOUCH0")
			(pinfunction "P3/D10")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at 7.62 -2.54)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.3V")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 7.62 -5.08)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 7.62 -7.62)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(M2-5V-Pad14)")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at 1.275 8.89 270)
			(size 2.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(M2-GND-Pad15)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -1.265 8.89 270)
			(size 2.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(M2-VIN-Pad16)")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "17" smd circle
			(at -1.27 -8.5)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "unconnected-(M2-SWDIO-Pad17)")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
		)
		(pad "18" smd circle
			(at -1.27 -5.96)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "unconnected-(M2-RESET-Pad18)")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "19" smd circle
			(at 1.27 -5.96)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(M2-GND-Pad19)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "20" smd circle
			(at 1.27 -8.5)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "unconnected-(M2-SWCLK-Pad20)")
			(pinfunction "SWCLK")
			(pintype "input")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Mask" "F.Paste" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 134.5 68.571) (xy 135.9 68.571) (xy 135.9 70.621) (xy 134.5 70.621)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Mask" "F.Paste" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 134.5 72.621) (xy 135.9 72.621) (xy 135.9 74.821) (xy 134.5 74.821)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Mask" "F.Paste" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 143.5 68.571) (xy 144.9 68.571) (xy 144.9 70.621) (xy 143.5 70.621)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "F.Mask" "F.Paste" "User.1")
			(name "USB_MECHA")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 143.5 72.621) (xy 144.9 72.621) (xy 144.9 74.821) (xy 143.5 74.821)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "B.Cu")
		(at 92.71 114.3 180)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "⌀ M3"
			(at -4.191 4.318 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 -4.2 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "B.Cu")
		(at 186.69 72.39 180)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "⌀ M3"
			(at 5.588 -3.048 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 -4.2 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "B.Cu")
		(at 92.71 72.39 180)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "⌀ M3"
			(at -5.334 -2.667 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 -4.2 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "B.Cu")
		(at 186.69 114.3 180)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "⌀ M3"
			(at 4.699 4.445 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 -4.2 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(gr_arc
		(start 88.9 72.39)
		(mid 90.015923 69.695923)
		(end 92.71 68.58)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 92.71 118.11)
		(mid 90.015923 116.994077)
		(end 88.9 114.3)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 190.5 114.3)
		(mid 189.384077 116.994077)
		(end 186.69 118.11)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 186.69 68.58)
		(end 92.71 68.58)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.9 114.3)
		(end 88.9 72.39)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.5 114.3)
		(end 190.5 72.39)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 186.69 68.58)
		(mid 189.384077 69.695923)
		(end 190.5 72.39)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.71 118.11)
		(end 186.69 118.11)
		(layer "Edge.Cuts")
	)
	(gr_text "Q2 [D8]"
		(at 106.68 108.966 0)
		(layer "F.SilkS")
	)
	(gr_text "0.96{dblquote} OLED module"
		(at 135.382 115.824 -0)
		(layer "F.SilkS")
	)
	(gr_text "3.7{dblquote} / 93.98mm"
		(at 160.02 72.009 -0)
		(layer "F.SilkS")
	)
	(gr_text "Q3 [D1]"
		(at 96.52 98.806 0)
		(layer "F.SilkS")
	)
	(gr_text "QPAD-XIAO"
		(at 168.021 115.824 0)
		(layer "F.SilkS")
	)
	(gr_text "Q5 [D0]"
		(at 106.68 88.773 0)
		(layer "F.SilkS")
	)
	(gr_text "1.65{dblquote} / 41.91mm"
		(at 188.468 107.696 90)
		(layer "F.SilkS")
	)
	(gr_text "Q4 [D7]"
		(at 116.84 98.806 0)
		(layer "F.SilkS")
	)
	(gr_text "HTMAA 2025"
		(at 111.125 115.824 0)
		(layer "F.SilkS")
	)
	(gr_text "Q1 [D9]"
		(at 168.275 101.346 0)
		(layer "F.SilkS")
	)
	(gr_text "Q0 [D10]"
		(at 181.102 92.456 0)
		(layer "F.SilkS")
	)
	(gr_text "MIT's Center for Bits and Atoms\nQuentin Bolsée, 2025"
		(at 123.19 116.586 0)
		(layer "B.SilkS")
	)
	(gr_text "If at first you don't succeed,\nfind out why"
		(at 180.975 116.713 0)
		(layer "B.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.3)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 88.9 68.58) (xy 190.5 68.58) (xy 190.5 118.11) (xy 88.9 118.11)
			)
		)
	)
	(embedded_fonts no)
)
