(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(J1-SHIELD1-PadSH1)")
	(net 2 "unconnected-(J1-SHIELD3-PadSH3)")
	(net 3 "unconnected-(J1-SHIELD2-PadSH2)")
	(net 4 "unconnected-(J1-SHIELD4-PadSH4)")
	(net 5 "GND")
	(net 6 "+3.3V")
	(net 7 "+5V")
	(net 8 "Net-(U1-VDDCORE)")
	(net 9 "/DATA+")
	(net 10 "/DATA-")
	(net 11 "unconnected-(J2-Pin_8-Pad8)")
	(net 12 "/nRESET")
	(net 13 "/SWDIO")
	(net 14 "unconnected-(J2-Pin_6-Pad6)")
	(net 15 "/SWCLK")
	(net 16 "unconnected-(J2-Pin_7-Pad7)")
	(net 17 "/SDA")
	(net 18 "/SCL")
	(net 19 "/TOUCH2")
	(net 20 "unconnected-(U1-PA23-Pad22)")
	(net 21 "unconnected-(U1-PA14-Pad15)")
	(net 22 "unconnected-(U1-PA19-Pad20)")
	(net 23 "/TOUCH3")
	(net 24 "unconnected-(U1-PA27-Pad25)")
	(net 25 "unconnected-(U1-PA10-Pad13)")
	(net 26 "unconnected-(U1-PA01-Pad2)")
	(net 27 "unconnected-(U1-PA28-Pad27)")
	(net 28 "unconnected-(U1-PA11-Pad14)")
	(net 29 "/TOUCH4")
	(net 30 "unconnected-(U1-PA09-Pad12)")
	(net 31 "/TOUCH1")
	(net 32 "/TOUCH0")
	(net 33 "unconnected-(U1-PA22-Pad21)")
	(net 34 "unconnected-(U1-PA08-Pad11)")
	(net 35 "/TOUCH5")
	(net 36 "unconnected-(U1-PA18-Pad19)")
	(net 37 "/LED")
	(net 38 "unconnected-(U1-PA00-Pad1)")
	(net 39 "Net-(D1-K)")
	(net 40 "unconnected-(J1-ID-Pad4)")
	(net 41 "unconnected-(J1-SHIELD5-PadSH5)")
	(net 42 "unconnected-(J1-SHIELD6-PadSH6)")
	(footprint "fab:PinHeader_2x05_P1.27mm_Vertical_SMD"
		(layer "F.Cu")
		(at 139.7 111.76 -90)
		(descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
		(tags "Surface mounted pin header SMD 2x05 1.27mm double row")
		(property "Reference" "J2"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_2x05_P1.27mm_Vertical_SMD"
			(at 0 4.235 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/20021121.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 10 position 0.050\" (1.27mm)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*2x05*")
		(sheetname "/")
		(sheetfile "design_micro.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.95 -2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.95 -2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/SWDIO")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.95 -1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.95 -1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "/SWCLK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.95 0 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.95 0 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(J2-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive+no_connect")
		)
		(pad "7" smd rect
			(at -1.95 1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(J2-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 1.95 1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(J2-Pin_8-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive+no_connect")
		)
		(pad "9" smd rect
			(at -1.95 2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 1.95 2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/nRESET")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:TQFP-32_7x7mm_P0.8mm"
		(layer "F.Cu")
		(at 139.7 96.266 90)
		(descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "QFP 0.8")
		(property "Reference" "U1"
			(at 1.651 6.604 180)
			(layer "F.SilkS")
		)
		(property "Value" "Microcontroller_ATSAMD21E17A-AUT"
			(at 0 6.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_DataSheet_DS40001882F.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash, 4K SRAM, TQFP-32"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TQFP*7x7mm*P0.8mm*")
		(sheetname "/")
		(sheetfile "design_micro.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.318 -2.806 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "unconnected-(U1-PA00-Pad1)")
			(pinfunction "PA00")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -4.318 -2.006 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(U1-PA01-Pad2)")
			(pinfunction "PA01")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -4.318 -1.206 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/TOUCH0")
			(pinfunction "PA02")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -4.318 -0.406 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "/TOUCH1")
			(pinfunction "PA03")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -4.318 0.394 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/TOUCH2")
			(pinfunction "PA04")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -4.318 1.194 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "/TOUCH3")
			(pinfunction "PA05")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -4.318 1.994 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "/TOUCH4")
			(pinfunction "PA06")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -4.318 2.794 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/TOUCH5")
			(pinfunction "PA07")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -2.806 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3.3V")
			(pinfunction "VDDANA")
			(pintype "power_in")
		)
		(pad "10" smd rect
			(at -2.006 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd rect
			(at -1.206 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "unconnected-(U1-PA08-Pad11)")
			(pinfunction "PA08")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -0.406 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "unconnected-(U1-PA09-Pad12)")
			(pinfunction "PA09")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 0.394 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "unconnected-(U1-PA10-Pad13)")
			(pinfunction "PA10")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at 1.194 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "unconnected-(U1-PA11-Pad14)")
			(pinfunction "PA11")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at 1.994 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(U1-PA14-Pad15)")
			(pinfunction "PA14")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at 2.794 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/LED")
			(pinfunction "PA15")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at 4.318 2.8 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/SDA")
			(pinfunction "PA16")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at 4.318 2 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/SCL")
			(pinfunction "PA17")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at 4.318 1.2 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "unconnected-(U1-PA18-Pad19)")
			(pinfunction "PA18")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at 4.318 0.4 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(U1-PA19-Pad20)")
			(pinfunction "PA19")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 4.318 -0.4 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "unconnected-(U1-PA22-Pad21)")
			(pinfunction "PA22")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 4.318 -1.2 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(U1-PA23-Pad22)")
			(pinfunction "PA23")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at 4.318 -2 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/DATA-")
			(pinfunction "PA24")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 4.318 -2.8 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/DATA+")
			(pinfunction "PA25")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 2.7936 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "unconnected-(U1-PA27-Pad25)")
			(pinfunction "PA27")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 1.9936 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/nRESET")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "27" smd rect
			(at 1.1936 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "unconnected-(U1-PA28-Pad27)")
			(pinfunction "PA28")
			(pintype "bidirectional")
		)
		(pad "28" smd rect
			(at 0.3936 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at -0.4064 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(U1-VDDCORE)")
			(pinfunction "VDDCORE")
			(pintype "power_out")
		)
		(pad "30" smd rect
			(at -1.2064 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3.3V")
			(pinfunction "VDDIN")
			(pintype "power_in")
		)
		(pad "31" smd rect
			(at -2.0064 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "/SWCLK")
			(pinfunction "PA30")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at -2.8064 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/SWDIO")
			(pinfunction "PA31")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 186.69 114.3)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "⌀ M3"
			(at -5.969 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "fab:C_1206"
		(layer "F.Cu")
		(at 132.302 94.488 -90)
		(descr "Capacitor SMD 1206, hand soldering")
		(tags "capacitor 1206")
		(property "Reference" "C3"
			(at -1.651 2.381 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/mlcc/UPY-GP_NP0_16V-to-50V_18.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, SMD, 1206"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*C*")
		(sheetname "/")
		(sheetfile "design_micro.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 270)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 270)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(U1-VDDCORE)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 92.71 72.39)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "⌀ M3"
			(at 6.35 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "fab:LED_1206"
		(layer "F.Cu")
		(at 159.893 70.104)
		(descr "LED SMD 1206, hand soldering")
		(tags "LED 1206")
		(property "Reference" "D1"
			(at 0 2.032 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_1206"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LED*1206*")
		(sheetname "/")
		(sheetfile "design_micro.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/LED")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 138.43 84.709)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R4"
			(at -3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "design_micro.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/SDA")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:MOLEX_1050170001"
		(layer "F.Cu")
		(at 139.7 69.596 180)
		(property "Reference" "J1"
			(at 2.73 -6.0225 0)
			(layer "F.SilkS")
		)
		(property "Value" "1050170001"
			(at 9.715 -7.435 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "OPTION" "MOLEX_CONFIG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "2.85mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Molex"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "design_micro.kicad_sch")
		(attr smd)
		(fp_text user "PTH 0.85 +/- 0.05"
			(at -4.445 -8.915 0)
			(layer "Dwgs.User")
		)
		(fp_text user "PTH Slot 1.3 +/- 0.05 X 0.6 +/- 0.05"
			(at -4.445 -8.28 0)
			(layer "Dwgs.User")
		)
		(fp_text user "PCB Edge"
			(at 4.5 -0.2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.3 -4.125 180)
			(size 0.4 1.35)
			(layers "F.Cu" "F.Paste")
			(net 7 "+5V")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -0.65 -4.125 180)
			(size 0.4 1.35)
			(layers "F.Cu" "F.Paste")
			(net 10 "/DATA-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at 0 -4.125 180)
			(size 0.4 1.35)
			(layers "F.Cu" "F.Paste")
			(net 9 "/DATA+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at 0.65 -4.125 180)
			(size 0.4 1.35)
			(layers "F.Cu" "F.Paste")
			(net 40 "unconnected-(J1-ID-Pad4)")
			(pinfunction "ID")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at 1.3 -4.125 180)
			(size 0.4 1.35)
			(layers "F.Cu" "F.Paste")
			(net 5 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "SH1" thru_hole circle
			(at -2.5 -4.15 180)
			(size 1.45 1.45)
			(drill 0.85)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "unconnected-(J1-SHIELD1-PadSH1)")
			(pinfunction "SHIELD1")
			(pintype "passive")
		)
		(pad "SH2" thru_hole circle
			(at 2.5 -4.15 180)
			(size 1.45 1.45)
			(drill 0.85)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 3 "unconnected-(J1-SHIELD2-PadSH2)")
			(pinfunction "SHIELD2")
			(pintype "passive")
		)
		(pad "SH3" thru_hole custom
			(at -3.5 -1.45 180)
			(size 1.2 1.9)
			(drill oval 0.6 1.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "unconnected-(J1-SHIELD3-PadSH3)")
			(pinfunction "SHIELD3")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1.2 0.95) (xy -0.1 0.95) (xy -0.126 0.949) (xy -0.152 0.947) (xy -0.178 0.944) (xy -0.204 0.939)
						(xy -0.229 0.933) (xy -0.255 0.926) (xy -0.279 0.917) (xy -0.303 0.907) (xy -0.327 0.896) (xy -0.35 0.883)
						(xy -0.372 0.869) (xy -0.394 0.855) (xy -0.415 0.839) (xy -0.435 0.822) (xy -0.454 0.804) (xy -0.472 0.785)
						(xy -0.489 0.765) (xy -0.505 0.744) (xy -0.519 0.722) (xy -0.533 0.7) (xy -0.546 0.677) (xy -0.557 0.653)
						(xy -0.567 0.629) (xy -0.576 0.605) (xy -0.583 0.579) (xy -0.589 0.554) (xy -0.594 0.528) (xy -0.597 0.502)
						(xy -0.599 0.476) (xy -0.6 0.45) (xy -0.6 -0.45) (xy -0.599 -0.476) (xy -0.597 -0.502) (xy -0.594 -0.528)
						(xy -0.589 -0.554) (xy -0.583 -0.579) (xy -0.576 -0.605) (xy -0.567 -0.629) (xy -0.557 -0.653)
						(xy -0.546 -0.677) (xy -0.533 -0.7) (xy -0.519 -0.722) (xy -0.505 -0.744) (xy -0.489 -0.765) (xy -0.472 -0.785)
						(xy -0.454 -0.804) (xy -0.435 -0.822) (xy -0.415 -0.839) (xy -0.394 -0.855) (xy -0.372 -0.869)
						(xy -0.35 -0.883) (xy -0.327 -0.896) (xy -0.303 -0.907) (xy -0.279 -0.917) (xy -0.255 -0.926)
						(xy -0.229 -0.933) (xy -0.204 -0.939) (xy -0.178 -0.944) (xy -0.152 -0.947) (xy -0.126 -0.949)
						(xy -0.1 -0.95) (xy 1.2 -0.95) (xy 1.2 0.95)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(pad "SH4" smd rect
			(at -1 -1.45 180)
			(size 1.5 1.9)
			(layers "F.Cu" "F.Paste")
			(net 4 "unconnected-(J1-SHIELD4-PadSH4)")
			(pinfunction "SHIELD4")
			(pintype "passive")
		)
		(pad "SH5" smd rect
			(at 1 -1.45 180)
			(size 1.5 1.9)
			(layers "F.Cu" "F.Paste")
			(net 41 "unconnected-(J1-SHIELD5-PadSH5)")
			(pinfunction "SHIELD5")
			(pintype "passive")
		)
		(pad "SH6" thru_hole custom
			(at 3.5 -1.45 180)
			(size 1.2 1.9)
			(drill oval 0.6 1.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "unconnected-(J1-SHIELD6-PadSH6)")
			(pinfunction "SHIELD6")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -1.2 0.95) (xy 0.1 0.95) (xy 0.126 0.949) (xy 0.152 0.947) (xy 0.178 0.944) (xy 0.204 0.939)
						(xy 0.229 0.933) (xy 0.255 0.926) (xy 0.279 0.917) (xy 0.303 0.907) (xy 0.327 0.896) (xy 0.35 0.883)
						(xy 0.372 0.869) (xy 0.394 0.855) (xy 0.415 0.839) (xy 0.435 0.822) (xy 0.454 0.804) (xy 0.472 0.785)
						(xy 0.489 0.765) (xy 0.505 0.744) (xy 0.519 0.722) (xy 0.533 0.7) (xy 0.546 0.677) (xy 0.557 0.653)
						(xy 0.567 0.629) (xy 0.576 0.605) (xy 0.583 0.579) (xy 0.589 0.554) (xy 0.594 0.528) (xy 0.597 0.502)
						(xy 0.599 0.476) (xy 0.6 0.45) (xy 0.6 -0.45) (xy 0.599 -0.476) (xy 0.597 -0.502) (xy 0.594 -0.528)
						(xy 0.589 -0.554) (xy 0.583 -0.579) (xy 0.576 -0.605) (xy 0.567 -0.629) (xy 0.557 -0.653) (xy 0.546 -0.677)
						(xy 0.533 -0.7) (xy 0.519 -0.722) (xy 0.505 -0.744) (xy 0.489 -0.765) (xy 0.472 -0.785) (xy 0.454 -0.804)
						(xy 0.435 -0.822) (xy 0.415 -0.839) (xy 0.394 -0.855) (xy 0.372 -0.869) (xy 0.35 -0.883) (xy 0.327 -0.896)
						(xy 0.303 -0.907) (xy 0.279 -0.917) (xy 0.255 -0.926) (xy 0.229 -0.933) (xy 0.204 -0.939) (xy 0.178 -0.944)
						(xy 0.152 -0.947) (xy 0.126 -0.949) (xy 0.1 -0.95) (xy -1.2 -0.95) (xy -1.2 0.95)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 153.797 70.104)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R3"
			(at -3.81 -0.381 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "design_micro.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "Net-(D1-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 186.69 72.39)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "⌀ M3"
			(at -6.477 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 131.191 90.17 180)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R6"
			(at 0.127 2.159 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 4.191 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "design_micro.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/nRESET")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 122.936 73.66 180)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U2"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Reg_Linear_3.3V_1A"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117I.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3.3V 1A Linear regulator from Diodes Incorporated in SOT-223-3 package"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223*TabPin2*")
		(sheetname "/")
		(sheetfile "design_micro.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.15 -2.3 180)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -3.15 0 180)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3.3V")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "2" smd rect
			(at 3.15 0 180)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3.3V")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" smd rect
			(at -3.15 2.3 180)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+5V")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 92.71 114.3)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "⌀ M3"
			(at 6.35 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "fab:C_1206"
		(layer "F.Cu")
		(at 122.936 79.629)
		(descr "Capacitor SMD 1206, hand soldering")
		(tags "capacitor 1206")
		(property "Reference" "C1"
			(at -3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_1206"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/mlcc/UPY-GP_NP0_16V-to-50V_18.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, SMD, 1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*C*")
		(sheetname "/")
		(sheetfile "design_micro.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 140.208 87.884)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R5"
			(at -3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "design_micro.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/SCL")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:Display_128x64_096_I2C"
		(layer "B.Cu")
		(at 139.827 81.661 180)
		(descr "Display 0.96\" OLED 128x64 pixel with SSD1306 controller and I2C interface")
		(tags "display OLED SSD1306 128x64")
		(property "Reference" "J4"
			(at -0.2286 -10.8712 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at -7.874 -4.699 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "design_micro.kicad_sch")
		(attr through_hole)
		(fp_text user "GND"
			(at -3.81 -2.159 0)
			(layer "B.SilkS")
		)
		(fp_text user "VDD"
			(at -1.27 -2.159 0)
			(layer "B.SilkS")
		)
		(fp_text user "SDA"
			(at 3.937 -2.159 0)
			(layer "B.SilkS")
		)
		(fp_text user "SCL"
			(at 1.27 -2.159 0)
			(layer "B.SilkS")
		)
		(pad "" np_thru_hole oval
			(at -11.176 -23.749 180)
			(size 3.8 2.9)
			(drill oval 3.8 2.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at -11.176 -0.635 180)
			(size 3.8 2.9)
			(drill oval 3.8 2.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 11.176 -23.749 180)
			(size 3.8 2.9)
			(drill oval 3.8 2.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 11.176 -0.635 180)
			(size 3.8 2.9)
			(drill oval 3.8 2.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at -3.81 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -1.27 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "+3.3V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 1.27 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 3.81 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/SDA")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(gr_arc
		(start 186.69 68.58)
		(mid 189.384077 69.695923)
		(end 190.5 72.39)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 190.5 114.3)
		(mid 189.384077 116.994077)
		(end 186.69 118.11)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 92.71 118.11)
		(mid 90.015923 116.994077)
		(end 88.9 114.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.71 68.58)
		(end 186.69 68.58)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.5 114.3)
		(end 190.5 72.39)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.9 114.3)
		(end 88.9 72.39)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 88.9 72.39)
		(mid 90.015923 69.695923)
		(end 92.71 68.58)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 186.69 118.11)
		(end 92.71 118.11)
		(layer "Edge.Cuts")
	)
	(gr_text "VREG"
		(at 117.602 70.612 0)
		(layer "F.SilkS")
	)
	(gr_text "10k"
		(at 144.653 87.884 0)
		(layer "F.SilkS")
	)
	(gr_text "Documentation"
		(at 165.1 81.915 0)
		(layer "F.SilkS")
	)
	(gr_text "3.3V"
		(at 117.221 76.962 0)
		(layer "F.SilkS")
	)
	(gr_text "[PA15]"
		(at 163.195 70.612 0)
		(layer "F.SilkS")
	)
	(gr_text "1uF"
		(at 122.936 81.915 0)
		(layer "F.SilkS")
	)
	(gr_text "1k"
		(at 153.797 72.136 0)
		(layer "F.SilkS")
	)
	(gr_text "MIT's Center for Bits and Atoms\nQuentin Bolsée, 2025"
		(at 157.353 116.84 0)
		(layer "F.SilkS")
	)
	(gr_text "10k"
		(at 142.875 84.836 0)
		(layer "F.SilkS")
	)
	(gr_text "1uF"
		(at 129.54 96.393 0)
		(layer "F.SilkS")
	)
	(gr_text "If at first you don't succeed,\nfind out why"
		(at 97.79 117.094 0)
		(layer "F.SilkS")
	)
	(gr_text "JTAG/SWD"
		(at 149.86 111.76 0)
		(layer "F.SilkS")
	)
	(gr_text "#define PIN_LED 15\n\nvoid setup() {\n  pinMode(PIN_LED, OUTPUT);\n}\n\nvoid loop() {\n  digitalWrite(PIN_LED, HIGH);\n  delay(500);\n  digitalWrite(PIN_LED, LOW);\n  delay(500);\n}\n"
		(at 91.948 102.87 0)
		(layer "F.SilkS")
	)
	(gr_text "blink_D21.ino"
		(at 91.313 81.915 0)
		(layer "F.SilkS")
	)
	(gr_text "ATSAMD21E"
		(at 148.717 96.393 0)
		(layer "F.SilkS")
	)
	(gr_text "0.96{dblquote} OLED module"
		(at 153.543 108.585 0)
		(layer "B.SilkS")
	)
	(gr_text "3.7{dblquote} / 93.98mm"
		(at 119.38 72.009 0)
		(layer "B.SilkS")
	)
	(gr_text "Q4 [PA06]"
		(at 162.56 99.06 0)
		(layer "B.SilkS")
	)
	(gr_text "Q3 [PA05]"
		(at 182.88 99.06 0)
		(layer "B.SilkS")
	)
	(gr_text "1.65{dblquote} / 41.91mm"
		(at 90.932 107.696 270)
		(layer "B.SilkS")
	)
	(gr_text "Q0 [PA02]"
		(at 98.298 92.71 0)
		(layer "B.SilkS")
	)
	(gr_text "HTMAA 2025 - QPAD21"
		(at 139.7 116.459 0)
		(layer "B.SilkS")
	)
	(gr_text "Q5 [PA07]"
		(at 172.72 89.027 0)
		(layer "B.SilkS")
	)
	(gr_text "Q2 [PA04]"
		(at 172.72 109.22 0)
		(layer "B.SilkS")
	)
	(gr_text "Q1 [PA03]"
		(at 111.125 101.6 0)
		(layer "B.SilkS")
	)
	(embedded_fonts no)
)
