(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(J1-SBU1-PadA8)")
	(net 2 "unconnected-(J1-SBU2-PadB8)")
	(net 3 "unconnected-(J1-SHIELD1-PadSH1)")
	(net 4 "unconnected-(J1-SHIELD3-PadSH3)")
	(net 5 "unconnected-(J1-SHIELD2-PadSH2)")
	(net 6 "unconnected-(J1-SHIELD4-PadSH4)")
	(net 7 "GND")
	(net 8 "+3.3V")
	(net 9 "+5V")
	(net 10 "Net-(U1-VDDCORE)")
	(net 11 "/DATA+")
	(net 12 "Net-(J1-CC2)")
	(net 13 "/DATA-")
	(net 14 "Net-(J1-CC1)")
	(net 15 "unconnected-(J2-Pin_8-Pad8)")
	(net 16 "/nRESET")
	(net 17 "/SWDIO")
	(net 18 "unconnected-(J2-Pin_6-Pad6)")
	(net 19 "/SWCLK")
	(net 20 "unconnected-(J2-Pin_7-Pad7)")
	(net 21 "/SDA")
	(net 22 "/SCL")
	(net 23 "/TOUCH2")
	(net 24 "unconnected-(U1-PA23-Pad22)")
	(net 25 "unconnected-(U1-PA14-Pad15)")
	(net 26 "unconnected-(U1-PA19-Pad20)")
	(net 27 "/TOUCH3")
	(net 28 "unconnected-(U1-PA27-Pad25)")
	(net 29 "unconnected-(U1-PA10-Pad13)")
	(net 30 "unconnected-(U1-PA01-Pad2)")
	(net 31 "unconnected-(U1-PA28-Pad27)")
	(net 32 "unconnected-(U1-PA11-Pad14)")
	(net 33 "/TOUCH4")
	(net 34 "unconnected-(U1-PA09-Pad12)")
	(net 35 "/TOUCH1")
	(net 36 "/TOUCH0")
	(net 37 "unconnected-(U1-PA22-Pad21)")
	(net 38 "unconnected-(U1-PA08-Pad11)")
	(net 39 "/TOUCH5")
	(net 40 "unconnected-(U1-PA18-Pad19)")
	(net 41 "/LED")
	(net 42 "unconnected-(U1-PA00-Pad1)")
	(net 43 "Net-(D1-K)")
	(footprint "footprints:MODULE_DM-OLED096-636"
		(layer "F.Cu")
		(at 139.7 93.14)
		(property "Reference" "J4"
			(at -10.414 -6.272 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0.635 13.97 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr through_hole allow_missing_courtyard)
		(pad "1" thru_hole rect
			(at -3.81 -11.5)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -1.27 -11.5)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "+3.3V")
			(pinfunction "Pin_2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at 1.27 -11.5)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 -11.5)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/SDA")
			(pinfunction "Pin_4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "S1" thru_hole circle
			(at -11 -11)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "S2" thru_hole circle
			(at 11 -11)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "S3" thru_hole circle
			(at 11 11)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "S4" thru_hole circle
			(at -11 11)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/Users/Quentin/Documents/KiCad/9.0/3dmodels/DM-OLED096-636.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "fab:PinHeader_2x05_P1.27mm_Vertical_SMD"
		(layer "F.Cu")
		(at 139.7 111.76 -90)
		(descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
		(tags "Surface mounted pin header SMD 2x05 1.27mm double row")
		(property "Reference" "J2"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_PinHeader_2x05_P1.27mm_Vertical_SMD"
			(at 0 4.235 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/20021121.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 10 position 0.050\" (1.27mm)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*2x05*")
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.95 -2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.95 -2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/SWDIO")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.95 -1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.95 -1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/SWCLK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.95 0 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.95 0 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(J2-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive+no_connect")
		)
		(pad "7" smd rect
			(at -1.95 1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(J2-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 1.95 1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "unconnected-(J2-Pin_8-Pad8)")
			(pinfunction "Pin_8")
			(pintype "passive+no_connect")
		)
		(pad "9" smd rect
			(at -1.95 2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 1.95 2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/nRESET")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:MOLEX_2137160001"
		(layer "F.Cu")
		(at 139.7 68.58 180)
		(property "Reference" "J1"
			(at 0 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "2137160001"
			(at 9.2825 -11.275 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Molex"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "OPTION" "MOLEX_CONFIG"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/2137160001/Molex/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "B"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/2137160001/Molex/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "2137160001"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "USB-C (USB TYPE-C) USB 2.0 Receptacle Connector 24 (16+8 Dummy) Position Through Hole, Right Angle"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Molex"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.36mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr through_hole)
		(fp_text user "PCB Edge"
			(at 5.5 -0.25 0)
			(layer "F.Fab")
		)
		(pad "A1" thru_hole custom
			(at -2.975 -7.65 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "GND1")
			(pintype "power_in")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.15 1.06281) (xy -0.15 0.287) (xy -0.2 0.255) (xy -0.242 0.216) (xy -0.276 0.17) (xy -0.302 0.119)
						(xy -0.318 0.064) (xy -0.324 0.007) (xy -0.32 -0.05) (xy -0.306 -0.106) (xy -0.283 -0.158) (xy -0.251 -0.205)
						(xy -0.211 -0.246) (xy -0.164 -0.279) (xy -0.112 -0.304) (xy -0.057 -0.319) (xy 0 -0.324) (xy 0.057 -0.319)
						(xy 0.112 -0.304) (xy 0.164 -0.279) (xy 0.211 -0.246) (xy 0.251 -0.205) (xy 0.283 -0.158) (xy 0.306 -0.106)
						(xy 0.32 -0.05) (xy 0.324 0.007) (xy 0.318 0.064) (xy 0.302 0.119) (xy 0.276 0.17) (xy 0.242 0.216)
						(xy 0.2 0.255) (xy 0.15 0.287) (xy 0.15 1.063) (xy 0.2 1.095) (xy 0.242 1.134) (xy 0.276 1.18)
						(xy 0.302 1.231) (xy 0.318 1.286) (xy 0.324 1.343) (xy 0.32 1.4) (xy 0.306 1.456) (xy 0.283 1.508)
						(xy 0.251 1.555) (xy 0.211 1.596) (xy 0.164 1.629) (xy 0.112 1.654) (xy 0.057 1.669) (xy 0 1.674)
						(xy -0.057 1.669) (xy -0.112 1.654) (xy -0.164 1.629) (xy -0.211 1.596) (xy -0.251 1.555) (xy -0.283 1.508)
						(xy -0.306 1.456) (xy -0.32 1.4) (xy -0.324 1.343) (xy -0.318 1.286) (xy -0.302 1.231) (xy -0.276 1.18)
						(xy -0.242 1.134) (xy -0.2 1.095) (xy -0.15 1.063) (xy -0.15 1.06281)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(pad "A4" thru_hole custom
			(at -2.125 -7.65 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 9 "+5V")
			(pinfunction "VBUS1")
			(pintype "power_in")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.15 1.06281) (xy -0.15 0.287) (xy -0.2 0.255) (xy -0.242 0.216) (xy -0.276 0.17) (xy -0.302 0.119)
						(xy -0.318 0.064) (xy -0.324 0.007) (xy -0.32 -0.05) (xy -0.306 -0.106) (xy -0.283 -0.158) (xy -0.251 -0.205)
						(xy -0.211 -0.246) (xy -0.164 -0.279) (xy -0.112 -0.304) (xy -0.057 -0.319) (xy 0 -0.324) (xy 0.057 -0.319)
						(xy 0.112 -0.304) (xy 0.164 -0.279) (xy 0.211 -0.246) (xy 0.251 -0.205) (xy 0.283 -0.158) (xy 0.306 -0.106)
						(xy 0.32 -0.05) (xy 0.324 0.007) (xy 0.318 0.064) (xy 0.302 0.119) (xy 0.276 0.17) (xy 0.242 0.216)
						(xy 0.2 0.255) (xy 0.15 0.287) (xy 0.15 1.063) (xy 0.2 1.095) (xy 0.242 1.134) (xy 0.276 1.18)
						(xy 0.302 1.231) (xy 0.318 1.286) (xy 0.324 1.343) (xy 0.32 1.4) (xy 0.306 1.456) (xy 0.283 1.508)
						(xy 0.251 1.555) (xy 0.211 1.596) (xy 0.164 1.629) (xy 0.112 1.654) (xy 0.057 1.669) (xy 0 1.674)
						(xy -0.057 1.669) (xy -0.112 1.654) (xy -0.164 1.629) (xy -0.211 1.596) (xy -0.251 1.555) (xy -0.283 1.508)
						(xy -0.306 1.456) (xy -0.32 1.4) (xy -0.324 1.343) (xy -0.318 1.286) (xy -0.302 1.231) (xy -0.276 1.18)
						(xy -0.242 1.134) (xy -0.2 1.095) (xy -0.15 1.063) (xy -0.15 1.06281)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(pad "A5" thru_hole circle
			(at -1.275 -7.65 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 14 "Net-(J1-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" thru_hole circle
			(at -0.425 -7.65 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 11 "/DATA+")
			(pinfunction "DA+")
			(pintype "bidirectional")
		)
		(pad "A7" thru_hole circle
			(at 0.425 -7.65 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 13 "/DATA-")
			(pinfunction "DA-")
			(pintype "bidirectional")
		)
		(pad "A8" thru_hole circle
			(at 1.275 -7.65 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "unconnected-(J1-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional")
		)
		(pad "A9" thru_hole custom
			(at 2.125 -7.65 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 9 "+5V")
			(pinfunction "VBUS2")
			(pintype "power_in")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.15 0.28719) (xy -0.15 1.063) (xy -0.2 1.095) (xy -0.242 1.134) (xy -0.276 1.18) (xy -0.302 1.231)
						(xy -0.318 1.286) (xy -0.324 1.343) (xy -0.32 1.4) (xy -0.306 1.456) (xy -0.283 1.508) (xy -0.251 1.555)
						(xy -0.211 1.596) (xy -0.164 1.629) (xy -0.112 1.654) (xy -0.057 1.669) (xy 0 1.674) (xy 0.057 1.669)
						(xy 0.112 1.654) (xy 0.164 1.629) (xy 0.211 1.596) (xy 0.251 1.555) (xy 0.283 1.508) (xy 0.306 1.456)
						(xy 0.32 1.4) (xy 0.324 1.343) (xy 0.318 1.286) (xy 0.302 1.231) (xy 0.276 1.18) (xy 0.242 1.134)
						(xy 0.2 1.095) (xy 0.15 1.063) (xy 0.15 0.287) (xy 0.2 0.255) (xy 0.242 0.216) (xy 0.276 0.17)
						(xy 0.302 0.119) (xy 0.318 0.064) (xy 0.324 0.007) (xy 0.32 -0.05) (xy 0.306 -0.106) (xy 0.283 -0.158)
						(xy 0.251 -0.205) (xy 0.211 -0.246) (xy 0.164 -0.279) (xy 0.112 -0.304) (xy 0.057 -0.319) (xy 0 -0.324)
						(xy -0.057 -0.319) (xy -0.112 -0.304) (xy -0.164 -0.279) (xy -0.211 -0.246) (xy -0.251 -0.205)
						(xy -0.283 -0.158) (xy -0.306 -0.106) (xy -0.32 -0.05) (xy -0.324 0.007) (xy -0.318 0.064) (xy -0.302 0.119)
						(xy -0.276 0.17) (xy -0.242 0.216) (xy -0.2 0.255) (xy -0.15 0.287) (xy -0.15 0.28719)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(pad "A12" thru_hole custom
			(at 2.975 -7.65 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "GND2")
			(pintype "power_in")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.15 1.06281) (xy -0.15 0.287) (xy -0.2 0.255) (xy -0.242 0.216) (xy -0.276 0.17) (xy -0.302 0.119)
						(xy -0.318 0.064) (xy -0.324 0.007) (xy -0.32 -0.05) (xy -0.306 -0.106) (xy -0.283 -0.158) (xy -0.251 -0.205)
						(xy -0.211 -0.246) (xy -0.164 -0.279) (xy -0.112 -0.304) (xy -0.057 -0.319) (xy 0 -0.324) (xy 0.057 -0.319)
						(xy 0.112 -0.304) (xy 0.164 -0.279) (xy 0.211 -0.246) (xy 0.251 -0.205) (xy 0.283 -0.158) (xy 0.306 -0.106)
						(xy 0.32 -0.05) (xy 0.324 0.007) (xy 0.318 0.064) (xy 0.302 0.119) (xy 0.276 0.17) (xy 0.242 0.216)
						(xy 0.2 0.255) (xy 0.15 0.287) (xy 0.15 1.063) (xy 0.2 1.095) (xy 0.242 1.134) (xy 0.276 1.18)
						(xy 0.302 1.231) (xy 0.318 1.286) (xy 0.324 1.343) (xy 0.32 1.4) (xy 0.306 1.456) (xy 0.283 1.508)
						(xy 0.251 1.555) (xy 0.211 1.596) (xy 0.164 1.629) (xy 0.112 1.654) (xy 0.057 1.669) (xy 0 1.674)
						(xy -0.057 1.669) (xy -0.112 1.654) (xy -0.164 1.629) (xy -0.211 1.596) (xy -0.251 1.555) (xy -0.283 1.508)
						(xy -0.306 1.456) (xy -0.32 1.4) (xy -0.324 1.343) (xy -0.318 1.286) (xy -0.302 1.231) (xy -0.276 1.18)
						(xy -0.242 1.134) (xy -0.2 1.095) (xy -0.15 1.063) (xy -0.15 1.06281)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(pad "B1" thru_hole circle
			(at 2.975 -6.3 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "GND3")
			(pintype "power_in")
		)
		(pad "B4" thru_hole circle
			(at 2.125 -6.3 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 9 "+5V")
			(pinfunction "VBUS3")
			(pintype "power_in")
		)
		(pad "B5" thru_hole circle
			(at 1.275 -6.3 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 12 "Net-(J1-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" thru_hole circle
			(at 0.425 -6.3 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 11 "/DATA+")
			(pinfunction "DB+")
			(pintype "bidirectional")
		)
		(pad "B7" thru_hole circle
			(at -0.425 -6.3 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 13 "/DATA-")
			(pinfunction "DB-")
			(pintype "bidirectional")
		)
		(pad "B8" thru_hole circle
			(at -1.275 -6.3 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "unconnected-(J1-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional")
		)
		(pad "B9" thru_hole circle
			(at -2.125 -6.3 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 9 "+5V")
			(pinfunction "VBUS4")
			(pintype "power_in")
		)
		(pad "B12" thru_hole circle
			(at -2.975 -6.3 180)
			(size 0.648 0.648)
			(drill 0.4)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 7 "GND")
			(pinfunction "GND4")
			(pintype "power_in")
		)
		(pad "SH1" thru_hole oval
			(at -4.32 -3 180)
			(size 1.3 2.5)
			(drill oval 0.7 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(J1-SHIELD1-PadSH1)")
			(pinfunction "SHIELD1")
			(pintype "passive")
			(solder_mask_margin 0.0762)
		)
		(pad "SH2" thru_hole oval
			(at 4.32 -3 180)
			(size 1.3 2.5)
			(drill oval 0.7 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J1-SHIELD2-PadSH2)")
			(pinfunction "SHIELD2")
			(pintype "passive")
			(solder_mask_margin 0.0762)
		)
		(pad "SH3" thru_hole oval
			(at -4.32 -7.15 180)
			(size 1.3 3.2)
			(drill oval 0.7 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(J1-SHIELD3-PadSH3)")
			(pinfunction "SHIELD3")
			(pintype "passive")
			(solder_mask_margin 0.0762)
		)
		(pad "SH4" thru_hole oval
			(at 4.32 -7.15 180)
			(size 1.3 3.2)
			(drill oval 0.7 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J1-SHIELD4-PadSH4)")
			(pinfunction "SHIELD4")
			(pintype "passive")
			(solder_mask_margin 0.0762)
		)
		(embedded_fonts no)
		(model "C:/Users/Quentin/Documents/KiCad/9.0/3dmodels/2137160001.step"
			(offset
				(xyz 0 -0.4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "fab:TQFP-32_7x7mm_P0.8mm"
		(layer "F.Cu")
		(at 139.7 96.266 90)
		(descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "QFP 0.8")
		(property "Reference" "U1"
			(at 1.651 6.604 180)
			(layer "F.SilkS")
		)
		(property "Value" "Microcontroller_ATSAMD21E17A-AUT"
			(at 0 6.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_DataSheet_DS40001882F.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash, 4K SRAM, TQFP-32"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TQFP*7x7mm*P0.8mm*")
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.318 -2.806 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "unconnected-(U1-PA00-Pad1)")
			(pinfunction "PA00")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -4.318 -2.006 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "unconnected-(U1-PA01-Pad2)")
			(pinfunction "PA01")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -4.318 -1.206 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "/TOUCH0")
			(pinfunction "PA02")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -4.318 -0.406 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/TOUCH1")
			(pinfunction "PA03")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -4.318 0.394 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "/TOUCH2")
			(pinfunction "PA04")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -4.318 1.194 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/TOUCH3")
			(pinfunction "PA05")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -4.318 1.994 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "/TOUCH4")
			(pinfunction "PA06")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -4.318 2.794 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "/TOUCH5")
			(pinfunction "PA07")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -2.806 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "+3.3V")
			(pinfunction "VDDANA")
			(pintype "power_in")
		)
		(pad "10" smd rect
			(at -2.006 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd rect
			(at -1.206 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "unconnected-(U1-PA08-Pad11)")
			(pinfunction "PA08")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -0.406 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "unconnected-(U1-PA09-Pad12)")
			(pinfunction "PA09")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 0.394 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "unconnected-(U1-PA10-Pad13)")
			(pinfunction "PA10")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at 1.194 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "unconnected-(U1-PA11-Pad14)")
			(pinfunction "PA11")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at 1.994 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "unconnected-(U1-PA14-Pad15)")
			(pinfunction "PA14")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at 2.794 4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/LED")
			(pinfunction "PA15")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at 4.318 2.8 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/SDA")
			(pinfunction "PA16")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at 4.318 2 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/SCL")
			(pinfunction "PA17")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at 4.318 1.2 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "unconnected-(U1-PA18-Pad19)")
			(pinfunction "PA18")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at 4.318 0.4 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(U1-PA19-Pad20)")
			(pinfunction "PA19")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 4.318 -0.4 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "unconnected-(U1-PA22-Pad21)")
			(pinfunction "PA22")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 4.318 -1.2 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "unconnected-(U1-PA23-Pad22)")
			(pinfunction "PA23")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at 4.318 -2 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/DATA-")
			(pinfunction "PA24")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 4.318 -2.8 90)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/DATA+")
			(pinfunction "PA25")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 2.7936 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "unconnected-(U1-PA27-Pad25)")
			(pinfunction "PA27")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 1.9936 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/nRESET")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "27" smd rect
			(at 1.1936 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "unconnected-(U1-PA28-Pad27)")
			(pinfunction "PA28")
			(pintype "bidirectional")
		)
		(pad "28" smd rect
			(at 0.3936 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at -0.4064 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(U1-VDDCORE)")
			(pinfunction "VDDCORE")
			(pintype "power_out")
		)
		(pad "30" smd rect
			(at -1.2064 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "+3.3V")
			(pinfunction "VDDIN")
			(pintype "power_in")
		)
		(pad "31" smd rect
			(at -2.0064 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/SWCLK")
			(pinfunction "PA30")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at -2.8064 -4.318 180)
			(size 1.6 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/SWDIO")
			(pinfunction "PA31")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 186.69 113.03)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "⌀ M3"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "fab:C_1206"
		(layer "F.Cu")
		(at 132.302 94.488 -90)
		(descr "Capacitor SMD 1206, hand soldering")
		(tags "capacitor 1206")
		(property "Reference" "C3"
			(at -2.032 2.635 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/mlcc/UPY-GP_NP0_16V-to-50V_18.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, SMD, 1206"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*C*")
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 270)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 270)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(U1-VDDCORE)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 92.71 72.39)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "⌀ M3"
			(at 0 4.318 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "fab:LED_1206"
		(layer "F.Cu")
		(at 159.512 72.898)
		(descr "LED SMD 1206, hand soldering")
		(tags "LED 1206")
		(property "Reference" "D1"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_1206"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*LED*1206*")
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/LED")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 140.462 84.836 180)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R4"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.9k"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/SDA")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 131.826 74.93 -90)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R1"
			(at -3.556 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 270)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(J1-CC2)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 270)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 153.416 72.898)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R3"
			(at 0 -2.032 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "Net-(D1-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 186.69 72.39)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "⌀ M3"
			(at 0 4.318 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "fab:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 122.936 73.66 180)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U2"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Reg_Linear_3.3V_1A"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ1117I.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3.3V 1A Linear regulator from Diodes Incorporated in SOT-223-3 package"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223*TabPin2*")
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.15 -2.3 180)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -3.15 0 180)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "+3.3V")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "2" smd rect
			(at 3.15 0 180)
			(size 2 3.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "+3.3V")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" smd rect
			(at -3.15 2.3 180)
			(size 2 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "+5V")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 92.71 113.03)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "⌀ M3"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "fab:C_1206"
		(layer "F.Cu")
		(at 122.936 79.629)
		(descr "Capacitor SMD 1206, hand soldering")
		(tags "capacitor 1206")
		(property "Reference" "C1"
			(at -3.937 0.635 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_1206"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.yageo.com/upload/media/product/productsearch/datasheet/mlcc/UPY-GP_NP0_16V-to-50V_18.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, SMD, 1206"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*C*")
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 147.574 74.93 90)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R2"
			(at 3.556 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 90)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(J1-CC1)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 90)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:R_1206"
		(layer "F.Cu")
		(at 138.684 87.376 180)
		(descr "Resistor SMD 1206, hand soldering")
		(tags "resistor 1206")
		(property "Reference" "R5"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.9k"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*R*1206*")
		(sheetname "/")
		(sheetfile "Qpad21.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/SCL")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 186.69 68.58)
		(mid 189.384077 69.695923)
		(end 190.5 72.39)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 190.5 113.03)
		(mid 189.384077 115.724077)
		(end 186.69 116.84)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 92.71 116.84)
		(mid 90.015923 115.724077)
		(end 88.9 113.03)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.71 68.58)
		(end 186.69 68.58)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 190.5 113.03)
		(end 190.5 72.39)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.9 113.03)
		(end 88.9 72.39)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 88.9 72.39)
		(mid 90.015923 69.695923)
		(end 92.71 68.58)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.71 116.84)
		(end 186.69 116.84)
		(layer "Edge.Cuts")
	)
	(gr_text "5.1k"
		(at 130.81 78.486 0)
		(layer "F.SilkS")
	)
	(gr_text "0.96{dblquote} OLED"
		(at 129.667 108.204 0)
		(layer "F.SilkS")
	)
	(gr_text "Q4/PA06"
		(at 163.067999 101.345999 0)
		(layer "F.SilkS")
	)
	(gr_text "VREG"
		(at 117.983 70.358 0)
		(layer "F.SilkS")
	)
	(gr_text "Q3/PA05"
		(at 101.854 108.966 0)
		(layer "F.SilkS")
	)
	(gr_text "QPAD21 - HTMAA 2025"
		(at 162.9664 115.8748 0)
		(layer "F.SilkS")
	)
	(gr_text "5.1k"
		(at 144.78 84.836 0)
		(layer "F.SilkS")
	)
	(gr_text "5.1k"
		(at 148.082 78.486 0)
		(layer "F.SilkS")
	)
	(gr_text "PA15"
		(at 162.814 73.787 0)
		(layer "F.SilkS")
	)
	(gr_text "1uF"
		(at 122.682 81.915 0)
		(layer "F.SilkS")
	)
	(gr_text "1k"
		(at 153.67 75.184 0)
		(layer "F.SilkS")
	)
	(gr_text "Q0/PA02"
		(at 101.854 88.646 0)
		(layer "F.SilkS")
	)
	(gr_text "5.1k"
		(at 143.002 87.376 0)
		(layer "F.SilkS")
	)
	(gr_text "1uF"
		(at 129.413 96.393 0)
		(layer "F.SilkS")
	)
	(gr_text "Q5/PA07"
		(at 175.514 92.456 0)
		(layer "F.SilkS")
	)
	(gr_text "JTAG/SWD"
		(at 147.828 111.76 0)
		(layer "F.SilkS")
	)
	(gr_text "Q2/PA04"
		(at 91.694 98.806 0)
		(layer "F.SilkS")
	)
	(gr_text "3.3V"
		(at 117.856 76.835 0)
		(layer "F.SilkS")
	)
	(gr_text "USB-C"
		(at 139.7 72.009 0)
		(layer "F.SilkS")
	)
	(gr_text "Q1/PA03"
		(at 112.014 98.806 0)
		(layer "F.SilkS")
	)
	(gr_text "ATSAMD21E"
		(at 148.717 96.393 0)
		(layer "F.SilkS")
	)
	(gr_text "Scan for\ndocumentation"
		(at 140.1064 105.6132 0)
		(layer "B.SilkS")
	)
	(gr_text "Quentin Bolsée 2025"
		(at 115.7732 116.1796 0)
		(layer "B.SilkS")
	)
	(gr_text "MIT's Center for Bits and Atoms"
		(at 181.1528 115.824 0)
		(layer "B.SilkS")
	)
	(embedded_fonts no)
)
