(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Device:LED"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode"
				(at 0 0 0)
			)
			(property "Sim.Pins" "1=K 2=A"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*"
				(at 0 0 0)
			)
			(symbol "LED_0_1"
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Switch:SW_Push"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 1.27 2.54 0)
			)
			(property "Value" "SW_Push"
				(at 0 -1.524 0)
			)
			(property "Footprint" ""
				(at 0 5.08 0)
			)
			(property "Datasheet" "~"
				(at 0 5.08 0)
			)
			(property "Description" "Push button switch, generic, two pins"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button"
				(at 0 0 0)
			)
			(symbol "SW_Push_0_1"
				(circle
					(center -2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 3.048)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.27) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "xiao:xiao"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -10.16 15.24 0)
			)
			(property "Value" "xiao"
				(at -8.89 12.7 0)
			)
			(property "Footprint" ""
				(at -8.89 5.08 0)
			)
			(property "Datasheet" ""
				(at -8.89 5.08 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "xiao_0_1"
				(rectangle
					(start -10.16 11.43)
					(end 10.16 -11.43)
					(fill
						(type none)
					)
				)
			)
			(symbol "xiao_1_1"
				(pin bidirectional line
					(at -12.7 7.62 0)
					(length 2.54)
					(name "A2")
					(number "1")
				)
				(pin bidirectional line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "A4")
					(number "2")
				)
				(pin bidirectional line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "A10")
					(number "3")
				)
				(pin bidirectional line
					(at -12.7 0 0)
					(length 2.54)
					(name "A11")
					(number "4")
				)
				(pin bidirectional line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "A8_SDA")
					(number "5")
				)
				(pin bidirectional line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "A9_SCL")
					(number "6")
				)
				(pin bidirectional line
					(at -12.7 -7.62 0)
					(length 2.54)
					(name "B8_TX")
					(number "7")
				)
				(pin input line
					(at -3.81 13.97 270)
					(length 2.54)
					(name "A31_SWDIO")
					(number "15")
				)
				(pin input line
					(at -1.27 13.97 270)
					(length 2.54)
					(name "A30_SWCLK")
					(number "16")
				)
				(pin input line
					(at 1.27 13.97 270)
					(length 2.54)
					(name "RESET")
					(number "17")
				)
				(pin power_out line
					(at 3.81 13.97 270)
					(length 2.54)
					(name "GND")
					(number "18")
				)
				(pin power_out line
					(at 12.7 7.62 180)
					(length 2.54)
					(name "5V")
					(number "14")
				)
				(pin power_out line
					(at 12.7 5.08 180)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin power_out line
					(at 12.7 2.54 180)
					(length 2.54)
					(name "3V3")
					(number "12")
				)
				(pin bidirectional line
					(at 12.7 0 180)
					(length 2.54)
					(name "A6_MOSI")
					(number "11")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "A5_MISO")
					(number "10")
				)
				(pin bidirectional line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "A7_SCK")
					(number "9")
				)
				(pin bidirectional line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "B9_RX")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
	)
	(wire
		(pts
			(xy 72.39 83.82) (xy 73.66 83.82)
		)
	)
	(wire
		(pts
			(xy 105.41 110.49) (xy 105.41 88.9)
		)
	)
	(wire
		(pts
			(xy 72.39 86.36) (xy 73.66 86.36)
		)
	)
	(wire
		(pts
			(xy 72.39 68.58) (xy 72.39 83.82)
		)
	)
	(wire
		(pts
			(xy 105.41 88.9) (xy 99.06 88.9)
		)
	)
	(wire
		(pts
			(xy 72.39 118.11) (xy 72.39 86.36)
		)
	)
	(wire
		(pts
			(xy 105.41 68.58) (xy 72.39 68.58)
		)
	)
	(wire
		(pts
			(xy 105.41 76.2) (xy 105.41 78.74)
		)
	)
	(wire
		(pts
			(xy 81.28 118.11) (xy 72.39 118.11)
		)
	)
	(wire
		(pts
			(xy 91.44 118.11) (xy 105.41 118.11)
		)
	)
	(wire
		(pts
			(xy 99.06 86.36) (xy 105.41 86.36)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 86.36 118.11 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW1"
			(at 86.36 110.49 0)
		)
		(property "Value" "SW_Push"
			(at 86.36 113.03 0)
		)
		(property "Footprint" "Button_Switch_SMD:SW_SPST_TL3342"
			(at 86.36 113.03 0)
		)
		(property "Datasheet" "~"
			(at 86.36 113.03 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 86.36 118.11 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "xiao:xiao")
		(at 86.36 91.44 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 86.36 105.41 0)
		)
		(property "Value" "xiao"
			(at 86.36 107.95 0)
		)
		(property "Footprint" "RF_Module:MCU_Seeed_ESP32C3"
			(at 77.47 86.36 0)
		)
		(property "Datasheet" ""
			(at 77.47 86.36 0)
		)
		(property "Description" ""
			(at 86.36 91.44 0)
		)
		(pin "1")
		(pin "3")
		(pin "14")
		(pin "13")
		(pin "6")
		(pin "12")
		(pin "16")
		(pin "15")
		(pin "11")
		(pin "7")
		(pin "5")
		(pin "4")
		(pin "2")
		(pin "17")
		(pin "10")
		(pin "9")
		(pin "8")
		(pin "18")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 105.41 114.3 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 107.95 113.0299 0)
		)
		(property "Value" "10k"
			(at 107.95 115.5699 0)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 103.632 114.3 90)
		)
		(property "Datasheet" "~"
			(at 105.41 114.3 0)
		)
		(property "Description" "Resistor"
			(at 105.41 114.3 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 105.41 72.39 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 107.95 71.1199 0)
		)
		(property "Value" "100"
			(at 107.95 73.6599 0)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 103.632 72.39 90)
		)
		(property "Datasheet" "~"
			(at 105.41 72.39 0)
		)
		(property "Description" "Resistor"
			(at 105.41 72.39 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:LED")
		(at 105.41 82.55 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 109.22 82.8674 90)
		)
		(property "Value" "LED"
			(at 109.22 85.4074 90)
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric"
			(at 105.41 82.55 0)
		)
		(property "Datasheet" "~"
			(at 105.41 82.55 0)
		)
		(property "Description" "Light emitting diode"
			(at 105.41 82.55 0)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 105.41 82.55 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
