(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_57557573)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(M1-GND-Pad21)")
	(net 2 "unconnected-(M1-D--Pad23)")
	(net 3 "unconnected-(M1-D+-Pad24)")
	(net 4 "unconnected-(M1-MTDO-Pad22)")
	(net 5 "/BAT_VIN")
	(net 6 "unconnected-(M1-THERMAL-Pad25)")
	(net 7 "unconnected-(M1-MTDI-Pad17)")
	(net 8 "unconnected-(M1-D7-Pad8)")
	(net 9 "unconnected-(M1-MTMS-Pad19)")
	(net 10 "unconnected-(M1-MTCK-Pad20)")
	(net 11 "unconnected-(M1-5V-Pad14)")
	(net 12 "unconnected-(M1-EN-Pad18)")
	(net 13 "unconnected-(M1-D9-Pad10)")
	(net 14 "unconnected-(M1-BAT_GND-Pad15)")
	(net 15 "/GND")
	(net 16 "/LED")
	(net 17 "/VCC")
	(net 18 "/CS")
	(net 19 "/MOSI")
	(net 20 "/RST")
	(net 21 "/CLK")
	(net 22 "/DC")
	(net 23 "/SCL")
	(net 24 "/BUSY")
	(net 25 "/SDA")
	(footprint "fab:Jumper_1206"
		(layer "F.Cu")
		(at 113.87 83.185)
		(descr "Jumper, based on SMD 1206 resistor")
		(tags "jumper smd 1206")
		(property "Reference" "JP3"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jumper_1206"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper based on 0 Ohm 1206 resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper*")
		(sheetname "/")
		(sheetfile "esp32_simple.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/CLK")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/CLK")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:Jumper_1206"
		(layer "F.Cu")
		(at 143.45 71.12 180)
		(descr "Jumper, based on SMD 1206 resistor")
		(tags "jumper smd 1206")
		(property "Reference" "JP2"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jumper_1206"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper based on 0 Ohm 1206 resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper*")
		(sheetname "/")
		(sheetfile "esp32_simple.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/MOSI")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/MOSI")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:Jumper_1206"
		(layer "F.Cu")
		(at 148.45 75.25)
		(descr "Jumper, based on SMD 1206 resistor")
		(tags "jumper smd 1206")
		(property "Reference" "JP4"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jumper_1206"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper based on 0 Ohm 1206 resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper*")
		(sheetname "/")
		(sheetfile "esp32_simple.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/MOSI")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/MOSI")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:Jumper_1206"
		(layer "F.Cu")
		(at 106.25 78.74)
		(descr "Jumper, based on SMD 1206 resistor")
		(tags "jumper smd 1206")
		(property "Reference" "JP5"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jumper_1206"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper based on 0 Ohm 1206 resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper*")
		(sheetname "/")
		(sheetfile "esp32_simple.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/BUSY")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/BUSY")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_01x02_P2.54mm_Vertical_THT_D1mm"
		(layer "F.Cu")
		(at 128.21 82.75 90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_01x02_P2.54mm_Vertical_THT_D1mm"
			(at 0 5.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x02*")
		(sheetname "/")
		(sheetfile "esp32_simple.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/BAT_VIN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/BAT_VIN")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/PinHeader-01x02_P2.54mm_Vertical_THT.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_01x04_P2.54mm_Vertical_THT_D1mm"
		(layer "F.Cu")
		(at 142.96 63.5 90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_01x04_P2.54mm_Vertical_THT_D1mm"
			(at 26.5 5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x04*")
		(sheetname "/")
		(sheetfile "esp32_simple.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/VCC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/SCL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/SDA")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/PinHeader-01x04_P2.54mm_Vertical_THT.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:Diode_Schottky_MiniSMA"
		(layer "F.Cu")
		(at 121.6 82.75)
		(descr "Mini-SMA  Schottky diode footprint")
		(tags "Mini-SMA schottky diode")
		(property "Reference" "D1"
			(at 0 2.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "Diode_Schottky_MiniSMA"
			(at 0 -2.35 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.st.com/content/ccc/resource/technical/document/datasheet/c6/32/d4/4a/28/d3/4b/11/CD00004930.pdf/files/CD00004930.pdf/jcr:content/translations/en.CD00004930.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode with Mini-SMA footprint"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Mini*SMA*")
		(sheetname "/")
		(sheetfile "esp32_simple.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at -1.65 0)
			(size 1.4 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/BAT_VIN")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0)
			(size 1.4 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/BAT_VIN")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "fab:SeeedStudio_XIAO_ESP32S3"
		(layer "F.Cu")
		(at 128.865 68.775)
		(descr "Footprint for Seeed Studio XIAO ESP32S3 module")
		(tags "xiao seeed studio module")
		(property "Reference" "M1"
			(at 0 5.39 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Module_XIAO-ESP32S3"
			(at 0.0025 0.391 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://wiki.seeedstudio.com/xiao_esp32s3_getting_started/"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESP32-C3 Transceiver; 802.11 a/b/g/n (Wi-Fi, WiFi, WLAN), Bluetooth® Smart 4.x Low Energy (BLE) 2.4GHz Evaluation Board"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SeeedStudio?XIAO?ESP32S*")
		(sheetname "/")
		(sheetfile "esp32_simple.kicad_sch")
		(attr smd)
		(fp_text user "BAT"
			(at -5 3.9 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "THERMAL"
			(at 3.5 2.2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "EN"
			(at 0 -6.14 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "MTMS"
			(at 0 -3.6 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "MTDI"
			(at 0 -8.68 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D+"
			(at 2.5 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -4.4 1.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "MTCK"
			(at 2.54 -3.6 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at -4.4 -3.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "MTDO"
			(at 2.54 -8.68 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 2.54 -6.14 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D-"
			(at 0 -1.2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0.0025 2.931 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -7.615 -7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/LED")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "1" smd rect
			(at -7.615 -7.62)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/LED")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at -7.615 -5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/CS")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -7.615 -5.08)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/CS")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at -7.615 -2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/DC")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -7.615 -2.54)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/DC")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at -7.615 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/RST")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -7.615 0)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "/RST")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at -7.615 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/SDA")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -7.615 2.54)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "/SDA")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at -7.615 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/SCL")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -7.615 5.08)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "/SCL")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at -7.615 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/BUSY")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -7.615 7.62)
			(size 3 1.6)
			(drill
				(offset -1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/BUSY")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole circle
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(M1-D7-Pad8)")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at 7.62 7.62)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "unconnected-(M1-D7-Pad8)")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole circle
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/CLK")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at 7.62 5.08)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/CLK")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(M1-D9-Pad10)")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 7.62 2.54)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "unconnected-(M1-D9-Pad10)")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/MOSI")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at 7.62 0)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/MOSI")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at 7.62 -2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/VCC")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "12" smd rect
			(at 7.62 -2.54)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/VCC")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at 7.62 -5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at 7.62 -5.08)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "/GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" thru_hole circle
			(at 7.62 -7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(M1-5V-Pad14)")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 7.62 -7.62)
			(size 3 1.6)
			(drill
				(offset 1 0)
			)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(M1-5V-Pad14)")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at -4.5 -2.3)
			(size 2.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(M1-BAT_GND-Pad15)")
			(pinfunction "BAT_GND")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -4.5 -0.2)
			(size 2.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/BAT_VIN")
			(pinfunction "BAT_VIN")
			(pintype "power_in")
		)
		(pad "17" smd circle
			(at -1.27 -8.68)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "unconnected-(M1-MTDI-Pad17)")
			(pinfunction "MTDI")
			(pintype "input")
		)
		(pad "18" smd circle
			(at -1.27 -6.14)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "unconnected-(M1-EN-Pad18)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "19" smd circle
			(at -1.27 -3.6)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "unconnected-(M1-MTMS-Pad19)")
			(pinfunction "MTMS")
			(pintype "input")
		)
		(pad "20" smd circle
			(at 1.27 -3.6)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "unconnected-(M1-MTCK-Pad20)")
			(pinfunction "MTCK")
			(pintype "input")
		)
		(pad "21" smd circle
			(at 1.27 -6.14)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "unconnected-(M1-GND-Pad21)")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "22" smd circle
			(at 1.27 -8.68)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "unconnected-(M1-MTDO-Pad22)")
			(pinfunction "MTDO")
			(pintype "output")
		)
		(pad "23" smd circle
			(at -1.25 -1.2)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "unconnected-(M1-D--Pad23)")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "24" smd circle
			(at 1.25 -1.2)
			(size 1.2 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "unconnected-(M1-D+-Pad24)")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 1.3 2.3)
			(size 3 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "unconnected-(M1-THERMAL-Pad25)")
			(pinfunction "THERMAL")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/Seeed_XIAO-nRF52840_Sense.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 180)
			)
		)
	)
	(footprint "fab:Jumper_1206"
		(layer "F.Cu")
		(at 113.87 78.74)
		(descr "Jumper, based on SMD 1206 resistor")
		(tags "jumper smd 1206")
		(property "Reference" "JP6"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jumper_1206"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper based on 0 Ohm 1206 resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper*")
		(sheetname "/")
		(sheetfile "esp32_simple.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/BUSY")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/BUSY")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_01x02_P2.54mm_Vertical_THT_D1mm"
		(layer "F.Cu")
		(at 135.71 82.75 90)
		(descr "Through hole straight pin header, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_01x02_P2.54mm_Vertical_THT_D1mm"
			(at 0 5.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Male connector, single row"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x02*")
		(sheetname "/")
		(sheetfile "esp32_simple.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.25 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/PinHeader-01x02_P2.54mm_Vertical_THT.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:PinHeader_01x08_P2.54mm_Vertical_THT_D1.4mm"
		(layer "F.Cu")
		(at 96.52 62.23)
		(descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x08 2.54mm single row")
		(property "Reference" "J1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_01x08_P2.54mm_Vertical_THT_D1.4mm"
			(at 0 20.11 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Through Hole 8 positions 0.100\" (2.54mm)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*PinHeader*1x08*")
		(sheetname "/")
		(sheetfile "esp32_simple.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 2.1 2.1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 2.1 2.1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/MOSI")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 2.1 2.1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/CLK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 2.1 2.1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/CS")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 2.1 2.1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/DC")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 2.1 2.1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/RST")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78)
			(size 2.1 2.1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/BUSY")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/PinHeader-01x08_P2.54mm_Vertical_THT.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fab:Jumper_1206"
		(layer "F.Cu")
		(at 106.25 83.185 180)
		(descr "Jumper, based on SMD 1206 resistor")
		(tags "jumper smd 1206")
		(property "Reference" "JP1"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jumper_1206"
			(at 0 -1.905 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper based on 0 Ohm 1206 resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper*")
		(sheetname "/")
		(sheetfile "esp32_simple.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/CLK")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 180)
			(size 1.4 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/CLK")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${FAB}/fab.3dshapes/R_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 89 90.25)
		(end 89 58.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.5 90.25)
		(end 89 90.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89 58.25)
		(end 118.5 58.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.5 58.25)
		(end 154.5 58.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 154.5 58.25)
		(end 154.5 90.25)
		(layer "Edge.Cuts")
	)
	(zone
		(net 15)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 84.5 55) (xy 85 95.5) (xy 166.75 94.25) (xy 167.5 54.25)
			)
		)
	)
	(embedded_fonts no)
)
