<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="1X06SMD">
</package>
<package name="XIAO_ESP32_C3_TAPED">
</package>
</packages>
</library>
<library name="IC_Power-Management">
<description>&lt;B&gt;Voltage Regulators, Drivers, Switching controllers</description>
<packages>
<package name="SOP65P640X110-28">
<description>28-SOP, 0.65 mm pitch, 6.40 mm span, 9.70 X 4.40 X 1.10 mm body
&lt;p&gt;28-pin SOP package with 0.65 mm pitch, 6.40 mm span with body size 9.70 X 4.40 X 1.10 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="fab" package="1X06SMD" value="CONN_06_FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="U$3" library="fab" package="1X06SMD" value="CONN_06_FTDI-SMD-HEADER">
<attribute name="NAME"/>
</element>
<element name="U1" library="IC_Power-Management" package="SOP65P640X110-28" value="PCA9685PW_28-TSSOP">
<attribute name="CATEGORY" value="Power Management IC"/>
<attribute name="DATASHEET" value="https://www.nxp.com/docs/en/data-sheet/PCA9685.pdf"/>
<attribute name="DESCRIPTION" value="LED Driver IC 16 Output Linear PWM Dimming 25mA 28-TSSOP"/>
<attribute name="INPUT_VOLTAGE" value="2.3V ~ 5.5V"/>
<attribute name="MANUFACTURER" value="NXP USA Inc."/>
<attribute name="MPN" value="PCA9685PW118"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMPERATURE" value="-40°C ~ 85°C"/>
<attribute name="OUTPUT_CURRENT" value="25mA"/>
<attribute name="OUTPUT_VOLTAGE" value="5.5V"/>
<attribute name="PACKAGE_SIZE" value="28-TSSOP"/>
<attribute name="PACKAGE_TYPE" value="Surface Mount"/>
<attribute name="PART_STATUS" value="Active"/>
<attribute name="ROHS" value="Compliant"/>
<attribute name="SERIES" value="PCA9685"/>
<attribute name="SUBCATEGORY" value="LED Drivers"/>
<attribute name="THERMALLOSS" value="0.4 W"/>
<attribute name="TOPOLOGY" value="NA"/>
<attribute name="TYPE" value="Linear"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fab" package="XIAO_ESP32_C3_TAPED" value="XIAO_ESP32_C3_TAPEDXIAO_ESP32_C3_TAPED">
</element>
<element name="R3" library="fab" package="R1206" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="3V3">
<contactref element="U1" pad="28"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="P$12"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="14"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$3" pad="4"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$1" pad="P$13"/>
</signal>
<signal name="SDA">
<contactref element="U$2" pad="5"/>
<contactref element="U$1" pad="P$5"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="26"/>
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="P$6"/>
</signal>
<signal name="5V">
<contactref element="U$3" pad="2"/>
<contactref element="U$3" pad="5"/>
<contactref element="U$1" pad="P$14"/>
</signal>
<signal name="CTRL1">
<contactref element="U1" pad="6"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="CTRL2">
<contactref element="U$3" pad="6"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="27"/>
<contactref element="R3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
