<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
<wire x1="8.128" y1="32.9184" x2="8.128" y2="6.5024" width="0.4064" layer="20"/>
<wire x1="8.128" y1="32.9184" x2="41.8592" y2="32.9184" width="0.4064" layer="20"/>
<wire x1="8.128" y1="6.5024" x2="41.6052" y2="6.5024" width="0.4064" layer="20"/>
<wire x1="41.6052" y1="6.5024" x2="41.8592" y2="6.7564" width="0.4064" layer="20" curve="90"/>
<wire x1="41.8592" y1="6.7564" x2="41.8592" y2="32.9184" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="6MM_SWITCH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="EFOBM">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML1206">
<description>&lt;b&gt;SML10XXKH-TR (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;SML10R3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10E3KH-TR&lt;/td&gt;&lt;td&gt;SUPER REDSUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10O3KH-TR&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PY3KH-TR&lt;/td&gt;&lt;td&gt;PURE YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10OY3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10AG3KH-TR&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10BG3KH-TR&lt;/td&gt;&lt;td&gt;BLUE GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PB1KH-TR&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10CW1KH-TR&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;

Source: http://www.ledtronics.com/ds/smd-1206/dstr0094.PDF</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06-SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="fab" package="SOIC14" value="ATTINY44-SSU"/>
<element name="LED1" library="led" package="SML1206" value=""/>
<element name="S1" library="fab" package="6MM_SWITCH" value=""/>
<element name="C1" library="fab" package="C1206" value="1uf"/>
<element name="R1" library="fab" package="R1206" value="10k"/>
<element name="R2" library="fab" package="R1206" value="499"/>
<element name="JP1" library="SparkFun" package="1X06-SMD" value=""/>
<element name="U$2" library="fab" package="2X03SMD" value="AVRISPSMD"/>
<element name="U$3" library="fab" package="EFOBM" value="RESONATOR"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="RST">
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="3"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="LED">
<contactref element="IC1" pad="6"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="BUTTON">
<contactref element="IC1" pad="10"/>
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="RX">
<contactref element="IC1" pad="12"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="TX">
<contactref element="IC1" pad="13"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="LED1" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="LED1" pad="C"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="JP1" pad="6"/>
<contactref element="U$3" pad="2"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="CTS">
<contactref element="JP1" pad="5"/>
</signal>
<signal name="RTS">
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="2"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="3"/>
<contactref element="U$3" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
