<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>Vcc and GND</text>
<wire x1="6.985" y1="53.6575" x2="6.985" y2="20.0025" width="0.4064" layer="20"/>
<wire x1="46.6598" y1="10.795" x2="46.6598" y2="61.9125" width="0.4064" layer="20"/>
<wire x1="46.6725" y1="61.9125" x2="46.6598" y2="61.9125" width="0.4064" layer="20"/>
<wire x1="46.6598" y1="61.9125" x2="13.335" y2="61.9125" width="0.4064" layer="20"/>
<wire x1="13.335" y1="61.9125" x2="13.335" y2="53.6575" width="0.4064" layer="20"/>
<wire x1="13.335" y1="53.6575" x2="6.985" y2="53.6575" width="0.4064" layer="20"/>
<wire x1="46.6598" y1="10.795" x2="13.335" y2="10.795" width="0.4064" layer="20"/>
<wire x1="13.335" y1="10.795" x2="13.335" y2="20.0025" width="0.4064" layer="20"/>
<wire x1="13.335" y1="20.0025" x2="6.985" y2="20.0025" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="C1206FAB">
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="2X03SMD">
</package>
<package name="1X06SMD">
</package>
<package name="R1206FAB">
</package>
<package name="2-SMD-5X3MM">
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="AYZ0102AGRLC">
</package>
</packages>
</library>
<library name="ATMEGA328P-AU">
<packages>
<package name="QFP80P900X900X120-32N">
</package>
</packages>
</library>
<library name="SparkFun-IC-Power">
<description>&lt;h3&gt;SparkFun Power Driver and Management ICs&lt;/h3&gt;
In this library you'll find anything that has to do with power delivery, or making power supplies.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;LDOs&lt;/li&gt;
&lt;li&gt;Boost/Buck controllers&lt;/li&gt;
&lt;li&gt;Charge pump controllers&lt;/li&gt;
&lt;li&gt;Power sequencers&lt;/li&gt;
&lt;li&gt;Power switches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="fab" package="C1206FAB" value="1uF">
<attribute name="C1" value="1uF"/>
</element>
<element name="C2" library="fab" package="C1206" value="10pF"/>
<element name="C3" library="fab" package="C1206" value="10pF"/>
<element name="J1" library="fab" package="2X03SMD" value="ISP">
<attribute name="J1" value="ISP"/>
</element>
<element name="J2" library="fab" package="1X06SMD" value="FTDI">
<attribute name="J2" value="FTDI"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="10K">
<attribute name="R1" value="10K"/>
</element>
<element name="U$1" library="fab" package="2-SMD-5X3MM" value="CRYSTAL"/>
<element name="U1" library="ATMEGA328P-AU" package="QFP80P900X900X120-32N" value="ATMEGA328P-AU">
<attribute name="MP" value="ATMEGA328P-AU"/>
<attribute name="MF" value="Atmel"/>
<attribute name="PRICE" value="2.80 USD"/>
<attribute name="DESCRIPTION" value="ATmega Series 20 MHz 32 KB Flash 2 KB SRAM 8-Bit Microcontroller - TQFP-32"/>
<attribute name="PACKAGE" value="TQFP-32 Atmel"/>
<attribute name="AVAILABILITY" value="Good"/>
</element>
<element name="C4" library="fab" package="C1206FAB" value="0.1uF">
<attribute name="C1" value="1uF"/>
</element>
<element name="U$2" library="fab" package="LED1206FAB" value="LEDFAB1206"/>
<element name="R3" library="fab" package="R1206FAB" value="1K">
<attribute name="R1" value="10K"/>
</element>
<element name="R4" library="fab" package="R1206FAB" value="0">
<attribute name="R1" value="10K"/>
</element>
<element name="R5" library="fab" package="R1206FAB" value="0">
<attribute name="R1" value="10K"/>
</element>
<element name="R6" library="fab" package="R1206FAB" value="0">
<attribute name="R1" value="10K"/>
</element>
<element name="R7" library="fab" package="R1206FAB" value="0">
<attribute name="R1" value="10K"/>
</element>
<element name="U2" library="SparkFun-IC-Power" package="SOT223" value="">
<attribute name="PROD_ID" value="VREG-08170"/>
</element>
<element name="S1" library="fab" package="AYZ0102AGRLC" value="SLIDE-SWITCH"/>
</elements>
<signals>
<signal name="PB0">
<contactref element="U1" pad="12"/>
</signal>
<signal name="PB1">
<contactref element="U1" pad="13"/>
</signal>
<signal name="PB3">
<contactref element="U1" pad="15"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="21"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="PB2">
<contactref element="U1" pad="14"/>
</signal>
<signal name="ADC0">
<contactref element="U1" pad="23"/>
</signal>
<signal name="ADC1">
<contactref element="U1" pad="24"/>
</signal>
<signal name="PC6">
<contactref element="U1" pad="29"/>
<contactref element="C4" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="PB4">
<contactref element="U1" pad="16"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="PB5">
<contactref element="U1" pad="17"/>
<contactref element="J1" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="PB6">
<contactref element="U1" pad="7"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="PB7">
<contactref element="U1" pad="8"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="J2" pad="5"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="TXD">
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="AIN1">
<contactref element="U1" pad="11"/>
</signal>
<signal name="ADC6">
<contactref element="U1" pad="19"/>
</signal>
<signal name="ADC7">
<contactref element="U1" pad="22"/>
</signal>
<signal name="AVCC">
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="6"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="RST">
<contactref element="J1" pad="5"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="X1">
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="X2">
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$3">
<contactref element="S1" pad="3"/>
<contactref element="U2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
