<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="100" width="0" layer="20"/>
<wire x1="160" y1="100" x2="0" y2="100" width="0" layer="20"/>
<wire x1="0" y1="100" x2="0" y2="0" width="0" layer="20"/>
<hole x="36.83" y="44.45" drill="2.032"/>
<hole x="36.83" y="39.37" drill="2.032"/>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="R1206FAB">
</package>
<package name="LED1206">
<description>LED 1206 pads (standard pattern)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="fab" package="R1206FAB" value=""/>
<element name="U$1" library="fab" package="LED1206" value="LED"/>
<element name="U$2" library="fab" package="LED1206" value="LED"/>
<element name="U$3" library="fab" package="LED1206" value="LED"/>
<element name="U$4" library="fab" package="LED1206" value="LED"/>
<element name="U$5" library="fab" package="LED1206" value="LED"/>
<element name="U$6" library="fab" package="LED1206" value="LED"/>
<element name="U$7" library="fab" package="LED1206" value="LED"/>
<element name="U$8" library="fab" package="LED1206" value="LED"/>
</elements>
<signals>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$5" pad="1"/>
<contactref element="U$6" pad="1"/>
<contactref element="U$7" pad="1"/>
<contactref element="U$8" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="U$4" pad="2"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$5" pad="2"/>
<contactref element="U$6" pad="2"/>
<contactref element="U$7" pad="2"/>
<contactref element="U$8" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
