<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="18.522" y2="0" width="0" layer="20"/>
<wire x1="18.522" y1="0" x2="18.522" y2="35.738" width="0" layer="20"/>
<wire x1="18.522" y1="35.738" x2="0" y2="35.738" width="0" layer="20"/>
<wire x1="0" y1="35.738" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="passives">
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="6_PIN_SERIAL_TARGET_SIDE_RA_SMT">
<description>&lt;h3&gt;6 pin Serial Target - Right Angle  SMT&lt;/h3&gt;
Package for devices meant to mate to an FTDI connector. 
&lt;p&gt; tDocu shows pin location. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;6_Pin_Serial_Target&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="fablab">
<packages>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="LED1206FAB">
<description>LED1206 FAB style (smaller pads to allow trace between)</description>
</package>
<package name="R1206FAB">
</package>
<package name="2X03SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="6_PIN_SERIAL_TARGET_SIDE_RA_SMT" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08971"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fablab" package="SOIC8" value="UC_ATTINY45SI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="fablab" package="LED1206FAB" value="LEDFAB1206">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="fablab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="fablab" package="R1206FAB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="passives" package="1206" value="">
<attribute name="NAME"/>
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="U$3" library="fablab" package="2X03SMD" value="CONN_03X2_AVRISPSMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="J1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="7"/>
<contactref element="J1" pad="3"/>
<contactref element="U$3" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="5"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="6"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$2" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="U$1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="4"/>
<contactref element="R3" pad="1"/>
<contactref element="J1" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="U$3" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
