<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<board>
<plain>
<wire x1="67.31" y1="30.48" x2="130.79" y2="30.48" width="0" layer="20"/>
<wire x1="130.79" y1="30.48" x2="130.79" y2="72.06" width="0" layer="20"/>
<wire x1="130.79" y1="72.06" x2="67.31" y2="72.06" width="0" layer="20"/>
<wire x1="67.31" y1="72.06" x2="67.31" y2="30.48" width="0" layer="20"/>
<wire x1="106.68" y1="45.72" x2="105.41" y2="59.69" width="0.4064" layer="20" curve="-315.753848"/>
<wire x1="105.41" y1="59.69" x2="109.22" y2="59.69" width="0.4064" layer="20"/>
<wire x1="109.22" y1="59.69" x2="113.03" y2="63.5" width="0.4064" layer="20"/>
<wire x1="113.03" y1="63.5" x2="129.54" y2="63.5" width="0.4064" layer="20"/>
<wire x1="129.54" y1="63.5" x2="129.54" y2="59.69" width="0.4064" layer="20"/>
<wire x1="129.54" y1="59.69" x2="124.46" y2="54.61" width="0.4064" layer="20"/>
<wire x1="124.46" y1="54.61" x2="124.46" y2="49.53" width="0.4064" layer="20"/>
<wire x1="124.46" y1="49.53" x2="128.27" y2="45.72" width="0.4064" layer="20"/>
<wire x1="128.27" y1="45.72" x2="128.27" y2="41.91" width="0.4064" layer="20"/>
<wire x1="114.3" y1="41.91" x2="110.49" y2="45.72" width="0.4064" layer="20"/>
<wire x1="110.49" y1="45.72" x2="106.68" y2="45.72" width="0.4064" layer="20"/>
<wire x1="114.3" y1="41.91" x2="128.27" y2="41.91" width="0.4064" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
<description>&lt;h3&gt;LED 1206 SMT&lt;/h3&gt;

1206, surface mount. 

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: &lt;/li&gt;
&lt;li&gt;Area: 0.125" x 0.06"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="95278-801A04LF">
<description>&lt;AMPHENOL ICC (FCI) - 95278-801A04LF - CONNECTOR, HEADER, 4POS, 2ROW, 2.54MM&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="95278801A04LF">
<description>&lt;b&gt;95278-801A04LF-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="Resistor">
<description>&lt;B&gt;Resistors, Potentiometers, TrimPot</description>
<packages>
<package name="RESC3216X70">
<description>Chip, 3.20 X 1.60 X 0.70 mm body
&lt;p&gt;Chip package with body size 3.20 X 1.60 X 0.70 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="switch_fab">
<packages>
<package name="SW_B3SN-3012_OMR">
</package>
</packages>
</library>
<library name="attiny_fab">
<packages>
<package name="SOIC14_SL_MCH">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="1206" value="1.0uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-09822"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-1206" value="GREEN">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-00862"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="95278-801A04LF" package="95278801A04LF" value="95278-801A04LF">
<attribute name="ARROW_PART_NUMBER" value="95278-801A04LF"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/95278-801a04lf/amphenol-fci"/>
<attribute name="DESCRIPTION" value="AMPHENOL ICC (FCI) - 95278-801A04LF - CONNECTOR, HEADER, 4POS, 2ROW, 2.54MM"/>
<attribute name="HEIGHT" value="8.64mm"/>
<attribute name="MANUFACTURER_NAME" value="Amphenol"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="95278-801A04LF"/>
<attribute name="MOUSER_PART_NUMBER" value="649-95278-801A04LF"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Amphenol-FCI/95278-801A04LF?qs=AwD%252BQufC0y6qE8XiryCwbA%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="Resistor" package="RESC3216X70" value="1k">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="Resistor" package="RESC3216X70" value="1k">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="Resistor" package="RESC3216X70" value="4.7k">
<attribute name="CATEGORY" value="Resistor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="RATING" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="switch_fab" package="SW_B3SN-3012_OMR" value="B3SN-3012">
<attribute name="BUILT_BY" value="EMA_Justin"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="https://omronfs.omron.com/en_US/ecb/products/pdf/en-b3sn.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="B3SN-3012"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Omron_2020-06-30"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="Omron"/>
</element>
<element name="U1" library="attiny_fab" package="SOIC14_SL_MCH" value="ATTINY1614-SSNR">
<attribute name="BUILT_BY" value="EMA_Molly"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATTINY1614-SSNR"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Microchip_2019-08-23_25"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="Microchip"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="VDD">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="SW-3">
<contactref element="U1" pad="3"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="UPDI">
<contactref element="J2" pad="4"/>
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
