(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "fab:Conn_PinHeader_1x05_P2.54mm_Horizontal_SMD" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 7.62 0))
      (property "Value" "Conn_PinHeader_1x05_P2.54mm_Horizontal_SMD" (at 0 -7.62 0))
      (property "Footprint" "fab:PinHeader_1x05_P2.54mm_Horizontal_SMD" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "single row male connector" (at 0 0 0))
      (property "ki_description" "Male connector, single row" (at 0 0 0))
      (property "ki_fp_filters" "*PinHeader*1x05*" (at 0 0 0))
      (symbol "Conn_PinHeader_1x05_P2.54mm_Horizontal_SMD_1_1"
        (rectangle (start -1.27 -4.445) (end 1.27 -5.715)
          (fill (type outline))
        )
        (rectangle (start -1.27 -1.905) (end 1.27 -3.175)
          (fill (type outline))
        )
        (rectangle (start -1.27 0.635) (end 1.27 -0.635)
          (fill (type outline))
        )
        (rectangle (start -1.27 3.175) (end 1.27 1.905)
          (fill (type outline))
        )
        (rectangle (start -1.27 5.715) (end 1.27 4.445)
          (fill (type outline))
        )
        (pin passive line (at 5.08 5.08 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at 5.08 -5.08 180) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
      )
    )
    (symbol "fab:Conn_PinHeader_1x06_P2.54mm_Horizontal_SMD" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 7.62 0))
      (property "Value" "Conn_PinHeader_1x06_P2.54mm_Horizontal_SMD" (at 0 -10.16 0))
      (property "Footprint" "fab:PinHeader_1x06_P2.54mm_Horizontal_SMD" (at 0 0 0))
      (property "Datasheet" "https://gct.co/files/specs/2.54mm-socket-spec.pdf" (at 0 0 0))
      (property "ki_keywords" "single row male connector BG300-06-A-L-A" (at 0 0 0))
      (property "ki_description" "Male connector, single row" (at 0 0 0))
      (property "ki_fp_filters" "*PinHeader*1x06*" (at 0 0 0))
      (symbol "Conn_PinHeader_1x06_P2.54mm_Horizontal_SMD_1_1"
        (rectangle (start -1.27 -6.985) (end 1.27 -8.255)
          (fill (type outline))
        )
        (rectangle (start -1.27 -4.445) (end 1.27 -5.715)
          (fill (type outline))
        )
        (rectangle (start -1.27 -1.905) (end 1.27 -3.175)
          (fill (type outline))
        )
        (rectangle (start -1.27 0.635) (end 1.27 -0.635)
          (fill (type outline))
        )
        (rectangle (start -1.27 3.175) (end 1.27 1.905)
          (fill (type outline))
        )
        (rectangle (start -1.27 5.715) (end 1.27 4.445)
          (fill (type outline))
        )
        (pin passive line (at 5.08 5.08 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at 5.08 -5.08 180) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 5.08 -7.62 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
      )
    )
    (symbol "fab:Conn_PinHeader_1x07_P2.54mm_Horizontal_SMD" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (at 0 10.16 0))
      (property "Value" "Conn_PinHeader_1x07_P2.54mm_Horizontal_SMD" (at 0 -10.16 0))
      (property "Footprint" "fab:PinHeader_1x07_P2.54mm_Horizontal_SMD" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "single row male connector" (at 0 0 0))
      (property "ki_description" "Male connector, single row" (at 0 0 0))
      (property "ki_fp_filters" "*PinHeader*1x07*" (at 0 0 0))
      (symbol "Conn_PinHeader_1x07_P2.54mm_Horizontal_SMD_1_1"
        (rectangle (start -1.27 -6.985) (end 1.27 -8.255)
          (fill (type outline))
        )
        (rectangle (start -1.27 -4.445) (end 1.27 -5.715)
          (fill (type outline))
        )
        (rectangle (start -1.27 -1.905) (end 1.27 -3.175)
          (fill (type outline))
        )
        (rectangle (start -1.27 0.635) (end 1.27 -0.635)
          (fill (type outline))
        )
        (rectangle (start -1.27 3.175) (end 1.27 1.905)
          (fill (type outline))
        )
        (rectangle (start -1.27 5.715) (end 1.27 4.445)
          (fill (type outline))
        )
        (rectangle (start -1.27 8.255) (end 1.27 6.985)
          (fill (type outline))
        )
        (pin passive line (at 5.08 7.62 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 5.08 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 5.08 -5.08 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at 5.08 -7.62 180) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
      )
    )
    (symbol "fab:Module_XIAO-RP2040" (in_bom yes) (on_board yes)
      (property "Reference" "M" (at -10.16 16.51 0))
      (property "Value" "Module_XIAO-RP2040" (at 3.81 16.51 0))
      (property "Footprint" "fab:SeeedStudio_XIAO_RP2040" (at 0 0 0))
      (property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/" (at 0 0 0))
      (property "ki_keywords" "XIAO RP2040 102010428" (at 0 0 0))
      (property "ki_description" "RP2040 XIAO RP2040 - ARM® Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board" (at 0 0 0))
      (property "ki_fp_filters" "*SeeedStudio?XIAO?RP2040*" (at 0 0 0))
      (symbol "Module_XIAO-RP2040_1_1"
        (rectangle (start -10.16 15.24) (end 10.16 -15.24)
          (fill (type background))
        )
        (pin bidirectional line (at -12.7 12.7 0) (length 2.54)
          (name "D0")
          (number "1")
        )
        (pin bidirectional line (at -12.7 -10.16 0) (length 2.54)
          (name "D9")
          (number "10")
        )
        (pin bidirectional line (at -12.7 -12.7 0) (length 2.54)
          (name "D10")
          (number "11")
        )
        (pin power_in line (at -2.54 17.78 270) (length 2.54)
          (name "3V3")
          (number "12")
        )
        (pin power_in line (at -2.54 -17.78 90) (length 2.54)
          (name "GND")
          (number "13")
        )
        (pin power_in line (at 0 17.78 270) (length 2.54)
          (name "5V")
          (number "14")
        )
        (pin power_in line (at 0 -17.78 90) (length 2.54)
          (name "GND")
          (number "15")
        )
        (pin power_in line (at 2.54 17.78 270) (length 2.54)
          (name "VIN")
          (number "16")
        )
        (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
          (name "SWDIO")
          (number "17")
        )
        (pin input line (at 12.7 -7.62 180) (length 2.54)
          (name "RESET")
          (number "18")
        )
        (pin power_in line (at 2.54 -17.78 90) (length 2.54)
          (name "GND")
          (number "19")
        )
        (pin bidirectional line (at -12.7 10.16 0) (length 2.54)
          (name "D1")
          (number "2")
        )
        (pin input line (at 12.7 -5.08 180) (length 2.54)
          (name "SWCLK")
          (number "20")
        )
        (pin bidirectional line (at -12.7 7.62 0) (length 2.54)
          (name "D2")
          (number "3")
        )
        (pin bidirectional line (at -12.7 5.08 0) (length 2.54)
          (name "D3")
          (number "4")
        )
        (pin bidirectional line (at -12.7 2.54 0) (length 2.54)
          (name "D4")
          (number "5")
        )
        (pin bidirectional line (at -12.7 0 0) (length 2.54)
          (name "D5")
          (number "6")
        )
        (pin bidirectional line (at -12.7 -2.54 0) (length 2.54)
          (name "D6")
          (number "7")
        )
        (pin bidirectional line (at -12.7 -5.08 0) (length 2.54)
          (name "D7")
          (number "8")
        )
        (pin bidirectional line (at -12.7 -7.62 0) (length 2.54)
          (name "D8")
          (number "9")
        )
      )
    )
    (symbol "fab:PWR_3V3" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "PWR_3V3" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "power-flag" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3V3\"" (at 0 0 0))
      (symbol "PWR_3V3_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "PWR_3V3_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "PWR_3V3")
          (number "1")
        )
      )
    )
    (symbol "fab:PWR_5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -3.81 0))
      (property "Value" "PWR_5V" (at 0 3.556 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "power-flag" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (at 0 0 0))
      (symbol "PWR_5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "PWR_5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "PWR_5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "power:PWR_FLAG" (power) (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "#FLG" (at 0 1.905 0))
      (property "Value" "PWR_FLAG" (at 0 3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "~" (at 0 0 0))
      (property "ki_keywords" "flag power" (at 0 0 0))
      (property "ki_description" "Special symbol for telling ERC where power comes from" (at 0 0 0))
      (symbol "PWR_FLAG_0_0"
        (pin power_out line (at 0 0 90) (length 0)
          (name "pwr")
          (number "1")
        )
      )
      (symbol "PWR_FLAG_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 1.27)
            (xy -1.016 1.905)
            (xy 0 2.54)
            (xy 1.016 1.905)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
    )
  )
  (junction (at 195.58 44.45) (diameter 0) (color 0 0 0 0))
  (junction (at 198.12 44.45) (diameter 0) (color 0 0 0 0))
  (junction (at 195.58 90.17) (diameter 0) (color 0 0 0 0))
  (no_connect (at 213.36 77.47))
  (no_connect (at 200.66 49.53))
  (no_connect (at 213.36 74.93))
  (no_connect (at 200.66 90.17))
  (no_connect (at 213.36 72.39))
  (no_connect (at 198.12 90.17))
  (wire (pts (xy 210.82 74.93) (xy 213.36 74.93)))
  (wire (pts (xy 96.52 59.69) (xy 102.87 59.69)))
  (wire (pts (xy 195.58 87.63) (xy 195.58 90.17)))
  (wire (pts (xy 43.18 54.61) (xy 49.53 54.61)))
  (wire (pts (xy 181.61 82.55) (xy 185.42 82.55)))
  (wire (pts (xy 181.61 67.31) (xy 185.42 67.31)))
  (wire (pts (xy 195.58 40.64) (xy 195.58 44.45)))
  (wire (pts (xy 96.52 85.09) (xy 102.87 85.09)))
  (wire (pts (xy 43.18 80.01) (xy 49.53 80.01)))
  (wire (pts (xy 43.18 49.53) (xy 49.53 49.53)))
  (wire (pts (xy 193.04 90.17) (xy 195.58 90.17)))
  (wire (pts (xy 198.12 40.64) (xy 198.12 44.45)))
  (wire (pts (xy 181.61 62.23) (xy 185.42 62.23)))
  (wire (pts (xy 96.52 57.15) (xy 102.87 57.15)))
  (wire (pts (xy 96.52 54.61) (xy 102.87 54.61)))
  (wire (pts (xy 43.18 82.55) (xy 49.53 82.55)))
  (wire (pts (xy 195.58 44.45) (xy 195.58 52.07)))
  (wire (pts (xy 43.18 87.63) (xy 49.53 87.63)))
  (wire (pts (xy 198.12 44.45) (xy 198.12 52.07)))
  (wire (pts (xy 96.52 90.17) (xy 102.87 90.17)))
  (wire (pts (xy 198.12 87.63) (xy 198.12 90.17)))
  (wire (pts (xy 43.18 90.17) (xy 49.53 90.17)))
  (wire (pts (xy 96.52 52.07) (xy 102.87 52.07)))
  (wire (pts (xy 181.61 69.85) (xy 185.42 69.85)))
  (wire (pts (xy 96.52 62.23) (xy 102.87 62.23)))
  (wire (pts (xy 189.23 40.64) (xy 195.58 40.64)))
  (wire (pts (xy 96.52 49.53) (xy 102.87 49.53)))
  (wire (pts (xy 210.82 77.47) (xy 213.36 77.47)))
  (wire (pts (xy 96.52 87.63) (xy 102.87 87.63)))
  (wire (pts (xy 43.18 59.69) (xy 49.53 59.69)))
  (wire (pts (xy 181.61 74.93) (xy 185.42 74.93)))
  (wire (pts (xy 96.52 80.01) (xy 102.87 80.01)))
  (wire (pts (xy 198.12 44.45) (xy 200.66 44.45)))
  (wire (pts (xy 181.61 72.39) (xy 185.42 72.39)))
  (wire (pts (xy 181.61 80.01) (xy 185.42 80.01)))
  (wire (pts (xy 210.82 72.39) (xy 213.36 72.39)))
  (wire (pts (xy 43.18 85.09) (xy 49.53 85.09)))
  (wire (pts (xy 193.04 44.45) (xy 195.58 44.45)))
  (wire (pts (xy 43.18 62.23) (xy 49.53 62.23)))
  (wire (pts (xy 181.61 59.69) (xy 185.42 59.69)))
  (wire (pts (xy 195.58 90.17) (xy 195.58 91.44)))
  (wire (pts (xy 200.66 49.53) (xy 200.66 52.07)))
  (wire (pts (xy 181.61 57.15) (xy 185.42 57.15)))
  (wire (pts (xy 181.61 77.47) (xy 185.42 77.47)))
  (wire (pts (xy 43.18 52.07) (xy 49.53 52.07)))
  (wire (pts (xy 96.52 82.55) (xy 102.87 82.55)))
  (wire (pts (xy 43.18 64.77) (xy 49.53 64.77)))
  (wire (pts (xy 181.61 64.77) (xy 185.42 64.77)))
  (wire (pts (xy 200.66 87.63) (xy 200.66 90.17)))
  (wire (pts (xy 43.18 57.15) (xy 49.53 57.15)))
  (global_label "MISO" (shape input) (at 102.87 59.69 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 110.4514 59.69 0))
  )
  (global_label "A0" (shape input) (at 181.61 57.15 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 176.3267 57.15 0))
  )
  (global_label "SCK" (shape input) (at 181.61 77.47 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 174.8753 77.47 0))
  )
  (global_label "A1" (shape input) (at 181.61 59.69 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 176.3267 59.69 0))
  )
  (global_label "MOSI" (shape input) (at 102.87 57.15 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 110.4514 57.15 0))
  )
  (global_label "TX" (shape input) (at 102.87 90.17 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 108.0323 90.17 0))
  )
  (global_label "A1" (shape input) (at 49.53 54.61 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 54.8133 54.61 0))
  )
  (global_label "A0" (shape input) (at 49.53 57.15 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 54.8133 57.15 0))
  )
  (global_label "SCL" (shape input) (at 181.61 69.85 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 175.1172 69.85 0))
  )
  (global_label "A2" (shape input) (at 181.61 62.23 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 176.3267 62.23 0))
  )
  (global_label "SCK" (shape input) (at 102.87 62.23 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 109.6047 62.23 0))
  )
  (global_label "RX" (shape input) (at 181.61 74.93 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 176.1453 74.93 0))
  )
  (global_label "RX" (shape input) (at 102.87 87.63 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 108.3347 87.63 0))
  )
  (global_label "SCL" (shape input) (at 49.53 80.01 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 56.0228 80.01 0))
  )
  (global_label "MISO" (shape input) (at 181.61 80.01 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 174.0286 80.01 0))
  )
  (global_label "SDA" (shape input) (at 49.53 82.55 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 56.0833 82.55 0))
  )
  (global_label "TX" (shape input) (at 181.61 72.39 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 176.4477 72.39 0))
  )
  (global_label "A3" (shape input) (at 49.53 49.53 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 54.8133 49.53 0))
  )
  (global_label "A3" (shape input) (at 181.61 64.77 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 176.3267 64.77 0))
  )
  (global_label "A2" (shape input) (at 49.53 52.07 0) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 54.8133 52.07 0))
  )
  (global_label "MOSI" (shape input) (at 181.61 82.55 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 174.0286 82.55 0))
  )
  (global_label "SDA" (shape input) (at 181.61 67.31 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 175.0567 67.31 0))
  )
  (symbol (lib_id "fab:Conn_PinHeader_1x07_P2.54mm_Horizontal_SMD") (at 38.1 57.15 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "ANALOG1" (at 38.1 41.91 0))
    (property "Value" "Conn_PinHeader_1x07_P2.54mm_Horizontal_SMD" (at 38.1 44.45 0))
    (property "Footprint" "fab:PinHeader_1x07_P2.54mm_Horizontal_SMD" (at 38.1 57.15 0))
    (property "Datasheet" "~" (at 38.1 57.15 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "ANALOG1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:PWR_5V") (at 102.87 80.01 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR013" (at 99.06 80.01 0))
    (property "Value" "PWR_5V" (at 106.68 80.01 90))
    (property "Footprint" "" (at 102.87 80.01 0))
    (property "Datasheet" "" (at 102.87 80.01 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR013") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 49.53 62.23 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR05" (at 55.88 62.23 0))
    (property "Value" "GND" (at 53.34 62.23 90))
    (property "Footprint" "" (at 49.53 62.23 0))
    (property "Datasheet" "" (at 49.53 62.23 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR05") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:PWR_3V3") (at 49.53 85.09 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR07" (at 45.72 85.09 0))
    (property "Value" "PWR_3V3" (at 53.34 85.09 90))
    (property "Footprint" "" (at 49.53 85.09 0))
    (property "Datasheet" "" (at 49.53 85.09 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR07") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 195.58 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR03" (at 195.58 97.79 0))
    (property "Value" "GND" (at 195.58 96.52 0))
    (property "Footprint" "" (at 195.58 91.44 0))
    (property "Datasheet" "" (at 195.58 91.44 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 102.87 52.07 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR011" (at 109.22 52.07 0))
    (property "Value" "GND" (at 106.68 52.07 90))
    (property "Footprint" "" (at 102.87 52.07 0))
    (property "Datasheet" "" (at 102.87 52.07 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR011") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:PWR_FLAG") (at 193.04 90.17 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#FLG03" (at 191.135 90.17 0))
    (property "Value" "PWR_FLAG" (at 189.23 90.17 90))
    (property "Footprint" "" (at 193.04 90.17 0))
    (property "Datasheet" "~" (at 193.04 90.17 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#FLG03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:Conn_PinHeader_1x06_P2.54mm_Horizontal_SMD") (at 91.44 54.61 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "SPI1" (at 91.44 41.91 0))
    (property "Value" "Conn_PinHeader_1x06_P2.54mm_Horizontal_SMD" (at 91.44 44.45 0))
    (property "Footprint" "fab:PinHeader_1x06_P2.54mm_Horizontal_SMD" (at 91.44 54.61 0))
    (property "Datasheet" "https://gct.co/files/specs/2.54mm-socket-spec.pdf" (at 91.44 54.61 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "SPI1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 102.87 82.55 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR014" (at 109.22 82.55 0))
    (property "Value" "GND" (at 106.68 82.55 90))
    (property "Footprint" "" (at 102.87 82.55 0))
    (property "Datasheet" "" (at 102.87 82.55 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR014") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:PWR_FLAG") (at 200.66 44.45 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#FLG01" (at 202.565 44.45 0))
    (property "Value" "PWR_FLAG" (at 204.47 44.45 90))
    (property "Footprint" "" (at 200.66 44.45 0))
    (property "Datasheet" "~" (at 200.66 44.45 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#FLG01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:PWR_5V") (at 102.87 49.53 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR012" (at 99.06 49.53 0))
    (property "Value" "PWR_5V" (at 106.68 49.53 90))
    (property "Footprint" "" (at 102.87 49.53 0))
    (property "Datasheet" "" (at 102.87 49.53 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR012") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:Conn_PinHeader_1x05_P2.54mm_Horizontal_SMD") (at 91.44 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "UART1" (at 93.98 73.66 0))
    (property "Value" "Conn_PinHeader_1x05_P2.54mm_Horizontal_SMD" (at 118.11 76.2 0))
    (property "Footprint" "fab:PinHeader_1x05_P2.54mm_Horizontal_SMD" (at 91.44 85.09 0))
    (property "Datasheet" "~" (at 91.44 85.09 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "UART1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:PWR_3V3") (at 49.53 59.69 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR06" (at 45.72 59.69 0))
    (property "Value" "PWR_3V3" (at 53.34 59.69 90))
    (property "Footprint" "" (at 49.53 59.69 0))
    (property "Datasheet" "" (at 49.53 59.69 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR06") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:Module_XIAO-RP2040") (at 198.12 69.85 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "M1" (at 219.71 65.4619 0))
    (property "Value" "Module_XIAO-RP2040" (at 219.71 68.0019 0))
    (property "Footprint" "fab:SeeedStudio_XIAO_RP2040" (at 198.12 69.85 0))
    (property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/" (at 198.12 69.85 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "M1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:PWR_5V") (at 198.12 40.64 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR01" (at 198.12 44.45 0))
    (property "Value" "PWR_5V" (at 198.12 35.56 0))
    (property "Footprint" "" (at 198.12 40.64 0))
    (property "Datasheet" "" (at 198.12 40.64 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:PWR_5V") (at 49.53 90.17 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR09" (at 45.72 90.17 0))
    (property "Value" "PWR_5V" (at 53.34 90.17 90))
    (property "Footprint" "" (at 49.53 90.17 0))
    (property "Datasheet" "" (at 49.53 90.17 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR09") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:PWR_5V") (at 49.53 64.77 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR04" (at 45.72 64.77 0))
    (property "Value" "PWR_5V" (at 53.34 64.77 90))
    (property "Footprint" "" (at 49.53 64.77 0))
    (property "Datasheet" "" (at 49.53 64.77 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 49.53 87.63 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR08" (at 55.88 87.63 0))
    (property "Value" "GND" (at 53.34 87.63 90))
    (property "Footprint" "" (at 49.53 87.63 0))
    (property "Datasheet" "" (at 49.53 87.63 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR08") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:Conn_PinHeader_1x05_P2.54mm_Horizontal_SMD") (at 38.1 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no)
    (property "Reference" "I2C1" (at 38.1 73.66 0))
    (property "Value" "Conn_PinHeader_1x05_P2.54mm_Horizontal_SMD" (at 38.1 76.2 0))
    (property "Footprint" "fab:PinHeader_1x05_P2.54mm_Horizontal_SMD" (at 38.1 85.09 0))
    (property "Datasheet" "~" (at 38.1 85.09 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "I2C1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:PWR_3V3") (at 102.87 85.09 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR015" (at 99.06 85.09 0))
    (property "Value" "PWR_3V3" (at 106.68 85.09 90))
    (property "Footprint" "" (at 102.87 85.09 0))
    (property "Datasheet" "" (at 102.87 85.09 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR015") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:PWR_3V3") (at 102.87 54.61 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR010" (at 99.06 54.61 0))
    (property "Value" "PWR_3V3" (at 106.68 54.61 90))
    (property "Footprint" "" (at 102.87 54.61 0))
    (property "Datasheet" "" (at 102.87 54.61 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR010") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:PWR_FLAG") (at 193.04 44.45 90) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#FLG02" (at 191.135 44.45 0))
    (property "Value" "PWR_FLAG" (at 189.23 44.45 90))
    (property "Footprint" "" (at 193.04 44.45 0))
    (property "Datasheet" "~" (at 193.04 44.45 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#FLG02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "fab:PWR_3V3") (at 189.23 40.64 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR02" (at 189.23 44.45 0))
    (property "Value" "PWR_3V3" (at 189.23 35.56 0))
    (property "Footprint" "" (at 189.23 40.64 0))
    (property "Datasheet" "" (at 189.23 40.64 0))
    (pin "1")
    (instances
      (project "xiao_breakout_v2"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
