(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "Connector:Conn_01x07_Pin"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 10.16 0)
			)
			(property "Value" "Conn_01x07_Pin"
				(at 0 -10.16 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x07, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x07_Pin_1_1"
				(rectangle
					(start 0.8636 7.747)
					(end 0 7.493)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 5.207)
					(end 0 4.953)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 2.667)
					(end 0 2.413)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 -2.413)
					(end 0 -2.667)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 -4.953)
					(end 0 -5.207)
					(fill
						(type outline)
					)
				)
				(rectangle
					(start 0.8636 -7.493)
					(end 0 -7.747)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.27 7.62) (xy 0.8636 7.62)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 5.08) (xy 0.8636 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 2.54) (xy 0.8636 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 0.8636 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -5.08) (xy 0.8636 -5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -7.62) (xy 0.8636 -7.62)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 5.08 7.62 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
				(pin passive line
					(at 5.08 5.08 180)
					(length 3.81)
					(name "Pin_2")
					(number "2")
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 3.81)
					(name "Pin_3")
					(number "3")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_4")
					(number "4")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 3.81)
					(name "Pin_5")
					(number "5")
				)
				(pin passive line
					(at 5.08 -5.08 180)
					(length 3.81)
					(name "Pin_6")
					(number "6")
				)
				(pin passive line
					(at 5.08 -7.62 180)
					(length 3.81)
					(name "Pin_7")
					(number "7")
				)
			)
			(embedded_fonts no)
		)
		(symbol "epressif:XIAO-ESP32-C6-SMD"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -18.542 23.114 0)
			)
			(property "Value" "XIAO-ESP32-S3-SMD"
				(at -8.382 21.336 0)
			)
			(property "Footprint" ""
				(at -8.89 5.08 0)
			)
			(property "Datasheet" ""
				(at -8.89 5.08 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "XIAO-ESP32-C6-SMD_0_1"
				(rectangle
					(start 19.05 -19.05)
					(end -19.05 20.32)
					(fill
						(type none)
					)
				)
			)
			(symbol "XIAO-ESP32-C6-SMD_1_1"
				(pin passive line
					(at -21.59 11.43 0)
					(length 2.54)
					(name "GPIO0_A0_D0")
					(number "1")
				)
				(pin passive line
					(at -21.59 7.62 0)
					(length 2.54)
					(name "GPIO1_A1_D1")
					(number "2")
				)
				(pin passive line
					(at -21.59 3.81 0)
					(length 2.54)
					(name "GPIO2_A2_D2")
					(number "3")
				)
				(pin passive line
					(at -21.59 0 0)
					(length 2.54)
					(name "GPIO21_D3")
					(number "4")
				)
				(pin passive line
					(at -21.59 -3.81 0)
					(length 2.54)
					(name "GPIO22_D4_SDA")
					(number "5")
				)
				(pin passive line
					(at -21.59 -7.62 0)
					(length 2.54)
					(name "GPIO23_D5_SCL")
					(number "6")
				)
				(pin passive line
					(at -21.59 -11.43 0)
					(length 2.54)
					(name "GPIO16_D6_TX")
					(number "7")
				)
				(pin passive line
					(at -12.7 22.86 270)
					(length 2.54)
					(name "MTDI")
					(number "17")
				)
				(pin passive line
					(at -8.89 22.86 270)
					(length 2.54)
					(name "MTDO")
					(number "18")
				)
				(pin passive line
					(at -5.08 22.86 270)
					(length 2.54)
					(name "CHIP_EN")
					(number "19")
				)
				(pin passive line
					(at -2.54 -21.59 90)
					(length 2.54)
					(name "BAT")
					(number "15")
				)
				(pin passive line
					(at -1.27 22.86 270)
					(length 2.54)
					(name "GND")
					(number "20")
				)
				(pin passive line
					(at 2.54 22.86 270)
					(length 2.54)
					(name "MTMS")
					(number "21")
				)
				(pin passive line
					(at 2.54 -21.59 90)
					(length 2.54)
					(name "GND")
					(number "16")
				)
				(pin passive line
					(at 6.35 22.86 270)
					(length 2.54)
					(name "MTCK")
					(number "22")
				)
				(pin passive line
					(at 10.16 22.86 270)
					(length 2.54)
					(name "BOOT")
					(number "23")
				)
				(pin passive line
					(at 13.97 22.86 270)
					(length 2.54)
					(name "3V3_1")
					(number "24")
				)
				(pin passive line
					(at 21.59 11.43 180)
					(length 2.54)
					(name "5V")
					(number "14")
				)
				(pin passive line
					(at 21.59 7.62 180)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin passive line
					(at 21.59 3.81 180)
					(length 2.54)
					(name "3V3")
					(number "12")
				)
				(pin passive line
					(at 21.59 0 180)
					(length 2.54)
					(name "GPIO18_D10_MOSI")
					(number "11")
				)
				(pin passive line
					(at 21.59 -3.81 180)
					(length 2.54)
					(name "GPIO20_D9_MISO")
					(number "10")
				)
				(pin passive line
					(at 21.59 -7.62 180)
					(length 2.54)
					(name "GPIO19_D8_SCK")
					(number "9")
				)
				(pin passive line
					(at 21.59 -11.43 180)
					(length 2.54)
					(name "GPIO17_D7_RX")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:Conn_PinHeader_SWD_2x02_P2.54mm_Vertical_SMD"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 3.81 0)
			)
			(property "Value" "Conn_PinHeader_SWD_2x02_P2.54mm_Vertical_SMD"
				(at 0 -3.81 0)
			)
			(property "Footprint" "fab:PinHeader_02x02_P2.54mm_Vertical_SMD"
				(at 0 0 0)
			)
			(property "Datasheet" "https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/95278.pdf"
				(at 0 0 0)
			)
			(property "Description" "Connector Header Surface Mount 4 position 0.100\" (2.54mm) for programming D11C chips"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector swd programming jtag"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*PinHeader*2x02*"
				(at 0 0 0)
			)
			(symbol "Conn_PinHeader_SWD_2x02_P2.54mm_Vertical_SMD_0_0"
				(text "GND"
					(at -4.445 1.27 0)
				)
				(text "DIO"
					(at -4.445 -1.27 0)
				)
				(text "RST"
					(at 4.445 1.27 0)
				)
				(text "CLK"
					(at 4.445 -1.27 0)
				)
			)
			(symbol "Conn_PinHeader_SWD_2x02_P2.54mm_Vertical_SMD_0_1"
				(polyline
					(pts
						(xy -1.524 1.524) (xy -1.27 1.27) (xy -1.524 1.016) (xy -1.524 1.524)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -1.524 -1.016) (xy -1.27 -1.27) (xy -1.524 -1.524) (xy -1.524 -1.016)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.524 1.524) (xy 1.27 1.27) (xy 1.524 1.016) (xy 1.524 1.524)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.524 -1.016) (xy 1.27 -1.27) (xy 1.524 -1.524) (xy 1.524 -1.016)
					)
					(fill
						(type outline)
					)
				)
			)
			(symbol "Conn_PinHeader_SWD_2x02_P2.54mm_Vertical_SMD_1_1"
				(rectangle
					(start -5.08 2.54)
					(end 5.08 -2.54)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -7.62 1.27 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at -7.62 -1.27 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 7.62 1.27 180)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 7.62 -1.27 180)
					(length 2.54)
					(name "")
					(number "4")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:Conn_PinHeader_UPDI_2x03_P2.54mm_Vertical_SMD"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 5.08 0)
			)
			(property "Value" "Conn_PinHeader_UPDI_2x03_P2.54mm_Vertical_SMD"
				(at 0 -5.08 0)
			)
			(property "Footprint" "fab:PinHeader_02x03_P2.54mm_Vertical_SMD"
				(at 0 0 0)
			)
			(property "Datasheet" "https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/95278.pdf"
				(at 0 0 0)
			)
			(property "Description" "Connector Header Surface Mount 6 position 0.100\" (2.54mm) Fab UPDI connector standard 2022"
				(at 0 0 0)
			)
			(property "ki_keywords" "connector fab updi"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*PinHeader*2x03*"
				(at 0 0 0)
			)
			(symbol "Conn_PinHeader_UPDI_2x03_P2.54mm_Vertical_SMD_0_0"
				(rectangle
					(start -5.08 3.81)
					(end 5.08 -3.81)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -1.27 2.54) (xy -1.524 2.286) (xy -1.524 2.794) (xy -1.27 2.54)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy -1.524 -0.254) (xy -1.524 0.254) (xy -1.27 0)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -1.27 -2.54) (xy -1.524 -2.794) (xy -1.524 -2.286) (xy -1.27 -2.54)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.27 2.54) (xy 1.524 2.794) (xy 1.524 2.286) (xy 1.27 2.54)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 1.524 0.254) (xy 1.524 -0.254) (xy 1.27 0)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.54) (xy 1.524 -2.286) (xy 1.524 -2.794) (xy 1.27 -2.54)
					)
					(fill
						(type outline)
					)
				)
				(text "UPDI"
					(at -4.445 2.54 0)
				)
				(text "GND"
					(at -4.445 0 0)
				)
				(text "VCC"
					(at -4.445 -2.54 0)
				)
				(text "VCC"
					(at 4.445 2.54 0)
				)
				(text "GND"
					(at 4.445 0 0)
				)
				(text "UPDI"
					(at 4.445 -2.54 0)
				)
			)
			(symbol "Conn_PinHeader_UPDI_2x03_P2.54mm_Vertical_SMD_1_1"
				(pin passive line
					(at -7.62 2.54 0)
					(length 2.54)
					(name "")
					(number "1")
				)
				(pin passive line
					(at -7.62 0 0)
					(length 2.54)
					(name "")
					(number "3")
				)
				(pin passive line
					(at -7.62 -2.54 0)
					(length 2.54)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 7.62 2.54 180)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 7.62 -2.54 180)
					(length 2.54)
					(name "")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:LED_1206"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED_1206"
				(at 0 -2.54 0)
			)
			(property "Footprint" "fab:LED_1206"
				(at 0 0 0)
			)
			(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode 1206 SML-LX1206IC-TR SML-LX1206GC-TR 5988230107F 150120BS75000 QBLP650-IW HIR11-21C/L11/TR8"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*LED*1206*"
				(at 0 0 0)
			)
			(symbol "LED_1206_0_1"
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1206_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:R_1206"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.54 0 90)
			)
			(property "Value" "R_1206"
				(at -2.54 0 90)
			)
			(property "Footprint" "fab:R_1206"
				(at 0 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor RC1206FR-074M99L RC1206FR-07499KL RC1206FR-0749K9L RC1206FR-0749R9L RC1206FR-074R99L ERJ-8BWJR100V RC1206FR-070RL RC1206FR-071RL RC1206FR-0710RL RC1206FR-07100RL RC1206FR-07499RL RC1206FR-071KL RC1206FR-074K99L RC1206FR-0710KL RC1206FR-07100KL RC1206FR-071ML RC1206FR-0710ML PT1206FR-070R1L"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*R*1206*"
				(at 0 0 0)
			)
			(symbol "R_1206_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type background)
					)
				)
			)
			(symbol "R_1206_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "jst ph:S2B-PH-K-S_LF__SN_"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at -5.08 3.302 0)
			)
			(property "Value" "S2B-PH-K-S_LF__SN_"
				(at -5.08 -7.62 0)
			)
			(property "Footprint" "S2B-PH-K-S_LF__SN_:JST_S2B-PH-K-S_LF__SN_"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Connector Header Through Hole, Right Angle 2 position"
				(at 0 0 0)
			)
			(property "MF" "JST Sales America Inc."
				(at 0 0 0)
			)
			(property "MAXIMUM_PACKAGE_HEIGHT" "4.8mm"
				(at 0 0 0)
			)
			(property "PACKAGE" "None"
				(at 0 0 0)
			)
			(property "PRICE" "None"
				(at 0 0 0)
			)
			(property "Package" "NON STANDARD-2 J.S.T."
				(at 0 0 0)
			)
			(property "Check_prices" "https://www.snapeda.com/parts/S2B-PH-K-S(LF)(SN)/JST/view-part/?ref=eda"
				(at 0 0 0)
			)
			(property "Price" "None"
				(at 0 0 0)
			)
			(property "SnapEDA_Link" "https://www.snapeda.com/parts/S2B-PH-K-S(LF)(SN)/JST/view-part/?ref=snap"
				(at 0 0 0)
			)
			(property "MP" "S2B-PH-K-S(LF)(SN)"
				(at 0 0 0)
			)
			(property "Description_1" "Connector Header Through Hole, Right Angle 2 position"
				(at 0 0 0)
			)
			(property "Availability" "In Stock"
				(at 0 0 0)
			)
			(property "AVAILABILITY" "Unavailable"
				(at 0 0 0)
			)
			(symbol "S2B-PH-K-S_LF__SN__0_0"
				(rectangle
					(start -5.08 -5.08)
					(end 5.08 2.54)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -10.16 0 0)
					(length 5.08)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at -10.16 -2.54 0)
					(length 5.08)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GNDREF"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GNDREF"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GNDREF\" , reference supply ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GNDREF_0_1"
				(polyline
					(pts
						(xy -0.635 -1.905) (xy 0.635 -1.905)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -0.127 -2.54) (xy 0.127 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -1.27) (xy 0 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy -1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GNDREF_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 114.3 52.07)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 99.06 46.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 101.6 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 95.25)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 97.79 77.47)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 92.71)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 73.66 62.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 71.12 77.47)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 71.12 80.01)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 130.81 125.73)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 102.87 82.55)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 234.95 62.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 191.77 46.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 223.52 102.87)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 93.98 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 74.93 123.19)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 99.06 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 77.47)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 62.23)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 96.52 64.77)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 127 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 130.81 99.06)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 46.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 234.95 87.63)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 97.79)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 54.61 46.99)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 72.39 49.53)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 73.66 64.77)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 135.89 96.52) (xy 135.89 99.06)
		)
	)
	(wire
		(pts
			(xy 54.61 123.19) (xy 74.93 123.19)
		)
	)
	(wire
		(pts
			(xy 234.95 46.99) (xy 191.77 46.99)
		)
	)
	(wire
		(pts
			(xy 179.07 50.8) (xy 170.18 50.8)
		)
	)
	(wire
		(pts
			(xy 102.87 92.71) (xy 102.87 82.55)
		)
	)
	(wire
		(pts
			(xy 114.3 82.55) (xy 114.3 67.31)
		)
	)
	(wire
		(pts
			(xy 118.11 95.25) (xy 118.11 69.85)
		)
	)
	(wire
		(pts
			(xy 185.42 99.06) (xy 185.42 73.66)
		)
	)
	(wire
		(pts
			(xy 138.43 99.06) (xy 138.43 95.25)
		)
	)
	(wire
		(pts
			(xy 93.98 46.99) (xy 99.06 46.99)
		)
	)
	(wire
		(pts
			(xy 128.27 92.71) (xy 179.07 92.71)
		)
	)
	(wire
		(pts
			(xy 93.98 52.07) (xy 114.3 52.07)
		)
	)
	(wire
		(pts
			(xy 128.27 99.06) (xy 128.27 92.71)
		)
	)
	(wire
		(pts
			(xy 54.61 77.47) (xy 71.12 77.47)
		)
	)
	(wire
		(pts
			(xy 123.19 104.14) (xy 123.19 73.66)
		)
	)
	(wire
		(pts
			(xy 101.6 95.25) (xy 118.11 95.25)
		)
	)
	(wire
		(pts
			(xy 96.52 64.77) (xy 115.57 64.77)
		)
	)
	(wire
		(pts
			(xy 54.61 95.25) (xy 54.61 97.79)
		)
	)
	(wire
		(pts
			(xy 74.93 123.19) (xy 93.98 123.19)
		)
	)
	(wire
		(pts
			(xy 123.19 73.66) (xy 127 73.66)
		)
	)
	(wire
		(pts
			(xy 186.69 105.41) (xy 186.69 99.06)
		)
	)
	(wire
		(pts
			(xy 72.39 52.07) (xy 72.39 49.53)
		)
	)
	(wire
		(pts
			(xy 116.84 62.23) (xy 127 62.23)
		)
	)
	(wire
		(pts
			(xy 172.72 54.61) (xy 170.18 54.61)
		)
	)
	(wire
		(pts
			(xy 179.07 92.71) (xy 179.07 50.8)
		)
	)
	(wire
		(pts
			(xy 54.61 62.23) (xy 54.61 77.47)
		)
	)
	(wire
		(pts
			(xy 78.74 80.01) (xy 71.12 80.01)
		)
	)
	(wire
		(pts
			(xy 71.12 77.47) (xy 78.74 77.47)
		)
	)
	(wire
		(pts
			(xy 167.64 96.52) (xy 167.64 105.41)
		)
	)
	(wire
		(pts
			(xy 172.72 46.99) (xy 172.72 54.61)
		)
	)
	(wire
		(pts
			(xy 191.77 46.99) (xy 172.72 46.99)
		)
	)
	(wire
		(pts
			(xy 123.19 54.61) (xy 127 54.61)
		)
	)
	(wire
		(pts
			(xy 140.97 96.52) (xy 140.97 99.06)
		)
	)
	(wire
		(pts
			(xy 130.81 99.06) (xy 130.81 96.52)
		)
	)
	(wire
		(pts
			(xy 99.06 104.14) (xy 123.19 104.14)
		)
	)
	(wire
		(pts
			(xy 198.12 105.41) (xy 195.58 105.41)
		)
	)
	(wire
		(pts
			(xy 93.98 64.77) (xy 96.52 64.77)
		)
	)
	(wire
		(pts
			(xy 167.64 105.41) (xy 186.69 105.41)
		)
	)
	(wire
		(pts
			(xy 71.12 82.55) (xy 71.12 80.01)
		)
	)
	(wire
		(pts
			(xy 130.81 96.52) (xy 135.89 96.52)
		)
	)
	(wire
		(pts
			(xy 198.12 118.11) (xy 198.12 105.41)
		)
	)
	(wire
		(pts
			(xy 95.25 114.3) (xy 99.06 114.3)
		)
	)
	(wire
		(pts
			(xy 93.98 80.01) (xy 97.79 80.01)
		)
	)
	(wire
		(pts
			(xy 78.74 64.77) (xy 73.66 64.77)
		)
	)
	(wire
		(pts
			(xy 111.76 77.47) (xy 111.76 66.04)
		)
	)
	(wire
		(pts
			(xy 102.87 82.55) (xy 114.3 82.55)
		)
	)
	(wire
		(pts
			(xy 170.18 95.25) (xy 170.18 102.87)
		)
	)
	(wire
		(pts
			(xy 170.18 102.87) (xy 182.88 102.87)
		)
	)
	(wire
		(pts
			(xy 111.76 66.04) (xy 116.84 66.04)
		)
	)
	(wire
		(pts
			(xy 54.61 46.99) (xy 72.39 46.99)
		)
	)
	(wire
		(pts
			(xy 118.11 69.85) (xy 127 69.85)
		)
	)
	(wire
		(pts
			(xy 170.18 62.23) (xy 184.15 62.23)
		)
	)
	(wire
		(pts
			(xy 97.79 77.47) (xy 111.76 77.47)
		)
	)
	(wire
		(pts
			(xy 138.43 95.25) (xy 170.18 95.25)
		)
	)
	(wire
		(pts
			(xy 116.84 66.04) (xy 116.84 62.23)
		)
	)
	(wire
		(pts
			(xy 54.61 92.71) (xy 78.74 92.71)
		)
	)
	(wire
		(pts
			(xy 114.3 67.31) (xy 119.38 67.31)
		)
	)
	(wire
		(pts
			(xy 73.66 64.77) (xy 73.66 62.23)
		)
	)
	(wire
		(pts
			(xy 115.57 58.42) (xy 127 58.42)
		)
	)
	(wire
		(pts
			(xy 54.61 62.23) (xy 73.66 62.23)
		)
	)
	(wire
		(pts
			(xy 195.58 105.41) (xy 195.58 102.87)
		)
	)
	(wire
		(pts
			(xy 130.81 99.06) (xy 130.81 125.73)
		)
	)
	(wire
		(pts
			(xy 123.19 52.07) (xy 123.19 54.61)
		)
	)
	(wire
		(pts
			(xy 101.6 97.79) (xy 101.6 95.25)
		)
	)
	(wire
		(pts
			(xy 99.06 114.3) (xy 99.06 104.14)
		)
	)
	(wire
		(pts
			(xy 199.39 102.87) (xy 223.52 102.87)
		)
	)
	(wire
		(pts
			(xy 72.39 46.99) (xy 78.74 46.99)
		)
	)
	(wire
		(pts
			(xy 191.77 33.02) (xy 191.77 46.99)
		)
	)
	(wire
		(pts
			(xy 93.98 125.73) (xy 93.98 123.19)
		)
	)
	(wire
		(pts
			(xy 130.81 125.73) (xy 223.52 125.73)
		)
	)
	(wire
		(pts
			(xy 119.38 66.04) (xy 127 66.04)
		)
	)
	(wire
		(pts
			(xy 73.66 67.31) (xy 73.66 64.77)
		)
	)
	(wire
		(pts
			(xy 119.38 67.31) (xy 119.38 66.04)
		)
	)
	(wire
		(pts
			(xy 175.26 69.85) (xy 170.18 69.85)
		)
	)
	(wire
		(pts
			(xy 93.98 77.47) (xy 97.79 77.47)
		)
	)
	(wire
		(pts
			(xy 140.97 96.52) (xy 167.64 96.52)
		)
	)
	(wire
		(pts
			(xy 114.3 62.23) (xy 114.3 52.07)
		)
	)
	(wire
		(pts
			(xy 114.3 52.07) (xy 123.19 52.07)
		)
	)
	(wire
		(pts
			(xy 223.52 102.87) (xy 234.95 102.87)
		)
	)
	(wire
		(pts
			(xy 93.98 62.23) (xy 114.3 62.23)
		)
	)
	(wire
		(pts
			(xy 54.61 33.02) (xy 191.77 33.02)
		)
	)
	(wire
		(pts
			(xy 234.95 87.63) (xy 234.95 62.23)
		)
	)
	(wire
		(pts
			(xy 194.31 62.23) (xy 201.93 62.23)
		)
	)
	(wire
		(pts
			(xy 115.57 64.77) (xy 115.57 58.42)
		)
	)
	(wire
		(pts
			(xy 73.66 62.23) (xy 78.74 62.23)
		)
	)
	(wire
		(pts
			(xy 71.12 80.01) (xy 71.12 77.47)
		)
	)
	(wire
		(pts
			(xy 54.61 33.02) (xy 54.61 46.99)
		)
	)
	(wire
		(pts
			(xy 78.74 52.07) (xy 72.39 52.07)
		)
	)
	(wire
		(pts
			(xy 223.52 125.73) (xy 223.52 102.87)
		)
	)
	(wire
		(pts
			(xy 93.98 125.73) (xy 130.81 125.73)
		)
	)
	(wire
		(pts
			(xy 54.61 95.25) (xy 78.74 95.25)
		)
	)
	(wire
		(pts
			(xy 54.61 46.99) (xy 54.61 62.23)
		)
	)
	(wire
		(pts
			(xy 170.18 73.66) (xy 185.42 73.66)
		)
	)
	(wire
		(pts
			(xy 127 46.99) (xy 127 49.53)
		)
	)
	(wire
		(pts
			(xy 99.06 46.99) (xy 127 46.99)
		)
	)
	(wire
		(pts
			(xy 93.98 49.53) (xy 99.06 49.53)
		)
	)
	(wire
		(pts
			(xy 182.88 66.04) (xy 182.88 102.87)
		)
	)
	(wire
		(pts
			(xy 93.98 82.55) (xy 102.87 82.55)
		)
	)
	(wire
		(pts
			(xy 97.79 80.01) (xy 97.79 77.47)
		)
	)
	(wire
		(pts
			(xy 146.05 118.11) (xy 198.12 118.11)
		)
	)
	(wire
		(pts
			(xy 143.51 99.06) (xy 175.26 99.06)
		)
	)
	(wire
		(pts
			(xy 74.93 114.3) (xy 74.93 123.19)
		)
	)
	(wire
		(pts
			(xy 72.39 49.53) (xy 72.39 46.99)
		)
	)
	(wire
		(pts
			(xy 186.69 99.06) (xy 185.42 99.06)
		)
	)
	(wire
		(pts
			(xy 182.88 66.04) (xy 170.18 66.04)
		)
	)
	(wire
		(pts
			(xy 96.52 67.31) (xy 96.52 64.77)
		)
	)
	(wire
		(pts
			(xy 234.95 102.87) (xy 234.95 87.63)
		)
	)
	(wire
		(pts
			(xy 234.95 62.23) (xy 234.95 46.99)
		)
	)
	(wire
		(pts
			(xy 54.61 97.79) (xy 54.61 123.19)
		)
	)
	(wire
		(pts
			(xy 209.55 62.23) (xy 234.95 62.23)
		)
	)
	(wire
		(pts
			(xy 93.98 97.79) (xy 101.6 97.79)
		)
	)
	(wire
		(pts
			(xy 93.98 67.31) (xy 96.52 67.31)
		)
	)
	(wire
		(pts
			(xy 99.06 49.53) (xy 99.06 46.99)
		)
	)
	(wire
		(pts
			(xy 146.05 83.82) (xy 146.05 118.11)
		)
	)
	(wire
		(pts
			(xy 54.61 77.47) (xy 54.61 92.71)
		)
	)
	(wire
		(pts
			(xy 92.71 49.53) (xy 93.98 49.53)
		)
	)
	(wire
		(pts
			(xy 195.58 102.87) (xy 196.85 102.87)
		)
	)
	(wire
		(pts
			(xy 175.26 69.85) (xy 175.26 99.06)
		)
	)
	(wire
		(pts
			(xy 99.06 49.53) (xy 127 49.53)
		)
	)
	(wire
		(pts
			(xy 127 49.53) (xy 127 50.8)
		)
	)
	(wire
		(pts
			(xy 54.61 97.79) (xy 78.74 97.79)
		)
	)
	(wire
		(pts
			(xy 93.98 95.25) (xy 101.6 95.25)
		)
	)
	(wire
		(pts
			(xy 78.74 49.53) (xy 72.39 49.53)
		)
	)
	(wire
		(pts
			(xy 78.74 67.31) (xy 73.66 67.31)
		)
	)
	(wire
		(pts
			(xy 78.74 82.55) (xy 71.12 82.55)
		)
	)
	(wire
		(pts
			(xy 93.98 92.71) (xy 102.87 92.71)
		)
	)
	(wire
		(pts
			(xy 80.01 114.3) (xy 74.93 114.3)
		)
	)
	(wire
		(pts
			(xy 54.61 92.71) (xy 54.61 95.25)
		)
	)
	(symbol
		(lib_id "power:GNDREF")
		(at 234.95 87.63 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 228.6 87.63 0)
		)
		(property "Value" "GNDREF"
			(at 231.14 87.6299 90)
		)
		(property "Footprint" ""
			(at 234.95 87.63 0)
		)
		(property "Datasheet" ""
			(at 234.95 87.63 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GNDREF\" , reference supply ground"
			(at 234.95 87.63 0)
		)
		(pin "1")
		(instances
			(project "FDP2"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_UPDI_2x03_P2.54mm_Vertical_SMD")
		(at 86.36 95.25 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J6"
			(at 86.36 86.36 0)
		)
		(property "Value" "Conn_PinHeader_UPDI_2x03_P2.54mm_Vertical_SMD"
			(at 86.36 88.9 0)
		)
		(property "Footprint" "fab:PinHeader_02x03_P2.54mm_Vertical_SMD"
			(at 86.36 95.25 0)
		)
		(property "Datasheet" "https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/95278.pdf"
			(at 86.36 95.25 0)
		)
		(property "Description" "Connector Header Surface Mount 6 position 0.100\" (2.54mm) Fab UPDI connector standard 2022"
			(at 86.36 95.25 0)
		)
		(pin "1")
		(pin "3")
		(pin "5")
		(pin "4")
		(pin "2")
		(pin "6")
		(instances
			(project ""
				(path
					(reference "J6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x07_Pin")
		(at 135.89 104.14 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J1"
			(at 136.144 108.966 90)
		)
		(property "Value" "Conn_01x07_Pin"
			(at 136.398 106.172 90)
		)
		(property "Footprint" "Connector_JST:JST_XH_B7B-XH-A_1x07_P2.50mm_Vertical"
			(at 135.89 104.14 0)
		)
		(property "Datasheet" "~"
			(at 135.89 104.14 0)
		)
		(property "Description" "Generic connector, single row, 01x07, script generated"
			(at 135.89 104.14 0)
		)
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "4")
		(pin "1")
		(pin "3")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:R_1206")
		(at 189.23 62.23 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 189.23 55.88 90)
		)
		(property "Value" "R_1206"
			(at 189.23 58.42 90)
		)
		(property "Footprint" "fab:R_1206"
			(at 189.23 62.23 90)
		)
		(property "Datasheet" "~"
			(at 189.23 62.23 0)
		)
		(property "Description" "Resistor"
			(at 189.23 62.23 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_UPDI_2x03_P2.54mm_Vertical_SMD")
		(at 86.36 80.01 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J5"
			(at 86.36 71.12 0)
		)
		(property "Value" "Conn_PinHeader_UPDI_2x03_P2.54mm_Vertical_SMD"
			(at 86.36 73.66 0)
		)
		(property "Footprint" "fab:PinHeader_02x03_P2.54mm_Vertical_SMD"
			(at 86.36 80.01 0)
		)
		(property "Datasheet" "https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/95278.pdf"
			(at 86.36 80.01 0)
		)
		(property "Description" "Connector Header Surface Mount 6 position 0.100\" (2.54mm) Fab UPDI connector standard 2022"
			(at 86.36 80.01 0)
		)
		(pin "6")
		(pin "2")
		(pin "1")
		(pin "3")
		(pin "5")
		(pin "4")
		(instances
			(project ""
				(path
					(reference "J5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "jst ph:S2B-PH-K-S_LF__SN_")
		(at 196.85 92.71 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J2"
			(at 203.2 91.4399 90)
		)
		(property "Value" "S2B-PH-K-S_LF__SN_"
			(at 203.2 93.9799 90)
		)
		(property "Footprint" "fab:JST_S2B-PH-K-S_LF__SN_"
			(at 196.85 92.71 0)
		)
		(property "Datasheet" ""
			(at 196.85 92.71 0)
		)
		(property "Description" ""
			(at 196.85 92.71 0)
		)
		(property "MF" "JST Sales America Inc."
			(at 196.85 92.71 0)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "4.8mm"
			(at 196.85 92.71 0)
		)
		(property "PACKAGE" "None"
			(at 196.85 92.71 0)
		)
		(property "PRICE" "None"
			(at 196.85 92.71 0)
		)
		(property "Package" "NON STANDARD-2 J.S.T."
			(at 196.85 92.71 0)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/S2B-PH-K-S(LF)(SN)/JST/view-part/?ref=eda"
			(at 196.85 92.71 0)
		)
		(property "Price" "None"
			(at 196.85 92.71 0)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/S2B-PH-K-S(LF)(SN)/JST/view-part/?ref=snap"
			(at 196.85 92.71 0)
		)
		(property "MP" "S2B-PH-K-S(LF)(SN)"
			(at 196.85 92.71 0)
		)
		(property "Description_1" "Connector Header Through Hole, Right Angle 2 position"
			(at 196.85 92.71 0)
		)
		(property "Availability" "In Stock"
			(at 196.85 92.71 0)
		)
		(property "AVAILABILITY" "Unavailable"
			(at 196.85 92.71 0)
		)
		(property "DESCRIPTION" "Connector Header Through Hole, Right Angle 2 position"
			(at 196.85 92.71 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_SWD_2x02_P2.54mm_Vertical_SMD")
		(at 87.63 115.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J7"
			(at 87.63 107.95 0)
		)
		(property "Value" "Conn_PinHeader_SWD_2x02_P2.54mm_Vertical_SMD"
			(at 87.63 110.49 0)
		)
		(property "Footprint" "fab:PinHeader_02x02_P2.54mm_Vertical_SMD"
			(at 87.63 115.57 0)
		)
		(property "Datasheet" "https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/95278.pdf"
			(at 87.63 115.57 0)
		)
		(property "Description" "Connector Header Surface Mount 4 position 0.100\" (2.54mm) for programming D11C chips"
			(at 87.63 115.57 0)
		)
		(pin "1")
		(pin "3")
		(pin "2")
		(pin "4")
		(instances
			(project ""
				(path
					(reference "J7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_UPDI_2x03_P2.54mm_Vertical_SMD")
		(at 86.36 64.77 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J4"
			(at 86.36 55.88 0)
		)
		(property "Value" "Conn_PinHeader_UPDI_2x03_P2.54mm_Vertical_SMD"
			(at 86.36 58.42 0)
		)
		(property "Footprint" "fab:PinHeader_02x03_P2.54mm_Vertical_SMD"
			(at 86.36 64.77 0)
		)
		(property "Datasheet" "https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/95278.pdf"
			(at 86.36 64.77 0)
		)
		(property "Description" "Connector Header Surface Mount 6 position 0.100\" (2.54mm) Fab UPDI connector standard 2022"
			(at 86.36 64.77 0)
		)
		(pin "5")
		(pin "3")
		(pin "4")
		(pin "2")
		(pin "6")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "J4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:LED_1206")
		(at 205.74 62.23 180)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 207.3402 54.61 0)
		)
		(property "Value" "LED_1206"
			(at 207.3402 57.15 0)
		)
		(property "Footprint" "fab:LED_1206"
			(at 205.74 62.23 0)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
			(at 205.74 62.23 0)
		)
		(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
			(at 205.74 62.23 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "epressif:XIAO-ESP32-C6-SMD")
		(at 148.59 62.23 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U2"
			(at 153.2733 83.82 0)
		)
		(property "Value" "XIAO-ESP32-S3-SMD"
			(at 153.2733 86.36 0)
		)
		(property "Footprint" "Seeed Studio XIAO Series Library:XIAO-ESP32C6-SMD"
			(at 139.7 57.15 0)
		)
		(property "Datasheet" ""
			(at 139.7 57.15 0)
		)
		(property "Description" ""
			(at 148.59 62.23 0)
		)
		(pin "24")
		(pin "7")
		(pin "2")
		(pin "4")
		(pin "5")
		(pin "18")
		(pin "1")
		(pin "19")
		(pin "15")
		(pin "20")
		(pin "6")
		(pin "3")
		(pin "17")
		(pin "23")
		(pin "16")
		(pin "22")
		(pin "21")
		(pin "10")
		(pin "14")
		(pin "9")
		(pin "12")
		(pin "13")
		(pin "8")
		(pin "11")
		(instances
			(project ""
				(path
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Conn_PinHeader_UPDI_2x03_P2.54mm_Vertical_SMD")
		(at 86.36 49.53 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J3"
			(at 86.106 40.386 0)
		)
		(property "Value" "Conn_PinHeader_UPDI_2x03_P2.54mm_Vertical_SMD"
			(at 87.884 43.434 0)
		)
		(property "Footprint" "fab:PinHeader_02x03_P2.54mm_Vertical_SMD"
			(at 86.36 49.53 0)
		)
		(property "Datasheet" "https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/95278.pdf"
			(at 86.36 49.53 0)
		)
		(property "Description" "Connector Header Surface Mount 6 position 0.100\" (2.54mm) Fab UPDI connector standard 2022"
			(at 86.36 49.53 0)
		)
		(pin "3")
		(pin "5")
		(pin "4")
		(pin "1")
		(pin "2")
		(pin "6")
		(instances
			(project ""
				(path
					(reference "J3")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
