(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(lib_symbols
		(symbol "fab:LED_1206"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at 0 2.54 0)
			)
			(property "Value" "LED_1206"
				(at 0 -2.54 0)
			)
			(property "Footprint" "fab:LED_1206"
				(at 0 0 0)
			)
			(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
				(at 0 0 0)
			)
			(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
				(at 0 0 0)
			)
			(property "ki_keywords" "LED diode 1206 SML-LX1206IC-TR SML-LX1206GC-TR 5988230107F 150120BS75000 QBLP650-IW HIR11-21C/L11/TR8"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*LED*1206*"
				(at 0 0 0)
			)
			(symbol "LED_1206_0_1"
				(polyline
					(pts
						(xy -3.048 -0.762) (xy -4.572 -2.286) (xy -3.81 -2.286) (xy -4.572 -2.286) (xy -4.572 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.778 -0.762) (xy -3.302 -2.286) (xy -2.54 -2.286) (xy -3.302 -2.286) (xy -3.302 -1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 0) (xy 1.27 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.27) (xy -1.27 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -1.27) (xy 1.27 1.27) (xy -1.27 0) (xy 1.27 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_1206_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 2.54)
					(name "K")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 2.54)
					(name "A")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:Module_XIAO-RP2040"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "M"
				(at -10.16 16.51 0)
			)
			(property "Value" "Module_XIAO-RP2040"
				(at 3.81 16.51 0)
			)
			(property "Footprint" "fab:SeeedStudio_XIAO_RP2040"
				(at 0 0 0)
			)
			(property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/"
				(at 0 0 0)
			)
			(property "Description" "RP2040 XIAO RP2040 - ARM® Dual-Core Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board"
				(at 0 0 0)
			)
			(property "ki_keywords" "XIAO RP2040 102010428"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*SeeedStudio?XIAO?RP2040*"
				(at 0 0 0)
			)
			(symbol "Module_XIAO-RP2040_1_1"
				(rectangle
					(start -10.16 15.24)
					(end 10.16 -15.24)
					(fill
						(type background)
					)
				)
				(pin bidirectional line
					(at -12.7 12.7 0)
					(length 2.54)
					(name "D0")
					(number "1")
				)
				(pin bidirectional line
					(at -12.7 10.16 0)
					(length 2.54)
					(name "D1")
					(number "2")
				)
				(pin bidirectional line
					(at -12.7 7.62 0)
					(length 2.54)
					(name "D2")
					(number "3")
				)
				(pin bidirectional line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "D3")
					(number "4")
				)
				(pin bidirectional line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "D4")
					(number "5")
				)
				(pin bidirectional line
					(at -12.7 0 0)
					(length 2.54)
					(name "D5")
					(number "6")
				)
				(pin bidirectional line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "D6")
					(number "7")
				)
				(pin bidirectional line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "D7")
					(number "8")
				)
				(pin bidirectional line
					(at -12.7 -7.62 0)
					(length 2.54)
					(name "D8")
					(number "9")
				)
				(pin bidirectional line
					(at -12.7 -10.16 0)
					(length 2.54)
					(name "D9")
					(number "10")
				)
				(pin bidirectional line
					(at -12.7 -12.7 0)
					(length 2.54)
					(name "D10")
					(number "11")
				)
				(pin power_in line
					(at -2.54 17.78 270)
					(length 2.54)
					(name "3V3")
					(number "12")
				)
				(pin power_in line
					(at -2.54 -17.78 90)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin power_in line
					(at 0 17.78 270)
					(length 2.54)
					(name "5V")
					(number "14")
				)
				(pin power_in line
					(at 0 -17.78 90)
					(length 2.54)
					(name "GND")
					(number "15")
				)
				(pin power_in line
					(at 2.54 17.78 270)
					(length 2.54)
					(name "VIN")
					(number "16")
				)
				(pin power_in line
					(at 2.54 -17.78 90)
					(length 2.54)
					(name "GND")
					(number "19")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "SWDIO")
					(number "17")
				)
				(pin input line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "SWCLK")
					(number "20")
				)
				(pin input line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "RESET")
					(number "18")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:PWR_GND"
			(power)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "PWR_GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "power-flag"
				(at 0 0 0)
			)
			(symbol "PWR_GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "PWR_GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(hide yes)
					(name "PWR_GND")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:Phototransistor_Visible_PT15-21C-TR8"
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 2.54 1.27 0)
			)
			(property "Value" "Phototransistor_Visible_PT15-21C-TR8"
				(at 2.54 -1.27 0)
			)
			(property "Footprint" "fab:Q_1206"
				(at 0 0 0)
			)
			(property "Datasheet" "https://www.everlight.com/file/ProductFile/PT15-21C-TR8.pdf"
				(at 0 0 0)
			)
			(property "Description" "PT15-21C/TR8 is a phototransistor in miniature SMD package which is molded in a water clear with flat top view lens. The device is Spectrally matched to visible AND infrared emitting diode."
				(at 0 0 0)
			)
			(property "ki_keywords" "phototransistor NPN PT15-21C/TR8"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*Q*1206*"
				(at 0 0 0)
			)
			(symbol "Phototransistor_Visible_PT15-21C-TR8_0_1"
				(polyline
					(pts
						(xy -5.08 4.445) (xy -3.81 3.175) (xy -3.81 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 4.445) (xy -2.54 3.175) (xy -2.54 3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 3.175) (xy -4.445 3.175)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.54 3.175) (xy -3.175 3.175)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 1.27) (xy -1.905 -1.27) (xy -1.905 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 0.635) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 -0.635) (xy 0 -2.54) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center -1.27 0)
					(radius 2.8194)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -1.778) (xy -0.762 -1.27) (xy -0.254 -2.286) (xy -1.27 -1.778) (xy -1.27 -1.778)
					)
					(fill
						(type outline)
					)
				)
			)
			(symbol "Phototransistor_Visible_PT15-21C-TR8_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "C")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "E")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:R_1206"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.54 0 90)
			)
			(property "Value" "R_1206"
				(at -2.54 0 90)
			)
			(property "Footprint" "fab:R_1206"
				(at 0 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor RC1206FR-074M99L RC1206FR-07499KL RC1206FR-0749K9L RC1206FR-0749R9L RC1206FR-074R99L ERJ-8BWJR100V RC1206FR-070RL RC1206FR-071RL RC1206FR-0710RL RC1206FR-07100RL RC1206FR-07499RL RC1206FR-071KL RC1206FR-074K99L RC1206FR-0710KL RC1206FR-07100KL RC1206FR-071ML RC1206FR-0710ML PT1206FR-070R1L"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*R*1206*"
				(at 0 0 0)
			)
			(symbol "R_1206_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type background)
					)
				)
			)
			(symbol "R_1206_1_1"
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "fab:Transistor_MOSFET_NCh_SOT23"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "Q"
				(at 3.81 1.27 0)
			)
			(property "Value" "Transistor_MOSFET_NCh_SOT23"
				(at 3.81 -1.27 0)
			)
			(property "Footprint" "fab:SOT-23-3"
				(at 0 0 0)
			)
			(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NDS355AN-D.PDF"
				(at 0 0 0)
			)
			(property "Description" "N-Channel mosfet NDS355AN in SOT-23 package"
				(at 0 0 0)
			)
			(property "ki_keywords" "field effect transistor SI2336DS-T1-GE3"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*SOT?23*"
				(at 0 0 0)
			)
			(symbol "Transistor_MOSFET_NCh_SOT23_0_1"
				(polyline
					(pts
						(xy 0 2.54) (xy 1.27 2.54) (xy 1.27 -2.54) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Transistor_MOSFET_NCh_SOT23_1_0"
				(text "G"
					(at -5.08 -1.27 0)
				)
				(text "D"
					(at 1.27 4.445 0)
				)
				(text "S"
					(at 1.27 -4.445 0)
				)
			)
			(symbol "Transistor_MOSFET_NCh_SOT23_1_1"
				(rectangle
					(start -3.175 3.175)
					(end 3.175 -3.175)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -2.54 -2.54) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 2.54) (xy -1.905 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.905 0) (xy -1.27 0.635) (xy -1.27 -0.635) (xy -1.905 0)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy -1.905 -2.54) (xy 0 -2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy -1.905 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 -2.54) (xy 0 0) (xy -1.905 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0.635 0.635) (xy 1.905 0.635)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0.635) (xy 1.905 0) (xy 0.635 0) (xy 1.27 0.635)
					)
					(fill
						(type outline)
					)
				)
				(pin passive line
					(at -5.08 -2.54 0)
					(length 2.54)
					(name "G")
					(number "1")
				)
				(pin passive line
					(at 0 5.08 270)
					(length 2.54)
					(name "D")
					(number "3")
				)
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "S")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "pads:Capsense"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U1"
				(at 0 2.54 0)
			)
			(property "Value" "~"
				(at 0 0 0)
			)
			(property "Footprint" "pads:lamp_pad"
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(symbol "Capsense_1_1"
				(text_box "Capsense"
					(at -6.35 -1.27 0)
					(size 12.7 -7.62)
					(margins 1.016 1.016 1.016 1.016)
					(fill
						(type none)
					)
				)
				(pin bidirectional line
					(at 8.89 -7.62 180)
					(length 2.54)
					(name "to_RP2040")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 66.04 74.93)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 151.13 81.28)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 151.13 68.58)
		(diameter 0)
		(color 0 0 0 0)
	)
	(wire
		(pts
			(xy 146.05 81.28) (xy 146.05 80.01)
		)
	)
	(wire
		(pts
			(xy 66.04 53.34) (xy 66.04 62.23)
		)
	)
	(wire
		(pts
			(xy 156.21 68.58) (xy 151.13 68.58)
		)
	)
	(wire
		(pts
			(xy 90.17 64.77) (xy 113.03 64.77)
		)
	)
	(wire
		(pts
			(xy 140.97 90.17) (xy 140.97 105.41)
		)
	)
	(wire
		(pts
			(xy 151.13 64.77) (xy 151.13 68.58)
		)
	)
	(wire
		(pts
			(xy 123.19 92.71) (xy 123.19 97.79)
		)
	)
	(wire
		(pts
			(xy 107.95 73.66) (xy 110.49 73.66)
		)
	)
	(wire
		(pts
			(xy 90.17 74.93) (xy 90.17 64.77)
		)
	)
	(wire
		(pts
			(xy 146.05 90.17) (xy 140.97 90.17)
		)
	)
	(wire
		(pts
			(xy 125.73 92.71) (xy 125.73 97.79)
		)
	)
	(wire
		(pts
			(xy 156.21 80.01) (xy 156.21 81.28)
		)
	)
	(wire
		(pts
			(xy 125.73 57.15) (xy 125.73 53.34)
		)
	)
	(wire
		(pts
			(xy 128.27 92.71) (xy 128.27 97.79)
		)
	)
	(wire
		(pts
			(xy 110.49 73.66) (xy 110.49 67.31)
		)
	)
	(wire
		(pts
			(xy 156.21 69.85) (xy 156.21 68.58)
		)
	)
	(wire
		(pts
			(xy 66.04 74.93) (xy 90.17 74.93)
		)
	)
	(wire
		(pts
			(xy 110.49 67.31) (xy 113.03 67.31)
		)
	)
	(wire
		(pts
			(xy 140.97 105.41) (xy 109.22 105.41)
		)
	)
	(wire
		(pts
			(xy 151.13 92.71) (xy 151.13 97.79)
		)
	)
	(wire
		(pts
			(xy 146.05 68.58) (xy 151.13 68.58)
		)
	)
	(wire
		(pts
			(xy 123.19 53.34) (xy 66.04 53.34)
		)
	)
	(wire
		(pts
			(xy 66.04 87.63) (xy 66.04 97.79)
		)
	)
	(wire
		(pts
			(xy 109.22 105.41) (xy 109.22 87.63)
		)
	)
	(wire
		(pts
			(xy 109.22 87.63) (xy 113.03 87.63)
		)
	)
	(wire
		(pts
			(xy 151.13 81.28) (xy 151.13 82.55)
		)
	)
	(wire
		(pts
			(xy 66.04 72.39) (xy 66.04 74.93)
		)
	)
	(wire
		(pts
			(xy 151.13 81.28) (xy 146.05 81.28)
		)
	)
	(wire
		(pts
			(xy 151.13 53.34) (xy 151.13 57.15)
		)
	)
	(wire
		(pts
			(xy 125.73 53.34) (xy 151.13 53.34)
		)
	)
	(wire
		(pts
			(xy 151.13 81.28) (xy 156.21 81.28)
		)
	)
	(wire
		(pts
			(xy 146.05 69.85) (xy 146.05 68.58)
		)
	)
	(wire
		(pts
			(xy 123.19 57.15) (xy 123.19 53.34)
		)
	)
	(wire
		(pts
			(xy 66.04 74.93) (xy 66.04 77.47)
		)
	)
	(symbol
		(lib_id "fab:LED_1206")
		(at 151.13 60.96 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "D1"
			(at 154.94 61.2901 90)
		)
		(property "Value" "LED_1206"
			(at 154.94 63.8301 90)
		)
		(property "Footprint" "fab:LED_1206"
			(at 151.13 60.96 0)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-22-98-0002/LTST-C150CKT.pdf"
			(at 151.13 60.96 0)
		)
		(property "Description" "Light emitting diode, Lite-On Inc. LTST, SMD"
			(at 151.13 60.96 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_GND")
		(at 151.13 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 151.13 104.14 0)
		)
		(property "Value" "PWR_GND"
			(at 151.13 102.87 0)
		)
		(property "Footprint" ""
			(at 151.13 97.79 0)
		)
		(property "Datasheet" ""
			(at 151.13 97.79 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 151.13 97.79 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:R_1206")
		(at 156.21 74.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R3"
			(at 158.75 73.6599 0)
		)
		(property "Value" "499"
			(at 158.75 76.1999 0)
		)
		(property "Footprint" "fab:R_1206"
			(at 156.21 74.93 90)
		)
		(property "Datasheet" "~"
			(at 156.21 74.93 0)
		)
		(property "Description" "Resistor"
			(at 156.21 74.93 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Week05_HTMAA"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_GND")
		(at 128.27 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR05"
			(at 128.27 104.14 0)
		)
		(property "Value" "PWR_GND"
			(at 128.27 102.87 0)
		)
		(property "Footprint" ""
			(at 128.27 97.79 0)
		)
		(property "Datasheet" ""
			(at 128.27 97.79 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 128.27 97.79 0)
		)
		(pin "1")
		(instances
			(project "Week05_HTMAA"
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Phototransistor_Visible_PT15-21C-TR8")
		(at 66.04 82.55 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Q2"
			(at 68.58 80.5306 0)
		)
		(property "Value" "Phototransistor_Visible_PT15-21C-TR8"
			(at 68.58 83.0706 0)
		)
		(property "Footprint" "fab:Q_1206"
			(at 66.04 82.55 0)
		)
		(property "Datasheet" "https://www.everlight.com/file/ProductFile/PT15-21C-TR8.pdf"
			(at 66.04 82.55 0)
		)
		(property "Description" "PT15-21C/TR8 is a phototransistor in miniature SMD package which is molded in a water clear with flat top view lens. The device is Spectrally matched to visible AND infrared emitting diode."
			(at 66.04 82.55 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "Q2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Module_XIAO-RP2040")
		(at 125.73 74.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "M1"
			(at 130.81 64.262 0)
		)
		(property "Value" "Module_XIAO-RP2040"
			(at 130.81 66.802 0)
		)
		(property "Footprint" "fab:SeeedStudio_XIAO_RP2040_no_holes"
			(at 125.73 74.93 0)
		)
		(property "Datasheet" "https://wiki.seeedstudio.com/XIAO-RP2040/"
			(at 125.73 74.93 0)
		)
		(property "Description" "RP2040 XIAO RP2040 - ARM® Dual-Core Cortex®-M0+ MCU 32-Bit Embedded Evaluation Board"
			(at 125.73 74.93 0)
		)
		(pin "1")
		(pin "2")
		(pin "3")
		(pin "4")
		(pin "5")
		(pin "6")
		(pin "7")
		(pin "8")
		(pin "9")
		(pin "10")
		(pin "11")
		(pin "12")
		(pin "13")
		(pin "14")
		(pin "15")
		(pin "16")
		(pin "19")
		(pin "17")
		(pin "20")
		(pin "18")
		(instances
			(project ""
				(path
					(reference "M1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_GND")
		(at 125.73 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 125.73 104.14 0)
		)
		(property "Value" "PWR_GND"
			(at 125.73 102.87 0)
		)
		(property "Footprint" ""
			(at 125.73 97.79 0)
		)
		(property "Datasheet" ""
			(at 125.73 97.79 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 125.73 97.79 0)
		)
		(pin "1")
		(instances
			(project "Week05_HTMAA"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "pads:Capsense")
		(at 99.06 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 99.06 63.5 0)
		)
		(property "Value" "~"
			(at 99.06 66.04 0)
		)
		(property "Footprint" "pads:lamp_pad"
			(at 99.06 66.04 0)
		)
		(property "Datasheet" ""
			(at 99.06 66.04 0)
		)
		(property "Description" ""
			(at 99.06 66.04 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:Transistor_MOSFET_NCh_SOT23")
		(at 151.13 87.63 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "Q1"
			(at 154.94 86.3599 0)
		)
		(property "Value" "Transistor_MOSFET_NCh_SOT23"
			(at 154.94 88.8999 0)
		)
		(property "Footprint" "fab:SOT-23-3"
			(at 151.13 87.63 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NDS355AN-D.PDF"
			(at 151.13 87.63 0)
		)
		(property "Description" "N-Channel mosfet NDS355AN in SOT-23 package"
			(at 151.13 87.63 0)
		)
		(pin "3")
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "Q1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_GND")
		(at 66.04 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 66.04 104.14 0)
		)
		(property "Value" "PWR_GND"
			(at 66.04 102.87 0)
		)
		(property "Footprint" ""
			(at 66.04 97.79 0)
		)
		(property "Datasheet" ""
			(at 66.04 97.79 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 66.04 97.79 0)
		)
		(pin "1")
		(instances
			(project "Week05_HTMAA"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:R_1206")
		(at 66.04 67.31 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R1"
			(at 68.58 66.0399 0)
		)
		(property "Value" "R_1206"
			(at 68.58 68.5799 0)
		)
		(property "Footprint" "fab:R_1206"
			(at 66.04 67.31 90)
		)
		(property "Datasheet" "~"
			(at 66.04 67.31 0)
		)
		(property "Description" "Resistor"
			(at 66.04 67.31 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "Week05_HTMAA"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:PWR_GND")
		(at 123.19 97.79 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 123.19 104.14 0)
		)
		(property "Value" "PWR_GND"
			(at 123.19 102.87 0)
		)
		(property "Footprint" ""
			(at 123.19 97.79 0)
		)
		(property "Datasheet" ""
			(at 123.19 97.79 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 123.19 97.79 0)
		)
		(pin "1")
		(instances
			(project "Week05_HTMAA"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "fab:R_1206")
		(at 146.05 74.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "R2"
			(at 148.59 73.6599 0)
		)
		(property "Value" "100"
			(at 148.59 76.1999 0)
		)
		(property "Footprint" "fab:R_1206"
			(at 146.05 74.93 90)
		)
		(property "Datasheet" "~"
			(at 146.05 74.93 0)
		)
		(property "Description" "Resistor"
			(at 146.05 74.93 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
